Before insert module:

After insert module:

Finding the device....
Found TI device
TI device: vendor=0x0000104c, dev=0x00008888, drv=0x00000000, irq=0x0003, bus=0x3fa81400
TI device requested: resource[0], Start 0xf4500000, End 0xf45fffff, Flags 0x200
TI device requested: resource[1], Start 0xf4400000, End 0xf447ffff, Flags 0x1208
TI device requested: resource[2], Start 0xf4000000, End 0xf43fffff, Flags 0x1208
TI device requested: resource[3], Start 0xf3000000, End 0xf3ffffff, Flags 0x1208
TI device requested: resource[4], Start 0xf4490000, End 0xf4490fff, Flags 0x1208
TI device requested: resource[5], Start 0xf4480000, End 0xf448ffff, Flags 0x1208
Reading the BAR areas....
BAR 0: start = 0xf4500000, Len = 0x00100000, Flags = 0x00000200
BAR 1: start = 0xf4400000, Len = 0x00080000, Flags = 0x00001208
BAR 2: start = 0xf4000000, Len = 0x00400000, Flags = 0x00001208
BAR 3: start = 0xf3000000, Len = 0x01000000, Flags = 0x00001208
REG memory region at address    0x01600000, base 0xf4500000
LL2RAM memory region at address 0x01780000, base 0xf4400000
MSMC memory region at address   0x01880000, base 0xf4000000
DDR memory region at address    0x01d00000, base 0xf3000000
Enabling the device....
ACPI: PCI Interrupt 0000:60:00.0[A] -> GSI 28 (level, low) -> IRQ 28
PCI: Setting latency timer of device 0000:60:00.0 to 64
Access PCIE application register ....
ptrReg is 0x01600000
PCIE_DEV->resource[0].start = 0xf4500000 (0x3f442ae0)
PCIE_DEV->resource[1].start = 0xf4400000 (0x3f442b18)
PCIE_DEV->resource[2].start = 0xf4000000 (0x3f442b50)
PCIE_DEV->resource[3].start = 0xf3000000 (0x3f442b88)