<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="49" y1="0" x2="30.5" y2="0" width="0" layer="20"/>
<wire x1="30.5" y1="0" x2="29.5" y2="1" width="0" layer="20"/>
<wire x1="29.5" y1="1" x2="29.5" y2="8.101" width="0" layer="20"/>
<wire x1="49" y1="0" x2="50" y2="1" width="0" layer="20"/>
<wire x1="50" y1="1" x2="50" y2="49" width="0" layer="20"/>
<wire x1="50" y1="49" x2="49" y2="50" width="0" layer="20"/>
<wire x1="49" y1="50" x2="26.5" y2="50" width="0" layer="20"/>
<wire x1="29.5" y1="8.101" x2="28.5" y2="8.101" width="0" layer="20"/>
<wire x1="28.5" y1="8.101" x2="28.5" y2="7.99" width="0" layer="20"/>
<wire x1="17.6" y1="48.99" x2="17.6" y2="8.99" width="0" layer="20"/>
<wire x1="17.6" y1="8.99" x2="18.6" y2="7.99" width="0" layer="20"/>
<wire x1="18.6" y1="7.99" x2="28.5" y2="7.99" width="0" layer="20"/>
<wire x1="26.5" y1="50" x2="26.5" y2="49.802" width="0" layer="20"/>
<wire x1="26.5" y1="49.802" x2="25.5" y2="49.802" width="0" layer="20"/>
<wire x1="25.5" y1="49.802" x2="25.5" y2="49.99" width="0" layer="20"/>
<wire x1="25.5" y1="49.99" x2="18.6" y2="49.99" width="0" layer="20"/>
<wire x1="18.6" y1="49.99" x2="17.6" y2="48.99" width="0" layer="20"/>
</plain>
<libraries>
<library name="BattleSabres">
<packages>
<package name="IND_2.2UH">
</package>
<package name="QFN-10-POWERPAD">
</package>
</packages>
</library>
<library name="SparkFun">
<description>Spark Fun Electronics' preferred foot prints. &lt;b&gt;Not to be used for commercial purposes.&lt;/b&gt; We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.</description>
<packages>
<package name="0603-RES">
</package>
<package name="0805">
</package>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,54/1,1">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="L1" library="BattleSabres" package="IND_2.2UH" value="INDUCTOR_2.2UH">
<attribute name="NAME"/>
</element>
<element name="C18" library="SparkFun" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="SparkFun" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BB3.3V" library="BattleSabres" package="QFN-10-POWERPAD" value="TPS63000">
<attribute name="NAME"/>
</element>
<element name="L2" library="BattleSabres" package="IND_2.2UH" value="INDUCTOR_2.2UH">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BB5V" library="BattleSabres" package="QFN-10-POWERPAD" value="TPS63000">
<attribute name="NAME"/>
</element>
<element name="BATT+" library="wirepad" package="2,54/1,1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BATT-" library="wirepad" package="2,54/1,1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="SparkFun" package="LED-0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="SparkFun" package="0603-RES" value="120">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BATT+2" library="wirepad" package="2,54/1,1" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C19" pad="2"/>
<contactref element="C18" pad="1"/>
<contactref element="BB3.3V" pad="9"/>
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="BB5V" pad="9"/>
<contactref element="BATT-" pad="1"/>
<contactref element="R18" pad="1"/>
<contactref element="BB3.3V" pad="3"/>
<contactref element="BB3.3V" pad="11"/>
<contactref element="BB5V" pad="3"/>
<contactref element="BB5V" pad="11"/>
</signal>
<signal name="4.2V">
<contactref element="BB3.3V" pad="5"/>
<contactref element="C18" pad="2"/>
<contactref element="BB5V" pad="5"/>
<contactref element="C6" pad="2"/>
<contactref element="BATT+" pad="1"/>
<contactref element="BB5V" pad="7"/>
<contactref element="BB5V" pad="8"/>
<contactref element="BB3.3V" pad="6"/>
<contactref element="BB3.3V" pad="7"/>
<contactref element="BB3.3V" pad="8"/>
<contactref element="BATT+2" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="BB3.3V" pad="2"/>
<contactref element="L1" pad="P$2"/>
</signal>
<signal name="N$39">
<contactref element="L1" pad="P$1"/>
<contactref element="BB3.3V" pad="4"/>
</signal>
<signal name="N$40">
<contactref element="BB5V" pad="2"/>
<contactref element="L2" pad="P$2"/>
</signal>
<signal name="N$44">
<contactref element="L2" pad="P$1"/>
<contactref element="BB5V" pad="4"/>
</signal>
<signal name="5V">
<contactref element="BB5V" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="BB5V" pad="10"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$50">
<contactref element="BB5V" pad="6"/>
</signal>
<signal name="N$24">
<contactref element="LED1" pad="C"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$48">
<contactref element="BB3.3V" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="BB3.3V" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
