<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="254" y1="254" x2="278.9936" y2="254" width="0.254" layer="20"/>
<wire x1="278.9936" y1="234.0102" x2="278.9936" y2="254" width="0.254" layer="20"/>
<wire x1="254" y1="234.0102" x2="278.9936" y2="234.0102" width="0.254" layer="20"/>
<wire x1="254" y1="234.0102" x2="254" y2="254" width="0.254" layer="20"/>
<text>REV B</text>
<text>TMP112EVM</text>
<text>DVDD</text>
<text>SDA</text>
<text>SCL</text>
<text>DVDD</text>
<text>GND</text>
<text>ALERT</text>
<text>9. LPI SOLDERMASK BOTH SIDES USING APPROPRIATE</text>
<text>CLASS 3 STANDARDS AND WORKMANSHIP SHALL CONFORM</text>
<text>3. BOARD MATERIAL AND CONSTRUCTION TO BE</text>
<text>APPROVED AND MARKED ON THE FINISHED BOARD.</text>
<text>4. LAMINATE MATERIAL: COPPER-CLAD FR-4</text>
<text>HIGH Tg MATERIAL; Tg &gt;= 175 DEGREES C,</text>
<text>Td &gt;= 350 DEGREES C.</text>
<text>5. COPPER WEIGHT: 1 oz FINISHED, ALL LAYERS</text>
<text>2. PWB TO BE FABRICATED TO MEET OR EXCEED IPC-6012,</text>
<text>AND MARKED AS PER IPC-1066.</text>
<text>Notes:</text>
<text>1. PWB TO BE MANUFACTURED RoHS COMPLIANT</text>
<text>7. MIN PLATING THICKNESS IN THROUGH HOLES: 0.001</text>
<text>8. BOARD FINISH: IMMERSION SILVER</text>
<text>TO IPC-A-600, CLASS 3 - CURRENT REVISIONS.</text>
<text>6. FINISHED THICKNESS: 0.062 +/- 0.010</text>
<text>LAYER ARTWORK: COLOR = GREEN</text>
<text>14. BOARD DIMENSIONS: .985 x .785</text>
<text>10. LPI SILKSCREEN AS REQUIRED: COLOR = WHITE</text>
<text>11. VENDOR INFORMATION TO BE INCORPORATED</text>
<text>12. MINIMUM COPPER CONDUCTOR WIDTH IS: 6</text>
<text>13. NUMBER OF FINISHED LAYERS: 2 </text>
<text>MINIMUM CONDUCTOR SPACING IS: 6</text>
<text>ON BACK SIDE WHENEVER POSSIBLE.</text>
</plain>
<libraries>
<library name="TMP112_REVA">
<packages>
<package name="TMP102_SOT563_1PRIMARY">
<description>Original name &lt;b&gt;TMP102_SOT563&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="TESTPOINT_1PRIMARY">
<description>Original name &lt;b&gt;TESTPOINT&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="0603_1PRIMARY">
<description>Original name &lt;b&gt;0603&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="0603_2PRIMARY">
<description>Original name &lt;b&gt;0603&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="0603_3PRIMARY">
<description>Original name &lt;b&gt;0603&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="0603_4PRIMARY">
<description>Original name &lt;b&gt;0603&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="0603_5PRIMARY">
<description>Original name &lt;b&gt;0603&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="SM-DIG_UNLABLED_1PRIMARY">
<description>Original name &lt;b&gt;SM-DIG_UNLABLED&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="LED_0603_1PRIMARY">
<description>Original name &lt;b&gt;LED_0603&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="LED_0603_2PRIMARY">
<description>Original name &lt;b&gt;LED_0603&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="0603_6PRIMARY">
<description>Original name &lt;b&gt;0603&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="TMP112_REVA" package="TMP102_SOT563_1PRIMARY" value="TMP102_SOT563">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP5" library="TMP112_REVA" package="TESTPOINT_1PRIMARY" value="TESTPOINT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="TMP112_REVA" package="TESTPOINT_1PRIMARY" value="TESTPOINT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP3" library="TMP112_REVA" package="TESTPOINT_1PRIMARY" value="TESTPOINT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="TMP112_REVA" package="TESTPOINT_1PRIMARY" value="TESTPOINT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="TMP112_REVA" package="TESTPOINT_1PRIMARY" value="TESTPOINT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="TMP112_REVA" package="0603_1PRIMARY" value="0603">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="TMP112_REVA" package="0603_2PRIMARY" value="0603">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="TMP112_REVA" package="0603_3PRIMARY" value="0603">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="TMP112_REVA" package="0603_4PRIMARY" value="0603">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="TMP112_REVA" package="0603_5PRIMARY" value="0603">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="TMP112_REVA" package="SM-DIG_UNLABLED_1PRIMARY" value="SM-DIG_UNLABLED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="TMP112_REVA" package="LED_0603_1PRIMARY" value="LED_0603">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="TMP112_REVA" package="LED_0603_2PRIMARY" value="LED_0603">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="TMP112_REVA" package="0603_6PRIMARY" value="0603">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="SCL">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="TP2" pad="1"/>
</signal>
<signal name="DVDD">
<contactref element="C1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="D1" pad="1"/>
<contactref element="D2" pad="1"/>
<contactref element="J1" pad="6"/>
<contactref element="TP5" pad="1"/>
</signal>
<signal name="$$$18501">
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="SDA">
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="J1" pad="3"/>
<contactref element="TP3" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="TP1" pad="1"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="ALERT">
<contactref element="U1" pad="3"/>
<contactref element="R4" pad="2"/>
<contactref element="TP4" pad="1"/>
</signal>
<signal name="$$$20884">
<contactref element="R5" pad="1"/>
<contactref element="D2" pad="2"/>
</signal>
<signal name="$$$18797">
<contactref element="D1" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
