<5>[    0.000000] Linux version 3.2.0-gb02ab39-dirty (rakz@ubuntu) (gcc version 4.4.3 (GCC) ) #1 Wed Oct 17 23:57:22 CEST 2012
<4>[    0.000000] CPU: ARMv7 Processor [413fc082] revision 2 (ARMv7), cr=10c53c7d
<4>[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, VIPT aliasing instruction cache
<4>[    0.000000] Machine: am335xevm
<4>[    0.000000] Memory policy: ECC disabled, Data cache writeback
<7>[    0.000000] On node 0 totalpages: 65536
<7>[    0.000000] free_area_init_node: node 0, pgdat c070d8c4, node_mem_map c083e000
<7>[    0.000000]   Normal zone: 512 pages used for memmap
<7>[    0.000000]   Normal zone: 0 pages reserved
<7>[    0.000000]   Normal zone: 65024 pages, LIFO batch:15
<6>[    0.000000] AM335X ES1.0 (sgx neon )
<7>[    0.000000] pcpu-alloc: s0 r0 d32768 u32768 alloc=1*32768
<7>[    0.000000] pcpu-alloc: [0] 0 
<4>[    0.000000] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 65024
<5>[    0.000000] Kernel command line: console=ttyO0,115200n8 androidboot.console=ttyO0 mem=256M root=/dev/mmcblk0p2 rw rootfstype=ext3 rootwait init=/init ip=off
<6>[    0.000000] PID hash table entries: 1024 (order: 0, 4096 bytes)
<6>[    0.000000] Dentry cache hash table entries: 32768 (order: 5, 131072 bytes)
<6>[    0.000000] Inode-cache hash table entries: 16384 (order: 4, 65536 bytes)
<6>[    0.000000] Memory: 256MB = 256MB total
<5>[    0.000000] Memory: 251416k/251416k available, 10728k reserved, 0K highmem
<5>[    0.000000] Virtual kernel memory layout:
<5>[    0.000000]     vector  : 0xffff0000 - 0xffff1000   (   4 kB)
<5>[    0.000000]     fixmap  : 0xfff00000 - 0xfffe0000   ( 896 kB)
<5>[    0.000000]     vmalloc : 0xd0800000 - 0xff000000   ( 744 MB)
<5>[    0.000000]     lowmem  : 0xc0000000 - 0xd0000000   ( 256 MB)
<5>[    0.000000]     modules : 0xbf000000 - 0xc0000000   (  16 MB)
<5>[    0.000000]       .text : 0xc0008000 - 0xc0679000   (6596 kB)
<5>[    0.000000]       .init : 0xc0679000 - 0xc06b5000   ( 240 kB)
<5>[    0.000000]       .data : 0xc06b6000 - 0xc070e2a0   ( 353 kB)
<5>[    0.000000]        .bss : 0xc070e2c4 - 0xc083da48   (1214 kB)
<6>[    0.000000] NR_IRQS:396
<6>[    0.000000] IRQ: Found an INTC at 0xfa200000 (revision 5.0) with 128 interrupts
<6>[    0.000000] Total of 128 interrupts on 1 active controller
<6>[    0.000000] OMAP clockevent source: GPTIMER2 at 24000000 Hz
<6>[    0.000000] OMAP clocksource: GPTIMER1 at 32768 Hz
<6>[    0.000000] sched_clock: 32 bits at 32kHz, resolution 30517ns, wraps every 131071999ms
<6>[    0.000000] Console: colour dummy device 80x30
<6>[    0.000152] Calibrating delay loop... 718.02 BogoMIPS (lpj=3590144)
<6>[    0.058929] pid_max: default: 32768 minimum: 301
<6>[    0.059051] Security Framework initialized
<6>[    0.059143] Mount-cache hash table entries: 512
<6>[    0.059509] CPU: Testing write buffer coherency: ok
<4>[    0.079498] omap_hwmod: gfx: failed to hardreset
<4>[    0.095764] omap_hwmod: pruss: failed to hardreset
<6>[    0.096527] print_constraints: dummy: 
<6>[    0.096740] NET: Registered protocol family 16
<6>[    0.097869] OMAP GPIO hardware version 0.1
<6>[    0.098907] omap_mux_init: Add partition: #1: core, flags: 0
<4>[    0.100189]  omap_i2c.1: alias fck already exists
<4>[    0.100677]  omap2_mcspi.1: alias fck already exists
<4>[    0.100799]  omap2_mcspi.2: alias fck already exists
<4>[    0.100952]  edma.0: alias fck already exists
<4>[    0.100982]  edma.0: alias fck already exists
<4>[    0.100982]  edma.0: alias fck already exists
<6>[    0.109863] bio: create slab <bio-0> at 0
<5>[    0.110839] SCSI subsystem initialized
<6>[    0.111663] usbcore: registered new interface driver usbfs
<6>[    0.111785] usbcore: registered new interface driver hub
<6>[    0.111907] usbcore: registered new device driver usb
<6>[    0.112030] musb-ti81xx musb-ti81xx: musb0, board_mode=0x13, plat_mode=0x3
<6>[    0.112182] musb-ti81xx musb-ti81xx: musb1, board_mode=0x13, plat_mode=0x1
<6>[    0.128997] omap_i2c omap_i2c.1: bus 1 rev2.4.0 at 100 kHz
<3>[    0.129791] tps65910 1-002d: could not be detected
<6>[    0.130157] Advanced Linux Sound Architecture Driver Version 1.0.24.
<6>[    0.130706] Bluetooth: Core ver 2.16
<6>[    0.130767] NET: Registered protocol family 31
<6>[    0.130798] Bluetooth: HCI device and connection manager initialized
<6>[    0.130798] Bluetooth: HCI socket layer initialized
<6>[    0.130798] Bluetooth: L2CAP socket layer initialized
<6>[    0.130828] Bluetooth: SCO socket layer initialized
<6>[    0.131011] Switching to clocksource gp timer
<6>[    0.138671] musb-hdrc: version 6.0, ?dma?, otg (peripheral+host)
<6>[    0.138854] musb-hdrc musb-hdrc.0: dma type: pio
<7>[    0.139190] musb-hdrc: ConfigData=0xde (UTMI-8, dyn FIFOs, bulk combine, bulk split, HB-ISO Rx, HB-ISO Tx, SoftConn)
<7>[    0.139190] musb-hdrc: MHDRC RTL version 2.0 
<7>[    0.139221] musb-hdrc: setup fifo_mode 4
<7>[    0.139251] musb-hdrc: 28/31 max ep, 16384/16384 memory
<6>[    0.139617] musb-hdrc musb-hdrc.0: USB OTG mode controller at d081c000 using PIO, IRQ 18
<6>[    0.139862] musb-hdrc musb-hdrc.1: dma type: pio
<7>[    0.140045] musb-hdrc: ConfigData=0xde (UTMI-8, dyn FIFOs, bulk combine, bulk split, HB-ISO Rx, HB-ISO Tx, SoftConn)
<7>[    0.140045] musb-hdrc: MHDRC RTL version 2.0 
<7>[    0.140075] musb-hdrc: setup fifo_mode 4
<7>[    0.140075] musb-hdrc: 28/31 max ep, 16384/16384 memory
<6>[    0.140106] musb-hdrc musb-hdrc.1: MUSB HDRC host driver
<6>[    0.140197] musb-hdrc musb-hdrc.1: new USB bus registered, assigned bus number 1
<6>[    0.140319] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002
<6>[    0.140350] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
<6>[    0.140350] usb usb1: Product: MUSB HDRC host driver
<6>[    0.140380] usb usb1: Manufacturer: Linux 3.2.0-gb02ab39-dirty musb-hcd
<6>[    0.140380] usb usb1: SerialNumber: musb-hdrc.1
<6>[    0.140930] hub 1-0:1.0: USB hub found
<6>[    0.140960] hub 1-0:1.0: 1 port detected
<6>[    0.141448] musb-hdrc musb-hdrc.1: USB Host mode controller at d081e800 using PIO, IRQ 19
<6>[    0.141784] NET: Registered protocol family 2
<6>[    0.141998] IP route cache hash table entries: 2048 (order: 1, 8192 bytes)
<6>[    0.142364] TCP established hash table entries: 8192 (order: 4, 65536 bytes)
<6>[    0.142547] TCP bind hash table entries: 8192 (order: 3, 32768 bytes)
<6>[    0.142639] TCP: Hash tables configured (established 8192 bind 8192)
<6>[    0.142639] TCP reno registered
<6>[    0.142669] UDP hash table entries: 256 (order: 0, 4096 bytes)
<6>[    0.142669] UDP-Lite hash table entries: 256 (order: 0, 4096 bytes)
<6>[    0.142883] NET: Registered protocol family 1
<6>[    0.143157] RPC: Registered named UNIX socket transport module.
<6>[    0.143188] RPC: Registered udp transport module.
<6>[    0.143188] RPC: Registered tcp transport module.
<6>[    0.143188] RPC: Registered tcp NFSv4.1 backchannel transport module.
<4>[    0.143463] NetWinder Floating Point Emulator V0.97 (double precision)
<6>[    0.272399] ashmem: initialized
<5>[    0.272674] VFS: Disk quotas dquot_6.5.2
<4>[    0.272735] Dquot-cache hash table entries: 1024 (order 0, 4096 bytes)
<6>[    0.273620] msgmni has been set to 491
<6>[    0.274597] io scheduler noop registered
<6>[    0.274627] io scheduler deadline registered
<6>[    0.274688] io scheduler cfq registered (default)
<3>[    0.275299] Could not set LED4 to fully on
<6>[    0.276458] omap_uart.0: ttyO0 at MMIO 0x44e09000 (irq = 72) is a OMAP UART0
<6>[    0.851867] console [ttyO0] enabled
<6>[    0.855895] omap_uart.1: ttyO1 at MMIO 0x48022000 (irq = 73) is a OMAP UART1
<6>[    0.863555] omap_uart.2: ttyO2 at MMIO 0x48024000 (irq = 74) is a OMAP UART2
<6>[    0.871185] omap_uart.3: ttyO3 at MMIO 0x481a6000 (irq = 44) is a OMAP UART3
<6>[    0.878845] omap_uart.4: ttyO4 at MMIO 0x481a8000 (irq = 45) is a OMAP UART4
<6>[    0.886474] omap_uart.5: ttyO5 at MMIO 0x481aa000 (irq = 46) is a OMAP UART5
<6>[    0.899932] brd: module loaded
<6>[    0.906433] loop: module loaded
<4>[    0.909881] i2c-core: driver [tsl2550] using legacy suspend method
<4>[    0.916381] i2c-core: driver [tsl2550] using legacy resume method
<6>[    0.922821] at24 1-0051: 32768 byte 24c256 EEPROM, writable, 64 bytes/write
<6>[    0.981597] No daughter card found on AM335x EVM
<6>[    0.986450] at24 1-0050: 32768 byte 24c256 EEPROM, writable, 64 bytes/write
<6>[    1.001647] Board name: A335BONE
<6>[    1.005004] Board version: 00A6
<6>[    1.008270] The board is a AM335x Beaglebone.
<6>[    1.013458] tps65217 1-0024: TPS65217 ID 0xf version 1.1
<6>[    1.020812] print_constraints: DCDC1: 900 <--> 1800 mV at 1800 mV 
<6>[    1.029113] print_constraints: DCDC2: 900 <--> 3300 mV at 1275 mV 
<6>[    1.037384] print_constraints: DCDC3: 900 <--> 1500 mV at 1100 mV 
<6>[    1.045654] print_constraints: LDO1: 1000 <--> 3300 mV at 1800 mV 
<6>[    1.053955] print_constraints: LDO2: 900 <--> 3300 mV at 3300 mV 
<6>[    1.062133] print_constraints: LDO3: 1800 <--> 3300 mV at 3300 mV 
<6>[    1.070373] print_constraints: LDO4: 1800 <--> 3300 mV at 3300 mV 
<4>[    1.077301]  omap_hsmmc.0: alias fck already exists
<4>[    1.082611]  omap_hsmmc.1: alias fck already exists
<4>[    1.087860]  omap_i2c.3: alias fck already exists
<6>[    1.111663] omap_i2c omap_i2c.3: bus 3 rev2.4.0 at 100 kHz
<4>[    1.117706]  omap_i2c.2: alias fck already exists
<6>[    1.141662] omap_i2c omap_i2c.2: bus 2 rev2.4.0 at 100 kHz
<6>[    1.147796] tsl2550 2-0039: standard operating mode
<3>[    2.151733] omap_i2c omap_i2c.2: controller timed out
<4>[    2.171752] tsl2550: probe of 2-0039 failed with error -110
<6>[    2.177764] am335xevm: bt init
<6>[    2.181152] WIFI platform set result is: 0
<6>[    2.185302] WIFI init correct!
<6>[    2.188964] at24 3-0054: 32768 byte 24c256 EEPROM, writable, 64 bytes/write
<6>[    2.196258] IN : bone_setup_daughter_board 
<3>[    3.191894] omap_i2c omap_i2c.3: controller timed out
<3>[    4.231719] omap_i2c omap_i2c.3: controller timed out
<6>[    4.271697] No daughter card found on BeagleBone
<4>[    4.276885]  da8xx_lcdc.0: alias fck already exists
<6>[    4.282226] da8xx_lcdc da8xx_lcdc.0: GLCD: Found Sharp_LCD035Q3DG01 panel
<6>[    4.296997] (stk) :sysfs entries created
<6>[    4.301116] (stk) : debugfs entries created 
<3>[    4.305511] lis3lv02d_i2c 2-0018: Failed to get supply 'Vdd': -19
<3>[    4.312927] mtdoops: mtd device (mtddev=name/number) must be supplied
<6>[    4.319824] omap2-nand driver initializing
<6>[    4.324188] OneNAND driver initializing
<6>[    4.328674] CAN device driver interface
<6>[    4.332702] CAN bus driver for Bosch D_CAN controller 1.0
<6>[    4.381713] davinci_mdio davinci_mdio.0: davinci mdio revision 1.6
<6>[    4.388183] davinci_mdio davinci_mdio.0: detected phy mask fffffffe
<6>[    4.395629] davinci_mdio.0: probed
<6>[    4.399200] davinci_mdio davinci_mdio.0: phy[0]: device 0:00, driver SMSC LAN8710/LAN8720
<6>[    4.407806] PPP generic driver version 2.4.2
<6>[    4.412445] PPP BSD Compression module registered
<6>[    4.417358] PPP Deflate Compression module registered
<6>[    4.422790] usbcore: registered new interface driver cdc_ether
<6>[    4.428924] usbcore: registered new interface driver cdc_eem
<6>[    4.434906] usbcore: registered new interface driver dm9601
<6>[    4.440765] usbcore: registered new interface driver cdc_subset
<6>[    4.446990] cdc_ncm: 04-Aug-2011
<6>[    4.450408] usbcore: registered new interface driver cdc_ncm
<6>[    4.456420] usbcore: registered new interface driver cdc_acm
<6>[    4.462341] cdc_acm: USB Abstract Control Model driver for USB modems and ISDN adapters
<6>[    4.470672] Initializing USB Mass Storage driver...
<6>[    4.475891] usbcore: registered new interface driver usb-storage
<6>[    4.482147] USB Mass Storage support registered.
<6>[    4.487121] usbcore: registered new interface driver usbserial
<6>[    4.493286] USB Serial support registered for generic
<6>[    4.498596] usbcore: registered new interface driver usbserial_generic
<6>[    4.505432] usbserial: USB Serial Driver core
<6>[    4.510009] USB Serial support registered for GSM modem (1-port)
<6>[    4.516418] usbcore: registered new interface driver option
<6>[    4.522247] option: v0.7.2:USB Driver for GSM modems
<6>[    4.529266]  gadget: Mass Storage Function, version: 2009/09/11
<6>[    4.535491]  gadget: Number of LUNs=1
<6>[    4.539306]  lun0: LUN: removable file: (no medium)
<6>[    4.544647]  gadget: android_usb ready
<6>[    4.548583] musb-hdrc musb-hdrc.0: MUSB HDRC host driver
<6>[    4.554199] musb-hdrc musb-hdrc.0: new USB bus registered, assigned bus number 2
<6>[    4.562011] usb usb2: New USB device found, idVendor=1d6b, idProduct=0002
<6>[    4.569091] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
<6>[    4.576660] usb usb2: Product: MUSB HDRC host driver
<6>[    4.581817] usb usb2: Manufacturer: Linux 3.2.0-gb02ab39-dirty musb-hcd
<6>[    4.588714] usb usb2: SerialNumber: musb-hdrc.0
<6>[    4.593933] hub 2-0:1.0: USB hub found
<6>[    4.597869] hub 2-0:1.0: 1 port detected
<6>[    4.602569] mousedev: PS/2 mouse device common for all mice
<6>[    4.609497] using rtc device, omap_rtc, for alarms
<6>[    4.614410] omap_rtc omap_rtc: rtc core: registered omap_rtc as rtc0
<6>[    4.621307] i2c /dev entries driver
<6>[    4.625396] Linux video capture interface: v2.00
<6>[    4.630340] usbcore: registered new interface driver uvcvideo
<6>[    4.636383] USB Video Class driver (1.1.1)
<3>[    5.631713] omap_i2c omap_i2c.2: controller timed out
<4>[    5.651763] lm75: probe of 2-0048 failed with error -110
<3>[    6.651702] omap_i2c omap_i2c.3: controller timed out
<3>[    7.671661] omap_i2c omap_i2c.3: controller timed out
<3>[    8.691711] omap_i2c omap_i2c.3: controller timed out
<3>[    9.711669] omap_i2c omap_i2c.3: controller timed out
<3>[   10.731689] omap_i2c omap_i2c.3: controller timed out
<3>[   11.751708] omap_i2c omap_i2c.3: controller timed out
<3>[   12.771697] omap_i2c omap_i2c.3: controller timed out
<3>[   13.791687] omap_i2c omap_i2c.3: controller timed out
<3>[   14.811706] omap_i2c omap_i2c.2: controller timed out
<3>[   15.831695] omap_i2c omap_i2c.2: controller timed out
<3>[   16.851684] omap_i2c omap_i2c.2: controller timed out
<3>[   17.871704] omap_i2c omap_i2c.2: controller timed out
<3>[   18.891662] omap_i2c omap_i2c.2: controller timed out
<3>[   19.911682] omap_i2c omap_i2c.2: controller timed out
<3>[   20.931701] omap_i2c omap_i2c.2: controller timed out
<6>[   20.952392] OMAP Watchdog Timer Rev 0x01: initial timeout 60 sec
<6>[   20.958862] device-mapper: uevent: version 1.0.3
<6>[   20.963897] device-mapper: ioctl: 4.22.0-ioctl (2011-10-19) initialised: dm-devel@redhat.com
<6>[   20.972717] Bluetooth: HCI UART driver ver 2.2
<6>[   20.977355] Bluetooth: HCI H4 protocol initialized
<6>[   20.982360] Bluetooth: HCILL protocol initialized
<6>[   20.987243] Bluetooth: Bluetooth Driver for TI WiLink - Version 1.0
<7>[   20.993865] hdev cf90b800
<7>[   20.994445] HCI device registered (hdev cf90b800)
<7>[   20.994720] hci0 cf90b800
<7>[   20.994720] plat_kim_chip_enable
<6>[   20.995391] cpuidle: using governor ladder
<6>[   20.999816] cpuidle: using governor menu
<6>[   21.007354] usbcore: registered new interface driver usbhid
<6>[   21.013244] usbhid: USB HID core driver
<6>[   21.122619] logger: created 256K log 'log_main'
<6>[   21.127471] logger: created 256K log 'log_events'
<6>[   21.132507] logger: created 256K log 'log_radio'
<6>[   21.137420] logger: created 256K log 'log_system'
<6>[   21.142852] usbcore: registered new interface driver snd-usb-audio
<6>[   21.150146] ALSA device list:
<6>[   21.153289]   No soundcards found.
<6>[   21.156829] oprofile: hardware counters not available
<6>[   21.162109] oprofile: using timer interrupt.
<6>[   21.166748] nf_conntrack version 0.5.0 (3928 buckets, 15712 max)
<6>[   21.173461] ip_tables: (C) 2000-2006 Netfilter Core Team
<6>[   21.179138] TCP cubic registered
<6>[   21.182708] NET: Registered protocol family 10
<6>[   21.188049] IPv6 over IPv4 tunneling driver
<6>[   21.193115] NET: Registered protocol family 17
<6>[   21.197753] can: controller area network core (rev 20090105 abi 8)
<6>[   21.204345] NET: Registered protocol family 29
<6>[   21.208984] can: raw protocol (rev 20090105)
<6>[   21.213439] can: broadcast manager protocol (rev 20090105 t)
<6>[   21.219787] Bluetooth: RFCOMM TTY layer initialized
<6>[   21.224914] Bluetooth: RFCOMM socket layer initialized
<6>[   21.230285] Bluetooth: RFCOMM ver 1.11
<6>[   21.234191] Bluetooth: BNEP (Ethernet Emulation) ver 1.3
<6>[   21.239746] Bluetooth: BNEP filters: protocol multicast
<6>[   21.245178] Bluetooth: HIDP (Human Interface Emulation) ver 1.2
<6>[   21.251525] lib80211: common routines for IEEE802.11 drivers
<7>[   21.257446] lib80211_crypt: registered algorithm 'NULL'
<7>[   21.257446] lib80211_crypt: registered algorithm 'WEP'
<7>[   21.257446] lib80211_crypt: registered algorithm 'CCMP'
<7>[   21.257476] lib80211_crypt: registered algorithm 'TKIP'
<5>[   21.257476] Registering the dns_resolver key type
<6>[   21.262451] VFP support v0.3: implementor 41 architecture 3 part 30 variant c rev 3
<6>[   21.270446] ThumbEE CPU extension supported.
<4>[   21.274993] mux: Failed to setup hwmod io irq -22
<6>[   21.280548] Power Management for AM33XX family
<6>[   21.285400] Trying to load am335x-pm-firmware.bin (60 secs timeout)
<6>[   21.292083] Copied the M3 firmware to UMEM
<3>[   21.296356] omap_hwmod: wkup_m3: wkup_m3: hwmod data error: OMAP4 does not support st_shift
<6>[   21.308898] clock: disabling unused clocks to save power
<6>[   21.316009] Detected MACID=0:18:31:e0:de:a1
<6>[   21.321472] omap_rtc omap_rtc: setting system clock to 2000-01-01 00:00:17 UTC (946684817)
<6>[   21.330749] Waiting for root device /dev/mmcblk0p2...
<4>[   21.372772] mmc0: host does not support reading read-only switch. assuming write-enable.
<6>[   21.383209] mmc0: new high speed SDHC card at address 0002
<6>[   21.389434] mmcblk0: mmc0:0002 00000 7.41 GiB 
<6>[   21.395996]  mmcblk0: p1 p2 p3
<6>[   21.475799] kjournald starting.  Commit interval 5 seconds
<4>[   21.506317] mmc1: card claims to support voltages below the defined range. These will be ignored.
<4>[   21.525421] mmc1: queuing unknown CIS tuple 0x91 (3 bytes)
<6>[   21.532104] mmc1: new SDIO card at address 0001
<6>[   21.639526] EXT3-fs (mmcblk0p2): using internal journal
<6>[   21.644989] EXT3-fs (mmcblk0p2): mounted filesystem with ordered data mode
<6>[   21.652221] VFS: Mounted root (ext3 filesystem) on device 179:2.
<6>[   21.658935] Freeing init memory: 240K
<4>[   21.686126] init (1): /proc/1/oom_adj is deprecated, please use /proc/1/oom_score_adj instead.
<3>[   21.785522] init: cannot open '/initlogo.rle'
<4>[   21.827758] Disabling lock debugging due to kernel taint
<6>[   21.833984] Compat-wireless backport release: compat-wireless-2011-12-05-1-g84dbe2c
<6>[   21.842010] Backport based on wl12xx.git v2.6.39-1328-g0890f48
<6>[   21.875671] cfg80211: Calling CRDA to update world regulatory domain
<3>[   21.968078] init: cannot find '/system/etc/install-recovery.sh', disabling 'flash_recovery'
<3>[   21.979370] android_usb: already disabled
<6>[   21.992645] adb_bind_config
<6>[   22.072082] warning: `adbd' uses 32-bit capabilities (legacy support in use)
<6>[   22.082275] adb_open
<3>[   22.124023] (stk) :line disc installation timed out 
<7>[   23.122467] plat_kim_chip_enable
<3>[   23.803100] init: untracked pid 64 exited
<3>[   24.242523] (stk) :line disc installation timed out 
<7>[   25.242553] plat_kim_chip_enable
<3>[   26.362548] (stk) :line disc installation timed out 
<7>[   27.362579] plat_kim_chip_enable
<3>[   28.482666] (stk) :line disc installation timed out 
<7>[   29.482604] plat_kim_chip_enable
<3>[   30.602630] (stk) :line disc installation timed out 
<7>[   31.602600] plat_kim_chip_enable
<3>[   32.722625] (stk) :line disc installation timed out 
<3>[   33.722686] Bluetooth: st_register failed -22
<6>[   37.557617] request_suspend_state: wakeup (3->0) at 37555053380 (2000-01-01 00:00:33.726696097 UTC)
<3>[   38.755187] 
<3>[   38.755187] CPSW phy found : id is : 0x7c0f1
<3>[   38.761932] PHY 0:01 not found
<6>[   38.767608] ADDRCONF(NETDEV_UP): eth0: link is not ready
<6>[   38.985473] acc_open
<6>[   38.987792] acc_release
<6>[   54.009857] alarm_release: clear alarm, pending 0
<6>[   54.014892] alarm_release: clear alarm, pending 0
<6>[   54.044006] request_suspend_state: wakeup (0->0) at 54041473057 (2000-01-01 00:00:50.213115774 UTC)
<3>[   54.107452] init: untracked pid 60 exited
<3>[   54.111694] init: untracked pid 65 exited
<3>[   54.148376] init: untracked pid 207 exited
<3>[   54.162841] init: untracked pid 221 exited
<3>[   54.167205] init: untracked pid 275 exited
<3>[   54.171539] init: untracked pid 307 exited
<3>[   54.226257] init: untracked pid 321 exited
<3>[   54.434082] init: untracked pid 240 exited
<6>[   61.025817] android_work: sent uevent USB_STATE=CONNECTED
<6>[   63.102783] android_work: sent uevent USB_STATE=DISCONNECTED
<6>[   63.143798] request_suspend_state: wakeup (0->0) at 63141235020 (2000-01-01 00:00:59.312877737 UTC)
<6>[   63.233520] android_work: sent uevent USB_STATE=CONNECTED
<6>[   63.243927]  gadget: high-speed config #1: android
<6>[   63.251647] android_work: sent uevent USB_STATE=CONFIGURED
<6>[   64.352661] acc_open
<6>[   64.354980] acc_release
<6>[   81.011688] alarm_release: clear alarm, pending 0
<6>[   81.016693] alarm_release: clear alarm, pending 0
<6>[   81.051727] request_suspend_state: wakeup (0->0) at 81049194003 (2000-01-01 00:01:17.220806202 UTC)
<3>[   81.129089] init: untracked pid 341 exited
<3>[   81.162841] init: untracked pid 342 exited
<3>[   81.167205] init: untracked pid 438 exited
<3>[   81.171539] init: untracked pid 452 exited
<3>[   81.208282] init: untracked pid 504 exited
<3>[   81.228515] init: untracked pid 535 exited
<3>[   81.263305] init: untracked pid 550 exited
<3>[   81.463470] init: untracked pid 471 exited
<6>[   89.641357] request_suspend_state: wakeup (0->0) at 89638824131 (2000-01-01 00:01:25.810466848 UTC)
<6>[   90.844665] acc_open
<6>[   90.846984] acc_release
<6>[  108.554412] alarm_release: clear alarm, pending 0
<6>[  108.559356] alarm_release: clear alarm, pending 0
<6>[  108.593078] request_suspend_state: wakeup (0->0) at 108590545323 (2000-01-01 00:01:44.762188040 UTC)
<3>[  108.657531] init: untracked pid 590 exited
<3>[  108.661895] init: untracked pid 591 exited
<3>[  108.702819] init: untracked pid 689 exited
<3>[  108.707153] init: untracked pid 703 exited
<3>[  108.711486] init: untracked pid 755 exited
<3>[  108.748962] init: untracked pid 787 exited
<3>[  108.787109] init: untracked pid 801 exited
<3>[  108.939880] init: untracked pid 720 exited
<6>[  117.221435] request_suspend_state: wakeup (0->0) at 117218902255 (2000-01-01 00:01:53.390544972 UTC)
<6>[  118.543334] acc_open
<6>[  118.545684] acc_release
<6>[  134.938171] alarm_release: clear alarm, pending 0
<6>[  134.943206] alarm_release: clear alarm, pending 0
<6>[  134.972991] request_suspend_state: wakeup (0->0) at 134970458654 (2000-01-01 00:02:11.142070853 UTC)
<3>[  135.036865] init: untracked pid 825 exited
<3>[  135.041198] init: untracked pid 826 exited
<3>[  135.082824] init: untracked pid 920 exited
<3>[  135.087188] init: untracked pid 934 exited
<3>[  135.091522] init: untracked pid 986 exited
<3>[  135.134521] init: untracked pid 1020 exited
<3>[  135.138977] init: untracked pid 1034 exited
<3>[  135.313446] init: untracked pid 951 exited
<6>[  143.170471] request_suspend_state: wakeup (0->0) at 143167937902 (2000-01-01 00:02:19.339580619 UTC)
<6>[  144.363739] acc_open
<6>[  144.366058] acc_release
<6>[  151.460632] binder: release 1087:1087 transaction 14889 in, still active
<6>[  151.467742] binder: send failed reply for transaction 14889 to 1153:1153
<6>[  151.474761] binder: release 1087:1098 transaction 14904 in, still active
<6>[  151.481750] binder: send failed reply for transaction 14904 to 1167:1167
<6>[  151.493438] alarm_release: clear alarm, pending 0
<6>[  151.498352] alarm_release: clear alarm, pending 0
<6>[  151.512145] request_suspend_state: wakeup (0->0) at 151509612707 (2000-01-01 00:02:27.681255424 UTC)
<3>[  151.544921] init: untracked pid 1058 exited
<3>[  151.549316] init: untracked pid 1059 exited
<3>[  151.578521] init: untracked pid 1153 exited
<3>[  151.583160] init: untracked pid 1167 exited
<6>[  160.880371] request_suspend_state: wakeup (0->0) at 160877807286 (2000-01-01 00:02:37.049450003 UTC)
<6>[  162.079681] acc_open
<6>[  162.082000] acc_release
<6>[  168.239410] alarm_release: clear alarm, pending 0
<6>[  168.244445] alarm_release: clear alarm, pending 0
<6>[  168.269287] request_suspend_state: wakeup (0->0) at 168266753819 (2000-01-01 00:02:44.438366018 UTC)
<3>[  168.279479] binder: release proc 1208, transaction 16920, not freed
<3>[  168.293640] init: untracked pid 1181 exited
<3>[  168.298065] init: untracked pid 1182 exited
<6>[  176.844665] request_suspend_state: wakeup (0->0) at 176842132237 (2000-01-01 00:02:53.013744437 UTC)
<6>[  178.045867] acc_open
<6>[  178.048187] acc_release
<6>[  178.432769] wl1271: loaded
<6>[  185.211456] alarm_release: clear alarm, pending 0
<6>[  185.233459] request_suspend_state: wakeup (0->0) at 185230926182 (2000-01-01 00:03:01.402568899 UTC)
<3>[  185.247955] init: untracked pid 1273 exited
<3>[  185.252380] init: untracked pid 1274 exited