**Topology & waveform for signal FP\_TFP2\_ODCK with 28(ST0\_OB2) as Driver and U1(lvcmos\_rrin) as Receiver. Freq – 162MHz.**





**Topology & waveform for signal FP\_TFP2\_ODCK with 28(ST0\_OB2) as Driver and U1(lvcmos\_rrin) as Receiver. Freq – 162MHz.**

****



**Note: Without 22E Series termination**

**Topology & waveform for signal FP\_TFP1\_DI0 with 27(ST0\_OB) as Driver and U1(lvcmos\_crin) as Receiver. Freq – 162MHz.**

****

****

**Topology & waveform for signal FP\_TFP1\_DI0 with 27(ST0\_OB) as Driver and U1(lvcmos\_crin) as Receiver. Freq – 50MHz.**

****

****

**Note : Able to See 3.3 V for Lesser frequency.**