<6>[    1.513641] usb usb2: New USB device found, idVendor=1d6b, idProduct=0002
<6>[    1.520721] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
<6>[    1.528259] usb usb2: Product: MUSB HDRC host driver
<6>[    1.533447] usb usb2: Manufacturer: Linux 3.2.0-gb02ab39-dirty musb-hcd
<6>[    1.540344] usb usb2: SerialNumber: musb-hdrc.0
<6>[    1.545532] hub 2-0:1.0: USB hub found
<6>[    1.549438] hub 2-0:1.0: 1 port detected
<6>[    1.554168] mousedev: PS/2 mouse device common for all mice
<6>[    1.561065] using rtc device, omap_rtc, for alarms
<6>[    1.565979] omap_rtc omap_rtc: rtc core: registered omap_rtc as rtc0
<6>[    1.572875] i2c /dev entries driver
<6>[    1.576721] Linux video capture interface: v2.00
<6>[    1.581726] usbcore: registered new interface driver uvcvideo
<6>[    1.587707] USB Video Class driver (1.1.1)
<6>[    1.593780] OMAP Watchdog Timer Rev 0x01: initial timeout 60 sec
<6>[    1.600311] device-mapper: uevent: version 1.0.3
<6>[    1.605346] device-mapper: ioctl: 4.22.0-ioctl (2011-10-19) initialised: dm-devel@redhat.com
<6>[    1.614166] Bluetooth: HCI UART driver ver 2.2
<6>[    1.618804] Bluetooth: HCI H4 protocol initialized
<6>[    1.623809] Bluetooth: HCILL protocol initialized
<6>[    1.628692] Bluetooth: Bluetooth Driver for TI WiLink - Version 1.0
<7>[    1.635314] hdev cfbc9800
<7>[    1.635864] HCI device registered (hdev cfbc9800)
<7>[    1.636199] hci0 cfbc9800
<7>[    1.636199] plat_kim_chip_enable
<6>[    1.636840] cpuidle: using governor ladder
<6>[    1.641235] cpuidle: using governor menu
<6>[    1.758972] usbcore: registered new interface driver usbhid
<6>[    1.764801] usbhid: USB HID core driver
<6>[    1.769226] logger: created 256K log 'log_main'
<6>[    1.774078] logger: created 256K log 'log_events'
<6>[    1.779083] logger: created 256K log 'log_radio'
<6>[    1.784027] logger: created 256K log 'log_system'
<6>[    1.789489] usbcore: registered new interface driver snd-usb-audio
<6>[    1.796752] ALSA device list:
<6>[    1.799835]   No soundcards found.
<6>[    1.803405] oprofile: hardware counters not available
<6>[    1.808685] oprofile: using timer interrupt.
<6>[    1.813323] nf_conntrack version 0.5.0 (3928 buckets, 15712 max)
<6>[    1.820007] ip_tables: (C) 2000-2006 Netfilter Core Team
<6>[    1.825744] TCP cubic registered
<6>[    1.829254] NET: Registered protocol family 10
<6>[    1.834625] IPv6 over IPv4 tunneling driver
<6>[    1.839630] NET: Registered protocol family 17
<6>[    1.844329] can: controller area network core (rev 20090105 abi 8)
<6>[    1.850891] NET: Registered protocol family 29
<6>[    1.855560] can: raw protocol (rev 20090105)
<6>[    1.860015] can: broadcast manager protocol (rev 20090105 t)
<6>[    1.866149] Bluetooth: RFCOMM TTY layer initialized
<6>[    1.871307] Bluetooth: RFCOMM socket layer initialized
<6>[    1.876678] Bluetooth: RFCOMM ver 1.11
<6>[    1.880584] Bluetooth: BNEP (Ethernet Emulation) ver 1.3
<6>[    1.886138] Bluetooth: BNEP filters: protocol multicast
<6>[    1.891571] Bluetooth: HIDP (Human Interface Emulation) ver 1.2
<6>[    1.897918] lib80211: common routines for IEEE802.11 drivers
<7>[    1.903839] lib80211_crypt: registered algorithm 'NULL'
<7>[    1.903839] lib80211_crypt: registered algorithm 'WEP'
<7>[    1.903839] lib80211_crypt: registered algorithm 'CCMP'
<7>[    1.903869] lib80211_crypt: registered algorithm 'TKIP'
<5>[    1.903869] Registering the dns_resolver key type
<6>[    1.908843] VFP support v0.3: implementor 41 architecture 3 part 30 variant c rev 3
<6>[    1.916839] ThumbEE CPU extension supported.
<4>[    1.921356] mux: Failed to setup hwmod io irq -22
<6>[    1.926971] Power Management for AM33XX family
<6>[    1.931823] Trying to load am335x-pm-firmware.bin (60 secs timeout)
<6>[    1.938476] Copied the M3 firmware to UMEM
<3>[    1.942810] omap_hwmod: wkup_m3: wkup_m3: hwmod data error: OMAP4 does not support st_shift
<6>[    1.955505] clock: disabling unused clocks to save power
<6>[    1.962707] Detected MACID=0:18:31:e0:de:86
<6>[    1.968200] omap_rtc omap_rtc: setting system clock to 2000-01-01 00:00:00 UTC (946684800)
<6>[    1.977508] Waiting for root device /dev/mmcblk0p2...
<4>[    2.022766] mmc0: host does not support reading read-only switch. assuming write-enable.
<6>[    2.033203] mmc0: new high speed SDHC card at address 0002
<6>[    2.039459] mmcblk0: mmc0:0002 00000 7.41 GiB 
<6>[    2.045684]  mmcblk0: p1 p2 p3
<6>[    2.049804] Callback switches WIFI power... 
<6>[    2.054138] ON
<4>[    2.166687] mmc1: card claims to support voltages below the defined range. These will be ignored.
<4>[    2.188140] mmc1: queuing unknown CIS tuple 0x91 (3 bytes)
<6>[    2.195434] mmc1: new SDIO card at address 0001
<6>[    2.200439] Callback switches WIFI power... 
<6>[    2.204742] OFF
<3>[    2.752014] (stk) :line disc installation timed out 
<7>[    3.752258] plat_kim_chip_enable
<3>[    4.872283] (stk) :line disc installation timed out 
<6>[    5.208801] kjournald starting.  Commit interval 5 seconds
<6>[    5.302368] EXT3-fs (mmcblk0p2): using internal journal
<6>[    5.307830] EXT3-fs (mmcblk0p2): recovery complete
<6>[    5.329467] EXT3-fs (mmcblk0p2): mounted filesystem with ordered data mode
<6>[    5.336730] VFS: Mounted root (ext3 filesystem) on device 179:2.
<6>[    5.343444] Freeing init memory: 240K
<4>[    5.372497] init (1): /proc/1/oom_adj is deprecated, please use /proc/1/oom_score_adj instead.
<3>[    5.461944] init: cannot open '/initlogo.rle'
<4>[    5.512451] Disabling lock debugging due to kernel taint
<6>[    5.518615] Compat-wireless backport release: compat-wireless-2011-12-05-1-g84dbe2c
<6>[    5.526641] Backport based on wl12xx.git v2.6.39-1328-g0890f48
<6>[    5.562591] cfg80211: Calling CRDA to update world regulatory domain
<4>[    5.657531] zxy100: zxy100_init
<4>[    5.660827] zxy100: Mark data stale
<4>[    5.668151] zxy100usb: Entered zxy100_usb_init
<4>[    5.672912] zxy100: Register usb device [dev:cf826c60]
<4>[    5.678283] zxy100: Mark data stale
<4>[    5.683715] zxy100: load_cal_data: read_eeprom retval = 0
<4>[    5.690124] zxy100: load_cal_data: zxy100_get_adv_settings = 0
<4>[    5.696228] zxy100usb: registered usb device
<4>[    5.700683] zxy100usb hid_probe: 0 = hid_parse()
<6>[    5.706542] input: Zytronic Displays Limited Zytronic Touchscreen Controller as /devices/platform/omap/musb-ti81xx/musb-hdrc.1/usb1/1-1/1-1:1.0/input/input0
<6>[    5.721466] zxy100_usb 0003:14C8:0005.0001: input: USB HID v1.01 Mouse [Zytronic Displays Limited Zytronic Touchscreen Controller] on usb-musb-hdrc.1-1/input0
<4>[    5.736267] zxy100usb hid_probe: 0 = hid_hw_start()
<4>[    5.741363] zxy100usb: HID Probe: normal exit. ret:0
<6>[    5.746734] usbcore: registered new interface driver zxy100_usb_bl
<3>[    5.773284] init: cannot find '/system/bin/drmserver', disabling 'drm'
<3>[    5.817657] init: cannot find '/system/etc/install-recovery.sh', disabling 'flash_recovery'
<3>[    5.832031] android_usb: already disabled
<6>[    5.845581] adb_bind_config
<7>[    5.872528] plat_kim_chip_enable
<6>[    6.072143] warning: `adbd' uses 32-bit capabilities (legacy support in use)
<3>[    6.992828] (stk) :line disc installation timed out 
<3>[    7.435852] init: untracked pid 65 exited
<7>[    7.992919] plat_kim_chip_enable
<3>[    9.112976] (stk) :line disc installation timed out 
<7>[   10.112945] plat_kim_chip_enable
<3>[   11.233001] (stk) :line disc installation timed out 
<7>[   12.233154] plat_kim_chip_enable
<3>[   13.352966] (stk) :line disc installation timed out 
<3>[   14.352996] Bluetooth: st_register failed -22
<6>[   22.171417] request_suspend_state: wakeup (3->0) at 22168491048 (2000-01-01 00:00:20.696496399 UTC)
<6>[   23.229034] Callback switches WIFI power... 
<6>[   23.233398] ON
<3>[   23.334503] 
<3>[   23.334503] CPSW phy found : id is : 0x7c0f1
<3>[   23.341247] PHY 0:01 not found
<6>[   23.347229] ADDRCONF(NETDEV_UP): eth0: link is not ready
<6>[   23.403930] wl1271: loaded
<6>[   23.407684] Callback switches WIFI power... 
<6>[   23.411956] OFF
<6>[   23.566070] acc_open
<6>[   23.568389] acc_release
<6>[   23.573516] Callback switches WIFI power... 
<6>[   23.577819] ON
<7>[   24.410919] wl1271: CMD_ROLE_ENABLE: 00000000: 00 03 00 18 31 e0 de 86
<7>[   24.411193] wl1271: CMD_ROLE_ENABLE: 00000000: 01 00 00 18 31 e0 de 86
<7>[   24.411773] wl1271: TEST_CMD_INI_FILE_RADIO_PARAM: 00000000: 00 00 00 00 19 00 00 00 00 00 ec f6 00 0c 18 f8
<7>[   24.411773] wl1271: TEST_CMD_INI_FILE_RADIO_PARAM: 00000010: fc 00 08 10 f0 f8 00 0a 14 00 00 00 00 00 00 00
<7>[   24.411804] wl1271: TEST_CMD_INI_FILE_RADIO_PARAM: 00000020: 00 00 00 00 00 00 00 ee f4 f8 fe 05 ea f3 fa 01
<7>[   24.411804] wl1271: TEST_CMD_INI_FILE_RADIO_PARAM: 00000030: 06 e5 f1 fa 02 07 d9 01 80 00 1d 1f 22 26 27 29
<7>[   24.411834] wl1271: TEST_CMD_INI_FILE_RADIO_PARAM: 00000040: 1d 1f 22 26 27 27 16 1d 1e 20 24 25 50 50 50 50
<7>[   24.411834] wl1271: TEST_CMD_INI_FILE_RADIO_PARAM: 00000050: 50 50 50 50 50 50 50 50 50 50 50 50 50 50 50 50
<7>[   24.411865] wl1271: TEST_CMD_INI_FILE_RADIO_PARAM: 00000060: 50 50 50 50 50 50 50 50 01 02 02 02 02 00 15 15
<7>[   24.411865] wl1271: TEST_CMD_INI_FILE_RADIO_PARAM: 00000070: 15 19 19 15 10 1e 2d 00 9a 01 ae 01 c2 01 cc 01
<7>[   24.411895] wl1271: TEST_CMD_INI_FILE_RADIO_PARAM: 00000080: db 01 db 01 d1 01 80 80 80 80 80 80 80 00 00 00
<7>[   24.411926] wl1271: TEST_CMD_INI_FILE_RADIO_PARAM: 00000090: 00 00 00 00 1c 1e 21 23 25 50 18 1e 21 23 25 50
<7>[   24.411926] wl1271: TEST_CMD_INI_FILE_RADIO_PARAM: 000000a0: 16 1c 1e 20 20 50 50 50 50 50 50 50 50 50 50 50
<7>[   24.411956] wl1271: TEST_CMD_INI_FILE_RADIO_PARAM: 000000b0: 50 50 50 50 50 50 50 50 50 50 50 50 50 50 50 50
<7>[   24.411956] wl1271: TEST_CMD_INI_FILE_RADIO_PARAM: 000000c0: 50 50 50 50 50 50 50 50 50 01 02 02 02 02 00 10
<7>[   24.411987] wl1271: TEST_CMD_INI_FILE_RADIO_PARAM: 000000d0: 10 10 10 10 10 10 10 10 10 10 10 10 1e 2d 00 00
<7>[   24.412292] wl1271: TEST_CMD_INI_FILE_EXT_RADIO_PARAM: 00000000: 00 00 00 00 26 00 00 00 00 00 00 00 00 00 00 00
<7>[   24.412292] wl1271: TEST_CMD_INI_FILE_EXT_RADIO_PARAM: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[   24.412322] wl1271: TEST_CMD_INI_FILE_EXT_RADIO_PARAM: 00000020: 00 00 00 00
<7>[   24.533782] wl1271: RATE_MGMT: 00000000: ff 00 00 7d 00 20 00 08 00 10 a4 1f 05 04 0a 04
<7>[   24.533813] wl1271: RATE_MGMT: 00000010: 0d 0a 08 02 0c 00 00 00 00 00 00 00 00 00 00 00
<7>[   24.533843] wl1271: RATE_MGMT: 00000020: 00 00 00 00
<6>[   24.535095] wl1271: firmware booted (Rev 6.3.6.0.79_2)
<6>[   24.540496] wl1271: Driver version: R4_SP2_03_00
<6>[   24.564361] ADDRCONF(NETDEV_UP): wlan0: link is not ready
<7>[   28.453826] wl1271: CMD_ROLE_START: 00000000: 00 00 01 00 01 00 00 00 00 00 00 00 00 00 00 00
<7>[   28.453857] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[   28.453857] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[   28.453887] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[   28.493499] wlan0: authenticate with 00:27:22:94:7d:73 (try 1)
<7>[   28.513427] wlan0: authenticated
<7>[   28.542205] wl1271: CMD_ROLE_START: 00000000: 00 00 01 00 01 00 00 00 00 00 00 00 00 00 00 00
<7>[   28.542236] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[   28.542236] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[   28.542266] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[   28.583160] wlan0: associate with 00:27:22:94:7d:73 (try 1)
<7>[   28.593170] wlan0: RX AssocResp from 00:27:22:94:7d:73 (capab=0x431 status=0 aid=3)
<7>[   28.593200] wlan0: associated
<6>[   28.664886] ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
<6>[   28.714355] wl1271: Association completed.
<7>[   38.922912] wlan0: no IPv6 routers present
<3>[ 1355.824920] init: untracked pid 615 exited
<3>[41513.618408] init: untracked pid 1646 exited
<7>[41513.823394] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 01 00 00 00 00 00 00 00 00 00 00
<7>[41513.823394] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[41513.823425] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[41513.823425] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[41513.845214] wlan0: deauthenticating from 00:27:22:94:7d:73 by local choice (reason=3)
<3>[41513.875274] wl1271: ERROR invalid hlid. dropping skb 0xc5dc4900
<6>[41513.915496] cfg80211: Calling CRDA to update world regulatory domain
<7>[41515.643676] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 01 00 00 00 00 00 00 00 00 00 00
<7>[41515.643707] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[41515.643737] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[41515.643737] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[41515.663665] wlan0: authenticate with 00:27:22:94:7d:73 (try 1)
<7>[41515.676300] wlan0: authenticated
<7>[41515.708557] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 01 00 00 00 00 00 00 00 00 00 00
<7>[41515.708557] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[41515.708587] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[41515.708587] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[41515.723663] wlan0: associate with 00:27:22:94:7d:73 (try 1)
<7>[41515.741302] wlan0: RX ReassocResp from 00:27:22:94:7d:73 (capab=0x431 status=0 aid=3)
<7>[41515.741333] wlan0: associated
<6>[41515.816101] ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
<6>[41515.844177] wl1271: Association completed.
<7>[41526.053527] wlan0: no IPv6 routers present
<6>[47871.883636] wl1271: No ack to nullfunc from AP.
<7>[47871.892181] wlan0: Connection to AP 00:27:22:94:7d:73 lost.
<7>[47871.897674] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 02 00 00 00 00 00 00 00 00 00 00
<7>[47871.897705] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[47871.897705] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[47871.897735] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<6>[47871.954772] cfg80211: Calling CRDA to update world regulatory domain
<3>[47871.986633] wl1271: ERROR invalid hlid. dropping skb 0xca38d300
<7>[47873.776092] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 02 00 00 00 00 00 00 00 00 00 00
<7>[47873.776092] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[47873.776123] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[47873.776123] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[47873.793670] wlan0: authenticate with 00:27:22:80:f2:02 (try 1)
<7>[47873.808715] wlan0: authenticated
<7>[47873.840972] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 02 00 00 00 00 00 00 00 00 00 00
<7>[47873.840972] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[47873.841003] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[47873.841003] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[47873.853729] wlan0: associate with 00:27:22:80:f2:02 (try 1)
<7>[47873.863739] wlan0: RX ReassocResp from 00:27:22:80:f2:02 (capab=0x431 status=0 aid=2)
<7>[47873.863769] wlan0: associated
<6>[47873.933593] ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
<6>[47873.963684] wl1271: Association completed.
<7>[47884.433532] wlan0: no IPv6 routers present
<6>[79737.242675] wl1271: Beacon loss detected.
<7>[79737.247009] wlan0: Connection to AP 00:27:22:80:f2:02 lost.
<7>[79737.258789] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 03 00 00 00 00 00 00 00 00 00 00
<7>[79737.258819] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[79737.258819] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[79737.258850] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<6>[79737.352722] cfg80211: Calling CRDA to update world regulatory domain
<3>[79737.371520] wl1271: ERROR invalid hlid. dropping skb 0xc5daea40
<7>[79739.142608] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 03 00 00 00 00 00 00 00 00 00 00
<7>[79739.142639] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[79739.142639] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[79739.142639] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[79739.153656] wlan0: authenticate with 00:27:22:94:7d:73 (try 1)
<7>[79739.175292] wlan0: authenticated
<7>[79739.233551] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 03 00 00 00 00 00 00 00 00 00 00
<7>[79739.233581] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[79739.233612] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[79739.233612] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[79739.253662] wlan0: associate with 00:27:22:94:7d:73 (try 1)
<7>[79739.272705] wlan0: RX ReassocResp from 00:27:22:94:7d:73 (capab=0x431 status=0 aid=3)
<7>[79739.272735] wlan0: associated
<6>[79739.333618] ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
<6>[79739.363708] wl1271: Association completed.
<7>[79750.363525] wlan0: no IPv6 routers present
<6>[89776.751495] wl1271: Beacon loss detected.
<7>[89776.755889] wlan0: Connection to AP 00:27:22:94:7d:73 lost.
<7>[89776.770751] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 04 00 00 00 00 00 00 00 00 00 00
<7>[89776.770782] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[89776.770782] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[89776.773559] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<6>[89776.867980] cfg80211: Calling CRDA to update world regulatory domain
<3>[89776.903533] wl1271: ERROR invalid hlid. dropping skb 0xc5dae140
<7>[89778.651428] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 04 00 00 00 00 00 00 00 00 00 00
<7>[89778.651458] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[89778.651489] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[89778.651489] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[89778.663726] wlan0: authenticate with 00:27:22:80:f2:02 (try 1)
<7>[89778.684082] wlan0: authenticated
<7>[89778.716308] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 04 00 00 00 00 00 00 00 00 00 00
<7>[89778.716339] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[89778.716339] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[89778.716369] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[89778.733642] wlan0: associate with 00:27:22:80:f2:02 (try 1)
<7>[89778.749023] wlan0: RX ReassocResp from 00:27:22:80:f2:02 (capab=0x431 status=0 aid=2)
<7>[89778.749053] wlan0: associated
<6>[89778.813598] ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
<6>[89778.863677] wl1271: Association completed.
<7>[89789.453521] wlan0: no IPv6 routers present
<6>[93692.824401] wl1271: Beacon loss detected.
<7>[93692.828704] wlan0: Connection to AP 00:27:22:80:f2:02 lost.
<7>[93692.841278] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 05 00 00 00 00 00 00 00 00 00 00
<7>[93692.841308] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[93692.841339] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[93692.841339] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<6>[93692.915283] cfg80211: Calling CRDA to update world regulatory domain
<3>[93692.937866] wl1271: ERROR invalid hlid. dropping skb 0xc5c63800
<7>[93694.683929] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 05 00 00 00 00 00 00 00 00 00 00
<7>[93694.683959] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[93694.683959] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[93694.683959] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[93694.703765] wlan0: authenticate with 00:27:22:94:7d:73 (try 1)
<7>[93694.717407] wlan0: authenticated
<7>[93694.753570] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 05 00 00 00 00 00 00 00 00 00 00
<7>[93694.753601] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[93694.753601] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[93694.753631] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[93694.773651] wlan0: associate with 00:27:22:94:7d:73 (try 1)
<7>[93694.789459] wlan0: RX ReassocResp from 00:27:22:94:7d:73 (capab=0x431 status=0 aid=3)
<7>[93694.789459] wlan0: associated
<6>[93694.854156] ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
<6>[93694.903686] wl1271: Association completed.
<7>[93705.593536] wlan0: no IPv6 routers present
<6>[95548.448883] wl1271: Beacon loss detected.
<7>[95548.453216] wlan0: Connection to AP 00:27:22:94:7d:73 lost.
<7>[95548.458374] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 06 00 00 00 00 00 00 00 00 00 00
<7>[95548.458404] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[95548.458404] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[95548.458435] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<6>[95548.553955] cfg80211: Calling CRDA to update world regulatory domain
<3>[95548.578613] wl1271: ERROR invalid hlid. dropping skb 0xc5c63500
<7>[95550.332550] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 06 00 00 00 00 00 00 00 00 00 00
<7>[95550.332580] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[95550.332611] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[95550.332611] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[95550.343688] wlan0: authenticate with 00:27:22:80:f2:02 (try 1)
<7>[95550.357299] wlan0: authenticated
<7>[95550.393737] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 06 00 00 00 00 00 00 00 00 00 00
<7>[95550.393768] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[95550.393798] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[95550.393798] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[95550.413665] wlan0: associate with 00:27:22:80:f2:02 (try 1)
<7>[95550.430175] wlan0: RX ReassocResp from 00:27:22:80:f2:02 (capab=0x431 status=0 aid=2)
<7>[95550.430175] wlan0: associated
<6>[95550.502777] ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
<6>[95550.544006] wl1271: Association completed.
<7>[95560.633514] wlan0: no IPv6 routers present
<6>[104182.667938] wl1271: No ack to nullfunc from AP.
<7>[104182.672882] wlan0: Connection to AP 00:27:22:80:f2:02 lost.
<7>[104182.678222] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 07 00 00 00 00 00 00 00 00 00 00
<7>[104182.678253] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[104182.678253] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[104182.683502] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<6>[104182.778259] cfg80211: Calling CRDA to update world regulatory domain
<3>[104182.800506] wl1271: ERROR invalid hlid. dropping skb 0xc5c63c80
<7>[104184.520507] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 07 00 00 00 00 00 00 00 00 00 00
<7>[104184.520538] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[104184.520538] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[104184.520568] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[104184.543670] wlan0: authenticate with 00:27:22:94:7d:73 (try 1)
<7>[104184.568145] wlan0: authenticated
<7>[104184.613739] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 07 00 00 00 00 00 00 00 00 00 00
<7>[104184.613769] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[104184.613769] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[104184.613800] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[104184.633666] wlan0: associate with 00:27:22:94:7d:73 (try 1)
<7>[104184.649322] wlan0: RX ReassocResp from 00:27:22:94:7d:73 (capab=0x431 status=0 aid=3)
<7>[104184.649353] wlan0: associated
<6>[104184.714080] ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
<6>[104184.743774] wl1271: Association completed.
<7>[104195.583526] wlan0: no IPv6 routers present
<6>[223168.730377] binder: 522:536 refcount change on invalid ref 18
<6>[223168.743865] binder: 522:536 refcount change on invalid ref 19
<6>[223168.750122] binder: 522:536 refcount change on invalid ref 20
<6>[309568.608428] binder: 522:547 refcount change on invalid ref 18
<6>[309568.614624] binder: 522:547 refcount change on invalid ref 18
<3>[309568.620758] binder: transaction release 247134 bad handle 18
<6>[309568.641876] binder: 522:577 refcount change on invalid ref 19
<6>[309568.648040] binder: 522:577 refcount change on invalid ref 19
<3>[309568.654144] binder: transaction release 603518 bad handle 19
<6>[363388.340362] binder: 522:575 refcount change on invalid ref 20
<6>[363388.346527] binder: 522:575 refcount change on invalid ref 20
<3>[363388.352630] binder: transaction release 603521 bad handle 20
<7>[963507.370574] wlan0: deauthenticated from 00:27:22:94:7d:73 (Reason: 6)
<7>[963507.378967] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 01 00 00 00 00 00 00 00 00 00 00
<7>[963507.378997] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[963507.378997] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[963507.379028] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<6>[963507.497039] cfg80211: Calling CRDA to update world regulatory domain
<7>[963509.234863] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 01 00 00 00 00 00 00 00 00 00 00
<7>[963509.234893] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[963509.234924] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[963509.234924] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[963509.254974] wlan0: authenticate with 00:27:22:94:7d:73 (try 1)
<7>[963509.270477] wlan0: authenticated
<7>[963509.302917] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 01 00 00 00 00 00 00 00 00 00 00
<7>[963509.302947] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[963509.302978] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[963509.302978] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[963509.314880] wlan0: associate with 00:27:22:94:7d:73 (try 1)
<7>[963509.335449] wlan0: RX ReassocResp from 00:27:22:94:7d:73 (capab=0x431 status=0 aid=3)
<7>[963509.335479] wlan0: associated
<6>[963509.432312] ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
<6>[963509.465087] wl1271: Association completed.
<7>[963519.974761] wlan0: no IPv6 routers present
<6>[1201746.532958] wl1271: Beacon loss detected.
<7>[1201746.537475] wlan0: Connection to AP 00:27:22:94:7d:73 lost.
<7>[1201746.550079] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 02 00 00 00 00 00 00 00 00 00 00
<7>[1201746.550079] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1201746.550109] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1201746.550109] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<6>[1201746.637603] cfg80211: Calling CRDA to update world regulatory domain
<3>[1201746.667480] wl1271: ERROR invalid hlid. dropping skb 0xc5c63380
<7>[1201748.400421] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 02 00 00 00 00 00 00 00 00 00 00
<7>[1201748.400451] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1201748.400451] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1201748.400482] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1201748.415527] wlan0: authenticate with 00:27:22:80:f2:02 (try 1)
<7>[1201748.433044] wlan0: authenticated
<7>[1201748.475585] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 02 00 00 00 00 00 00 00 00 00 00
<7>[1201748.475616] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1201748.475646] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1201748.475646] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1201748.495513] wlan0: associate with 00:27:22:80:f2:02 (try 1)
<7>[1201748.514251] wlan0: RX ReassocResp from 00:27:22:80:f2:02 (capab=0x431 status=0 aid=2)
<7>[1201748.514282] wlan0: associated
<6>[1201748.579040] ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
<6>[1201748.625518] wl1271: Association completed.
<7>[1201759.545379] wlan0: no IPv6 routers present
<6>[1203042.548522] wl1271: Beacon loss detected.
<7>[1203042.553039] wlan0: Connection to AP 00:27:22:80:f2:02 lost.
<7>[1203042.562316] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 03 00 00 00 00 00 00 00 00 00 00
<7>[1203042.562316] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1203042.562347] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1203042.562347] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<6>[1203042.653564] cfg80211: Calling CRDA to update world regulatory domain
<3>[1203042.685394] wl1271: ERROR invalid hlid. dropping skb 0xc5dae380
<7>[1203044.448455] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 03 00 00 00 00 00 00 00 00 00 00
<7>[1203044.448486] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1203044.448516] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1203044.448516] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1203044.465515] wlan0: authenticate with 00:27:22:94:7d:73 (try 1)
<7>[1203044.481018] wlan0: authenticated
<7>[1203044.525573] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 03 00 00 00 00 00 00 00 00 00 00
<7>[1203044.525604] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1203044.525604] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1203044.525634] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1203044.545501] wlan0: associate with 00:27:22:94:7d:73 (try 1)
<7>[1203044.562286] wlan0: RX ReassocResp from 00:27:22:94:7d:73 (capab=0x431 status=0 aid=3)
<7>[1203044.562316] wlan0: associated
<6>[1203044.627044] ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
<6>[1203044.655517] wl1271: Association completed.
<7>[1203055.095367] wlan0: no IPv6 routers present
<6>[1203410.172973] wl1271: Beacon loss detected.
<7>[1203410.177459] wlan0: Connection to AP 00:27:22:94:7d:73 lost.
<7>[1203410.193206] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 04 00 00 00 00 00 00 00 00 00 00
<7>[1203410.193237] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1203410.193267] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1203410.193267] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<6>[1203410.285797] cfg80211: Calling CRDA to update world regulatory domain
<3>[1203410.317687] wl1271: ERROR invalid hlid. dropping skb 0xc3c9b380
<7>[1203412.056732] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 04 00 00 00 00 00 00 00 00 00 00
<7>[1203412.056762] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1203412.056793] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1203412.056793] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1203412.075531] wlan0: authenticate with 00:27:22:80:f2:02 (try 1)
<7>[1203412.091217] wlan0: authenticated
<7>[1203412.137847] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 04 00 00 00 00 00 00 00 00 00 00
<7>[1203412.137847] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1203412.137878] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1203412.137878] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1203412.155487] wlan0: associate with 00:27:22:80:f2:02 (try 1)
<7>[1203412.170562] wlan0: RX ReassocResp from 00:27:22:80:f2:02 (capab=0x431 status=0 aid=2)
<7>[1203412.170562] wlan0: associated
<6>[1203412.245391] ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
<6>[1203412.275543] wl1271: Association completed.
<7>[1203422.625366] wlan0: no IPv6 routers present
<6>[1218236.258728] wl1271: Beacon loss detected.
<7>[1218236.263214] wlan0: Connection to AP 00:27:22:80:f2:02 lost.
<7>[1218236.275573] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 05 00 00 00 00 00 00 00 00 00 00
<7>[1218236.275604] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1218236.275604] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1218236.275634] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<6>[1218236.377471] cfg80211: Calling CRDA to update world regulatory domain
<3>[1218236.395477] wl1271: ERROR invalid hlid. dropping skb 0xc5dae740
<7>[1218238.158599] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 05 00 00 00 00 00 00 00 00 00 00
<7>[1218238.158630] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1218238.158630] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1218238.158660] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1218238.175567] wlan0: authenticate with 00:27:22:94:7d:73 (try 1)
<7>[1218238.191345] wlan0: authenticated
<7>[1218238.235412] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 05 00 00 00 00 00 00 00 00 00 00
<7>[1218238.235443] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1218238.235443] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1218238.235473] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1218238.255523] wlan0: associate with 00:27:22:94:7d:73 (try 1)
<7>[1218238.272491] wlan0: RX ReassocResp from 00:27:22:94:7d:73 (capab=0x431 status=0 aid=6)
<7>[1218238.272491] wlan0: associated
<6>[1218238.342315] ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
<6>[1218238.375915] wl1271: Association completed.
<7>[1218248.895385] wlan0: no IPv6 routers present
<6>[1228954.505645] PVR_K: User requested SGX debug info
<6>[1228954.510681] PVR_K: SGX debug (blaze_android_sgx_ogles1_ogles2_GPL sgxddk 18 1.8@789263)
<6>[1228954.519256] PVR_K: Flip Command Complete Data 0 for display device 1:
<6>[1228954.526184] PVR_K: 	SRC 0: ROC DevVAddr:0xD800054 ROP:0x2da1f ROC:0x2da1e, WOC DevVAddr:0xD800044 WOP:0x16d10 WOC:0x16d10
<6>[1228954.537811] PVR_K: 	SRC 1: ROC DevVAddr:0xD800034 ROP:0x2da1e ROC:0x2da1d, WOC DevVAddr:0xD800024 WOP:0x16d10 WOC:0x16d0f
<6>[1228954.549407] PVR_K: Flip Command Complete Data 1 for display device 1:
<6>[1228954.556335] PVR_K: 	SRC 0: (Not in use)
<6>[1228954.560516] PVR_K: 	SRC 1: (Not in use)
<6>[1228954.564697] PVR_K: SGX Host control:
<6>[1228954.568603] PVR_K: 	(HC-0) 0x00000001 0x0000000C 0x00000000 0x00000001
<6>[1228954.575592] PVR_K: 	(HC-10) 0x00000000 0x00000000 0x0000000A 0x00030D40
<6>[1228954.582672] PVR_K: 	(HC-20) 0x00000065 0x00000004 0x00000000 0x00000000
<6>[1228954.589782] PVR_K: 	(HC-30) 0x0000728F 0x006393DF 0x1136A300 0x00000000
<6>[1228954.596862] PVR_K: 	(HC-40) 0x00000000 0x00000000 0xEB5BEFB7 0xEB27BBBD
<6>[1228954.603942] PVR_K: SGX TA/3D control:
<6>[1228954.607971] PVR_K: 	(T3C-0) 0x0F003000 0x0F003120 0x0F002000 0x00000000
<6>[1228954.615051] PVR_K: 	(T3C-10) 0x0F0C1580 0x00000001 0x00000002 0x00000001
<6>[1228954.622222] PVR_K: 	(T3C-20) 0x0F00AE80 0x00000000 0x00000000 0x00000000
<6>[1228954.629425] PVR_K: 	(T3C-30) 0x00000000 0x00000000 0x00000000 0x00000000
<6>[1228954.636596] PVR_K: 	(T3C-40) 0x00000000 0x00000000 0x00000000 0x00000000
<6>[1228954.643768] PVR_K: 	(T3C-50) 0x00000000 0x00000000 0x00000000 0x00000000
<6>[1228954.650970] PVR_K: 	(T3C-60) 0x00000000 0x00000000 0x00000000 0x0F00AE80
<6>[1228954.658142] PVR_K: 	(T3C-70) 0x00000000 0x00000000 0x0F00AE80 0x00000000
<6>[1228954.665313] PVR_K: 	(T3C-80) 0x00000000 0x00000000 0x00000000 0x0F000000
<6>[1228954.672485] PVR_K: 	(T3C-90) 0x8F224000 0x0F095600 0x00000000 0x0F08B4A0
<6>[1228954.679687] PVR_K: 	(T3C-A0) 0x0F00AE80 0x00000000 0x0F08B4A0 0x00000000
<6>[1228954.686859] PVR_K: 	(T3C-B0) 0x0F0AD500 0x00000000 0x00000000 0x00000000
<6>[1228954.694030] PVR_K: 	(T3C-C0) 0x00000000 0x00000000 0x00000000 0x0002DA1F
<6>[1228954.701202] PVR_K: 	(T3C-D0) 0x0002DA1E 0x0F000000 0x8000B000 0x8004B000
<6>[1228954.708404] PVR_K: 	(T3C-E0) 0x0F004000 0x0F00A420 0x0F00A740 0x00000000
<6>[1228954.715576] PVR_K: 	(T3C-F0) 0x00000000 0x00000000 0x0000007A 0x0000007A
<6>[1228954.722747] PVR_K: 	(T3C-100) 0x00000000 0x00000003 0x00000000 0x00000000
<6>[1228954.730041] PVR_K: 	(T3C-110) 0x00000001 0x00000000 0x83BCB6FB 0xE42FBCFF
<6>[1228954.737304] PVR_K: SGX Kernel CCB WO:0x0 RO:0x0
<6>[1228959.745605] PVR_K: User requested SGX debug info
<6>[1228959.750640] PVR_K: SGX debug (blaze_android_sgx_ogles1_ogles2_GPL sgxddk 18 1.8@789263)
<6>[1228959.759246] PVR_K: Flip Command Complete Data 0 for display device 1:
<6>[1228959.766174] PVR_K: 	SRC 0: ROC DevVAddr:0xD800054 ROP:0x2da20 ROC:0x2da1e, WOC DevVAddr:0xD800044 WOP:0x16d11 WOC:0x16d10
<6>[1228959.777801] PVR_K: 	SRC 1: ROC DevVAddr:0xD800034 ROP:0x2da1f ROC:0x2da1d, WOC DevVAddr:0xD800024 WOP:0x16d10 WOC:0x16d0f
<6>[1228959.789428] PVR_K: Flip Command Complete Data 1 for display device 1:
<6>[1228959.796325] PVR_K: 	SRC 0: (Not in use)
<6>[1228959.800506] PVR_K: 	SRC 1: (Not in use)
<6>[1228959.804687] PVR_K: SGX Host control:
<6>[1228959.808593] PVR_K: 	(HC-0) 0x00000001 0x0000000C 0x00000000 0x00000001
<6>[1228959.815612] PVR_K: 	(HC-10) 0x00000000 0x00000000 0x0000000A 0x00030D40
<6>[1228959.822692] PVR_K: 	(HC-20) 0x00000065 0x00000004 0x00000000 0x00000000
<6>[1228959.829772] PVR_K: 	(HC-30) 0x00007290 0x00639444 0x11875B10 0x00000000
<6>[1228959.836883] PVR_K: 	(HC-40) 0x00000000 0x00000000 0xEB5BEFB7 0xEB27BBBD
<6>[1228959.843963] PVR_K: SGX TA/3D control:
<6>[1228959.847961] PVR_K: 	(T3C-0) 0x0F003000 0x0F003120 0x0F002000 0x00000000
<6>[1228959.855041] PVR_K: 	(T3C-10) 0x0F0C1580 0x00000001 0x00000002 0x00000001
<6>[1228959.862213] PVR_K: 	(T3C-20) 0x0F00AE80 0x00000000 0x00000000 0x00000000
<6>[1228959.869415] PVR_K: 	(T3C-30) 0x00000000 0x00000000 0x00000000 0x00000000
<6>[1228959.876586] PVR_K: 	(T3C-40) 0x00000000 0x00000000 0x00000000 0x00000000
<6>[1228959.883758] PVR_K: 	(T3C-50) 0x00000000 0x00000000 0x00000000 0x00000000
<6>[1228959.890930] PVR_K: 	(T3C-60) 0x00000000 0x00000000 0x00000000 0x0F00AE80
<6>[1228959.898132] PVR_K: 	(T3C-70) 0x00000000 0x00000000 0x0F00AE80 0x00000000
<6>[1228959.905303] PVR_K: 	(T3C-80) 0x00000000 0x00000000 0x00000000 0x0F000000
<6>[1228959.912475] PVR_K: 	(T3C-90) 0x8F224000 0x0F095C00 0x00000000 0x0F08B280
<6>[1228959.919647] PVR_K: 	(T3C-A0) 0x0F00AE80 0x00000000 0x0F08B4A0 0x00000000
<6>[1228959.926849] PVR_K: 	(T3C-B0) 0x0F0AD500 0x00000000 0x00000000 0x00000000
<6>[1228959.934020] PVR_K: 	(T3C-C0) 0x00000000 0x00000000 0x00000000 0x0002DA20
<6>[1228959.941192] PVR_K: 	(T3C-D0) 0x0002DA1E 0x0F000000 0x8000B000 0x8004B000
<6>[1228959.948364] PVR_K: 	(T3C-E0) 0x0F004000 0x0F00A420 0x0F00A740 0x00000000
<6>[1228959.955566] PVR_K: 	(T3C-F0) 0x00000000 0x00000000 0x0000007A 0x0000007A
<6>[1228959.962738] PVR_K: 	(T3C-100) 0x00000000 0x00000003 0x00000000 0x00000000
<6>[1228959.970001] PVR_K: 	(T3C-110) 0x00000001 0x00000000 0x83BCB6FB 0xE42FBCFF
<6>[1228959.977264] PVR_K: SGX Kernel CCB WO:0x3 RO:0x3
<6>[1228959.982238] PVR_K: User requested SGX debug info
<6>[1228959.987304] PVR_K: SGX debug (blaze_android_sgx_ogles1_ogles2_GPL sgxddk 18 1.8@789263)
<6>[1228959.995849] PVR_K: Flip Command Complete Data 0 for display device 1:
<6>[1228960.002746] PVR_K: 	SRC 0: ROC DevVAddr:0xD800054 ROP:0x2da20 ROC:0x2da1e, WOC DevVAddr:0xD800044 WOP:0x16d11 WOC:0x16d10
<6>[1228960.014373] PVR_K: 	SRC 1: ROC DevVAddr:0xD800034 ROP:0x2da1f ROC:0x2da1d, WOC DevVAddr:0xD800024 WOP:0x16d10 WOC:0x16d0f
<6>[1228960.026000] PVR_K: Flip Command Complete Data 1 for display device 1:
<6>[1228960.032897] PVR_K: 	SRC 0: (Not in use)
<6>[1228960.037078] PVR_K: 	SRC 1: (Not in use)
<6>[1228960.041259] PVR_K: SGX Host control:
<6>[1228960.045166] PVR_K: 	(HC-0) 0x00000001 0x0000000C 0x00000000 0x00000001
<6>[1228960.052185] PVR_K: 	(HC-10) 0x00000000 0x00000000 0x0000000A 0x00030D40
<6>[1228960.059265] PVR_K: 	(HC-20) 0x00000065 0x00000004 0x00000000 0x00000000
<6>[1228960.066345] PVR_K: 	(HC-30) 0x00007290 0x00639444 0x11875B10 0x00000000
<6>[1228960.073425] PVR_K: 	(HC-40) 0x00000000 0x00000000 0xEB5BEFB7 0xEB27BBBD
<6>[1228960.080535] PVR_K: SGX TA/3D control:
<6>[1228960.084533] PVR_K: 	(T3C-0) 0x0F003000 0x0F003120 0x0F002000 0x00000000
<6>[1228960.091613] PVR_K: 	(T3C-10) 0x0F0C1580 0x00000001 0x00000002 0x00000001
<6>[1228960.098815] PVR_K: 	(T3C-20) 0x0F00AE80 0x00000000 0x00000000 0x00000000
<6>[1228960.105987] PVR_K: 	(T3C-30) 0x00000000 0x00000000 0x00000000 0x00000000
<6>[1228960.113159] PVR_K: 	(T3C-40) 0x00000000 0x00000000 0x00000000 0x00000000
<6>[1228960.120330] PVR_K: 	(T3C-50) 0x00000000 0x00000000 0x00000000 0x00000000
<6>[1228960.127502] PVR_K: 	(T3C-60) 0x00000000 0x00000000 0x00000000 0x0F00AE80
<6>[1228960.134674] PVR_K: 	(T3C-70) 0x00000000 0x00000000 0x0F00AE80 0x00000000
<6>[1228960.141876] PVR_K: 	(T3C-80) 0x00000000 0x00000000 0x00000000 0x0F000000
<6>[1228960.149047] PVR_K: 	(T3C-90) 0x8F224000 0x0F095C00 0x00000000 0x0F08B280
<6>[1228960.156219] PVR_K: 	(T3C-A0) 0x0F00AE80 0x00000000 0x0F08B4A0 0x00000000
<6>[1228960.163391] PVR_K: 	(T3C-B0) 0x0F0AD500 0x00000000 0x00000000 0x00000000
<6>[1228960.170562] PVR_K: 	(T3C-C0) 0x00000000 0x00000000 0x00000000 0x0002DA20
<6>[1228960.177764] PVR_K: 	(T3C-D0) 0x0002DA1E 0x0F000000 0x8000B000 0x8004B000
<6>[1228960.184936] PVR_K: 	(T3C-E0) 0x0F004000 0x0F00A420 0x0F00A740 0x00000000
<6>[1228960.192108] PVR_K: 	(T3C-F0) 0x00000000 0x00000000 0x0000007A 0x0000007A
<6>[1228960.199279] PVR_K: 	(T3C-100) 0x00000000 0x00000003 0x00000000 0x00000000
<6>[1228960.206573] PVR_K: 	(T3C-110) 0x00000001 0x00000000 0x83BCB6FB 0xE42FBCFF
<6>[1228960.213836] PVR_K: SGX Kernel CCB WO:0x3 RO:0x3
<6>[1228960.218811] PVR_K: User requested SGX debug info
<6>[1228960.223815] PVR_K: SGX debug (blaze_android_sgx_ogles1_ogles2_GPL sgxddk 18 1.8@789263)
<6>[1228960.232391] PVR_K: Flip Command Complete Data 0 for display device 1:
<6>[1228960.239288] PVR_K: 	SRC 0: ROC DevVAddr:0xD800054 ROP:0x2da20 ROC:0x2da1e, WOC DevVAddr:0xD800044 WOP:0x16d11 WOC:0x16d10
<6>[1228960.250915] PVR_K: 	SRC 1: ROC DevVAddr:0xD800034 ROP:0x2da1f ROC:0x2da1d, WOC DevVAddr:0xD800024 WOP:0x16d10 WOC:0x16d0f
<6>[1228960.262542] PVR_K: Flip Command Complete Data 1 for display device 1:
<6>[1228960.269439] PVR_K: 	SRC 0: (Not in use)
<6>[1228960.273620] PVR_K: 	SRC 1: (Not in use)
<6>[1228960.277832] PVR_K: SGX Host control:
<6>[1228960.281738] PVR_K: 	(HC-0) 0x00000001 0x0000000C 0x00000000 0x00000001
<6>[1228960.288726] PVR_K: 	(HC-10) 0x00000000 0x00000000 0x0000000A 0x00030D40
<6>[1228960.295837] PVR_K: 	(HC-20) 0x00000065 0x00000004 0x00000000 0x00000000
<6>[1228960.302917] PVR_K: 	(HC-30) 0x00007290 0x00639444 0x11875B10 0x00000000
<6>[1228960.309997] PVR_K: 	(HC-40) 0x00000000 0x00000000 0xEB5BEFB7 0xEB27BBBD
<6>[1228960.317077] PVR_K: SGX TA/3D control:
<6>[1228960.321075] PVR_K: 	(T3C-0) 0x0F003000 0x0F003120 0x0F002000 0x00000000
<6>[1228960.328186] PVR_K: 	(T3C-10) 0x0F0C1580 0x00000001 0x00000002 0x00000001
<6>[1228960.335357] PVR_K: 	(T3C-20) 0x0F00AE80 0x00000000 0x00000000 0x00000000
<6>[1228960.342529] PVR_K: 	(T3C-30) 0x00000000 0x00000000 0x00000000 0x00000000
<6>[1228960.349700] PVR_K: 	(T3C-40) 0x00000000 0x00000000 0x00000000 0x00000000
<6>[1228960.356903] PVR_K: 	(T3C-50) 0x00000000 0x00000000 0x00000000 0x00000000
<6>[1228960.364074] PVR_K: 	(T3C-60) 0x00000000 0x00000000 0x00000000 0x0F00AE80
<6>[1228960.371246] PVR_K: 	(T3C-70) 0x00000000 0x00000000 0x0F00AE80 0x00000000
<6>[1228960.378417] PVR_K: 	(T3C-80) 0x00000000 0x00000000 0x00000000 0x0F000000
<6>[1228960.385620] PVR_K: 	(T3C-90) 0x8F224000 0x0F095C00 0x00000000 0x0F08B280
<6>[1228960.392791] PVR_K: 	(T3C-A0) 0x0F00AE80 0x00000000 0x0F08B4A0 0x00000000
<6>[1228960.399963] PVR_K: 	(T3C-B0) 0x0F0AD500 0x00000000 0x00000000 0x00000000
<6>[1228960.407135] PVR_K: 	(T3C-C0) 0x00000000 0x00000000 0x00000000 0x0002DA20
<6>[1228960.414306] PVR_K: 	(T3C-D0) 0x0002DA1E 0x0F000000 0x8000B000 0x8004B000
<6>[1228960.421508] PVR_K: 	(T3C-E0) 0x0F004000 0x0F00A420 0x0F00A740 0x00000000
<6>[1228960.428680] PVR_K: 	(T3C-F0) 0x00000000 0x00000000 0x0000007A 0x0000007A
<6>[1228960.435852] PVR_K: 	(T3C-100) 0x00000000 0x00000003 0x00000000 0x00000000
<6>[1228960.443115] PVR_K: 	(T3C-110) 0x00000001 0x00000000 0x83BCB6FB 0xE42FBCFF
<6>[1228960.450408] PVR_K: SGX Kernel CCB WO:0x3 RO:0x3
<6>[1228965.715545] PVR_K: User requested SGX debug info
<6>[1228965.720581] PVR_K: SGX debug (blaze_android_sgx_ogles1_ogles2_GPL sgxddk 18 1.8@789263)
<6>[1228965.729125] PVR_K: Flip Command Complete Data 0 for display device 1:
<6>[1228965.736053] PVR_K: 	SRC 0: ROC DevVAddr:0xD800054 ROP:0x2da21 ROC:0x2da1e, WOC DevVAddr:0xD800044 WOP:0x16d11 WOC:0x16d10
<6>[1228965.747680] PVR_K: 	SRC 1: ROC DevVAddr:0xD800034 ROP:0x2da20 ROC:0x2da1d, WOC DevVAddr:0xD800024 WOP:0x16d11 WOC:0x16d0f
<6>[1228965.759307] PVR_K: Flip Command Complete Data 1 for display device 1:
<6>[1228965.766204] PVR_K: 	SRC 0: (Not in use)
<6>[1228965.770385] PVR_K: 	SRC 1: (Not in use)
<6>[1228965.774566] PVR_K: SGX Host control:
<6>[1228965.778503] PVR_K: 	(HC-0) 0x00000001 0x0000000C 0x00000000 0x00000001
<6>[1228965.785491] PVR_K: 	(HC-10) 0x00000000 0x00000000 0x0000000A 0x00030D40
<6>[1228965.792572] PVR_K: 	(HC-20) 0x00000065 0x00000004 0x00000000 0x00000000
<6>[1228965.799652] PVR_K: 	(HC-30) 0x00007291 0x006394A9 0x11E29A70 0x00000000
<6>[1228965.806762] PVR_K: 	(HC-40) 0x00000000 0x00000000 0xEB5BEFB7 0xEB27BBBD
<6>[1228965.813842] PVR_K: SGX TA/3D control:
<6>[1228965.817840] PVR_K: 	(T3C-0) 0x0F003000 0x0F003120 0x0F002000 0x00000000
<6>[1228965.824920] PVR_K: 	(T3C-10) 0x0F0C1580 0x00000001 0x00000002 0x00000001
<6>[1228965.832092] PVR_K: 	(T3C-20) 0x0F00AE80 0x00000000 0x00000000 0x00000000
<6>[1228965.839294] PVR_K: 	(T3C-30) 0x00000000 0x00000000 0x00000000 0x00000000
<6>[1228965.846466] PVR_K: 	(T3C-40) 0x00000000 0x00000000 0x00000000 0x00000000
<6>[1228965.853637] PVR_K: 	(T3C-50) 0x00000000 0x0F00AE80 0x00000000 0x00000000
<6>[1228965.860809] PVR_K: 	(T3C-60) 0x0F00AE80 0x00000000 0x00000000 0x0F00AE80
<6>[1228965.868011] PVR_K: 	(T3C-70) 0x00000000 0x00000000 0x0F00AE80 0x00000000
<6>[1228965.875183] PVR_K: 	(T3C-80) 0x00000000 0x00000000 0x00000000 0x0F000000
<6>[1228965.882354] PVR_K: 	(T3C-90) 0x8F224000 0x0F095C00 0x00000000 0x0F08B280
<6>[1228965.889526] PVR_K: 	(T3C-A0) 0x0F00AE80 0x00000000 0x0F08B4A0 0x00000000
<6>[1228965.896697] PVR_K: 	(T3C-B0) 0x0F0AD500 0x00000000 0x00000000 0x00000000
<6>[1228965.903869] PVR_K: 	(T3C-C0) 0x00000000 0x00000000 0x00000000 0x0002DA20
<6>[1228965.911071] PVR_K: 	(T3C-D0) 0x0002DA1E 0x0F000000 0x8000B000 0x8004B000
<6>[1228965.918243] PVR_K: 	(T3C-E0) 0x0F004000 0x0F00A420 0x0F00A740 0x00000000
<6>[1228965.925415] PVR_K: 	(T3C-F0) 0x00000000 0x00000000 0x0000007A 0x0000007A
<6>[1228965.932586] PVR_K: 	(T3C-100) 0x00000000 0x00000003 0x00000000 0x00000000
<6>[1228965.939880] PVR_K: 	(T3C-110) 0x00000001 0x00000000 0x83BCB6FB 0xE42FBCFF
<6>[1228965.947143] PVR_K: SGX Kernel CCB WO:0x7 RO:0x7
<6>[1228970.955596] PVR_K: User requested SGX debug info
<6>[1228970.960601] PVR_K: SGX debug (blaze_android_sgx_ogles1_ogles2_GPL sgxddk 18 1.8@789263)
<6>[1228970.969177] PVR_K: Flip Command Complete Data 0 for display device 1:
<6>[1228970.976104] PVR_K: 	SRC 0: ROC DevVAddr:0xD800054 ROP:0x2da22 ROC:0x2da1e, WOC DevVAddr:0xD800044 WOP:0x16d11 WOC:0x16d10
<6>[1228970.987731] PVR_K: 	SRC 1: ROC DevVAddr:0xD800034 ROP:0x2da21 ROC:0x2da1d, WOC DevVAddr:0xD800024 WOP:0x16d11 WOC:0x16d0f
<6>[1228970.999328] PVR_K: Flip Command Complete Data 1 for display device 1:
<6>[1228971.006256] PVR_K: 	SRC 0: (Not in use)
<6>[1228971.010437] PVR_K: 	SRC 1: (Not in use)
<6>[1228971.014617] PVR_K: SGX Host control:
<6>[1228971.018554] PVR_K: 	(HC-0) 0x00000001 0x0000000C 0x00000000 0x00000001
<6>[1228971.025543] PVR_K: 	(HC-10) 0x00000000 0x00000000 0x0000000A 0x00030D40
<6>[1228971.032623] PVR_K: 	(HC-20) 0x00000065 0x00000004 0x00000000 0x00000000
<6>[1228971.039733] PVR_K: 	(HC-30) 0x00007291 0x006394A9 0x11E29A70 0x00000000
<6>[1228971.046813] PVR_K: 	(HC-40) 0x00000000 0x00000000 0xEB5BEFB7 0xEB27BBBD
<6>[1228971.053894] PVR_K: SGX TA/3D control:
<6>[1228971.057891] PVR_K: 	(T3C-0) 0x0F003000 0x0F003120 0x0F002000 0x00000000
<6>[1228971.064971] PVR_K: 	(T3C-10) 0x0F0C1580 0x00000001 0x00000002 0x00000001
<6>[1228971.072174] PVR_K: 	(T3C-20) 0x0F00AE80 0x00000000 0x00000000 0x00000000
<6>[1228971.079345] PVR_K: 	(T3C-30) 0x00000000 0x00000000 0x00000000 0x00000000
<6>[1228971.086517] PVR_K: 	(T3C-40) 0x00000000 0x00000000 0x00000000 0x00000000
<6>[1228971.093688] PVR_K: 	(T3C-50) 0x00000000 0x0F00AE80 0x00000000 0x00000000
<6>[1228971.100891] PVR_K: 	(T3C-60) 0x0F00AE80 0x00000000 0x00000000 0x0F00AE80
<6>[1228971.108062] PVR_K: 	(T3C-70) 0x00000000 0x00000000 0x0F00AE80 0x00000000
<6>[1228971.115234] PVR_K: 	(T3C-80) 0x00000000 0x00000000 0x00000000 0x0F000000
<6>[1228971.122406] PVR_K: 	(T3C-90) 0x8F224000 0x0F095C00 0x00000000 0x0F08B280
<6>[1228971.129577] PVR_K: 	(T3C-A0) 0x0F00AE80 0x00000000 0x0F08B4A0 0x00000000
<6>[1228971.136779] PVR_K: 	(T3C-B0) 0x0F0AD500 0x00000000 0x00000000 0x00000000
<6>[1228971.143951] PVR_K: 	(T3C-C0) 0x00000000 0x00000000 0x00000000 0x0002DA20
<6>[1228971.151123] PVR_K: 	(T3C-D0) 0x0002DA1E 0x0F000000 0x8000B000 0x8004B000
<6>[1228971.158294] PVR_K: 	(T3C-E0) 0x0F004000 0x0F00A420 0x0F00A740 0x00000000
<6>[1228971.165496] PVR_K: 	(T3C-F0) 0x00000000 0x00000000 0x0000007A 0x0000007A
<6>[1228971.172668] PVR_K: 	(T3C-100) 0x00000000 0x00000003 0x00000000 0x00000000
<6>[1228971.179931] PVR_K: 	(T3C-110) 0x00000001 0x00000000 0x83BCB6FB 0xE42FBCFF
<6>[1228971.187194] PVR_K: SGX Kernel CCB WO:0x7 RO:0x7
<6>[1228976.185577] PVR_K: User requested SGX debug info
<6>[1228976.190582] PVR_K: SGX debug (blaze_android_sgx_ogles1_ogles2_GPL sgxddk 18 1.8@789263)
<6>[1228976.199157] PVR_K: Flip Command Complete Data 0 for display device 1:
<6>[1228976.206054] PVR_K: 	SRC 0: ROC DevVAddr:0xD800054 ROP:0x2da22 ROC:0x2da1e, WOC DevVAddr:0xD800044 WOP:0x16d11 WOC:0x16d10
<6>[1228976.217681] PVR_K: 	SRC 1: ROC DevVAddr:0xD800034 ROP:0x2da21 ROC:0x2da1d, WOC DevVAddr:0xD800024 WOP:0x16d11 WOC:0x16d0f
<6>[1228976.229309] PVR_K: Flip Command Complete Data 1 for display device 1:
<6>[1228976.236206] PVR_K: 	SRC 0: (Not in use)
<6>[1228976.240386] PVR_K: 	SRC 1: (Not in use)
<6>[1228976.244567] PVR_K: SGX Host control:
<6>[1228976.248504] PVR_K: 	(HC-0) 0x00000001 0x0000000C 0x00000000 0x00000001
<6>[1228976.255493] PVR_K: 	(HC-10) 0x00000000 0x00000000 0x0000000A 0x00030D40
<6>[1228976.262573] PVR_K: 	(HC-20) 0x00000065 0x00000004 0x00000000 0x00000000
<6>[1228976.269683] PVR_K: 	(HC-30) 0x00007292 0x0063950E 0x12825CE0 0x00000000
<6>[1228976.276763] PVR_K: 	(HC-40) 0x00000000 0x00000000 0xEB5BEFB7 0xEB27BBBD
<6>[1228976.283843] PVR_K: SGX TA/3D control:
<6>[1228976.287841] PVR_K: 	(T3C-0) 0x0F003000 0x0F003120 0x0F002000 0x00000000
<6>[1228976.294952] PVR_K: 	(T3C-10) 0x0F0C1580 0x00000001 0x00000002 0x00000001
<6>[1228976.302124] PVR_K: 	(T3C-20) 0x0F00AE80 0x00000000 0x00000000 0x00000000
<6>[1228976.309295] PVR_K: 	(T3C-30) 0x00000000 0x00000000 0x00000000 0x00000000
<6>[1228976.316467] PVR_K: 	(T3C-40) 0x00000000 0x00000000 0x00000000 0x00000000
<6>[1228976.323638] PVR_K: 	(T3C-50) 0x00000000 0x0F00AE80 0x00000000 0x00000000
<6>[1228976.330841] PVR_K: 	(T3C-60) 0x0F00AE80 0x00000000 0x00000000 0x0F00AE80
<6>[1228976.338043] PVR_K: 	(T3C-70) 0x00000000 0x00000000 0x0F00AE80 0x00000000
<6>[1228976.345214] PVR_K: 	(T3C-80) 0x00000000 0x00000000 0x00000000 0x0F000000
<6>[1228976.352386] PVR_K: 	(T3C-90) 0x8F224000 0x0F095C00 0x00000000 0x0F08B280
<6>[1228976.359558] PVR_K: 	(T3C-A0) 0x0F00AE80 0x00000000 0x0F08B4A0 0x00000000
<6>[1228976.366760] PVR_K: 	(T3C-B0) 0x0F0AD500 0x00000000 0x00000000 0x00000000
<6>[1228976.373931] PVR_K: 	(T3C-C0) 0x00000000 0x00000000 0x00000000 0x0002DA20
<6>[1228976.381103] PVR_K: 	(T3C-D0) 0x0002DA1E 0x0F000000 0x8000B000 0x8004B000
<6>[1228976.388275] PVR_K: 	(T3C-E0) 0x0F004000 0x0F00A420 0x0F00A740 0x00000000
<6>[1228976.395446] PVR_K: 	(T3C-F0) 0x00000000 0x00000000 0x0000007A 0x0000007A
<6>[1228976.402618] PVR_K: 	(T3C-100) 0x00000000 0x00000003 0x00000000 0x00000000
<6>[1228976.409912] PVR_K: 	(T3C-110) 0x00000001 0x00000000 0x83BCB6FB 0xE42FBCFF
<6>[1228976.417175] PVR_K: SGX Kernel CCB WO:0xA RO:0xA
<6>[1228981.415618] PVR_K: User requested SGX debug info
<6>[1228981.420623] PVR_K: SGX debug (blaze_android_sgx_ogles1_ogles2_GPL sgxddk 18 1.8@789263)
<6>[1228981.429199] PVR_K: Flip Command Complete Data 0 for display device 1:
<6>[1228981.436126] PVR_K: 	SRC 0: ROC DevVAddr:0xD800054 ROP:0x2da22 ROC:0x2da1e, WOC DevVAddr:0xD800044 WOP:0x16d11 WOC:0x16d10
<6>[1228981.447753] PVR_K: 	SRC 1: ROC DevVAddr:0xD800034 ROP:0x2da21 ROC:0x2da1d, WOC DevVAddr:0xD800024 WOP:0x16d11 WOC:0x16d0f
<6>[1228981.459381] PVR_K: Flip Command Complete Data 1 for display device 1:
<6>[1228981.466278] PVR_K: 	SRC 0: (Not in use)
<6>[1228981.470458] PVR_K: 	SRC 1: (Not in use)
<6>[1228981.474639] PVR_K: SGX Host control:
<6>[1228981.478576] PVR_K: 	(HC-0) 0x00000001 0x0000000C 0x00000000 0x00000001
<6>[1228981.485565] PVR_K: 	(HC-10) 0x00000000 0x00000000 0x0000000A 0x00030D40
<6>[1228981.492675] PVR_K: 	(HC-20) 0x00000065 0x00000004 0x00000000 0x00000000
<6>[1228981.499755] PVR_K: 	(HC-30) 0x00007292 0x0063950E 0x12825CE0 0x00000000
<6>[1228981.506835] PVR_K: 	(HC-40) 0x00000000 0x00000000 0xEB5BEFB7 0xEB27BBBD
<6>[1228981.513916] PVR_K: SGX TA/3D control:
<6>[1228981.517944] PVR_K: 	(T3C-0) 0x0F003000 0x0F003120 0x0F002000 0x00000000
<6>[1228981.525024] PVR_K: 	(T3C-10) 0x0F0C1580 0x00000001 0x00000002 0x00000001
<6>[1228981.532196] PVR_K: 	(T3C-20) 0x0F00AE80 0x00000000 0x00000000 0x00000000
<6>[1228981.539367] PVR_K: 	(T3C-30) 0x00000000 0x00000000 0x00000000 0x00000000
<6>[1228981.546569] PVR_K: 	(T3C-40) 0x00000000 0x00000000 0x00000000 0x00000000
<6>[1228981.553741] PVR_K: 	(T3C-50) 0x00000000 0x0F00AE80 0x00000000 0x00000000
<6>[1228981.560913] PVR_K: 	(T3C-60) 0x0F00AE80 0x00000000 0x00000000 0x0F00AE80
<6>[1228981.568084] PVR_K: 	(T3C-70) 0x00000000 0x00000000 0x0F00AE80 0x00000000
<6>[1228981.575256] PVR_K: 	(T3C-80) 0x00000000 0x00000000 0x00000000 0x0F000000
<6>[1228981.582458] PVR_K: 	(T3C-90) 0x8F224000 0x0F095C00 0x00000000 0x0F08B280
<6>[1228981.589630] PVR_K: 	(T3C-A0) 0x0F00AE80 0x00000000 0x0F08B4A0 0x00000000
<6>[1228981.596801] PVR_K: 	(T3C-B0) 0x0F0AD500 0x00000000 0x00000000 0x00000000
<6>[1228981.603973] PVR_K: 	(T3C-C0) 0x00000000 0x00000000 0x00000000 0x0002DA20
<6>[1228981.611175] PVR_K: 	(T3C-D0) 0x0002DA1E 0x0F000000 0x8000B000 0x8004B000
<6>[1228981.618347] PVR_K: 	(T3C-E0) 0x0F004000 0x0F00A420 0x0F00A740 0x00000000
<6>[1228981.625518] PVR_K: 	(T3C-F0) 0x00000000 0x00000000 0x0000007A 0x0000007A
<6>[1228981.632690] PVR_K: 	(T3C-100) 0x00000000 0x00000003 0x00000000 0x00000000
<6>[1228981.639953] PVR_K: 	(T3C-110) 0x00000001 0x00000000 0x83BCB6FB 0xE42FBCFF
<6>[1228981.647247] PVR_K: SGX Kernel CCB WO:0xA RO:0xA
<3>[1229071.788970] binder: release proc 446, transaction 4582318, not freed
<6>[1260686.660278] wl1271: Beacon loss detected.
<7>[1260686.664733] wlan0: Connection to AP 00:27:22:94:7d:73 lost.
<7>[1260686.670104] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 06 00 00 00 00 00 00 00 00 00 00
<7>[1260686.670135] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1260686.670135] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1260686.670166] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<6>[1260686.754699] cfg80211: Calling CRDA to update world regulatory domain
<3>[1260686.785400] wl1271: ERROR invalid hlid. dropping skb 0xc3e3ba40
<7>[1260688.536804] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 06 00 00 00 00 00 00 00 00 00 00
<7>[1260688.536804] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1260688.536834] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1260688.536834] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1260688.555541] wlan0: authenticate with 00:27:22:80:f2:02 (try 1)
<7>[1260688.576660] wlan0: authenticated
<7>[1260688.609039] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 06 00 00 00 00 00 00 00 00 00 00
<7>[1260688.609069] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1260688.609069] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1260688.609100] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1260688.625488] wlan0: associate with 00:27:22:80:f2:02 (try 1)
<7>[1260688.641571] wlan0: RX ReassocResp from 00:27:22:80:f2:02 (capab=0x431 status=0 aid=2)
<7>[1260688.641601] wlan0: associated
<6>[1260688.706481] ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
<6>[1260688.735565] wl1271: Association completed.
<7>[1260698.785369] wlan0: no IPv6 routers present
<6>[1271204.227447] wl1271: Beacon loss detected.
<7>[1271204.231933] wlan0: Connection to AP 00:27:22:80:f2:02 lost.
<7>[1271204.245025] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 07 00 00 00 00 00 00 00 00 00 00
<7>[1271204.245025] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1271204.245056] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1271204.245056] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<6>[1271204.344360] cfg80211: Calling CRDA to update world regulatory domain
<3>[1271204.363433] wl1271: ERROR invalid hlid. dropping skb 0xc5dae380
<7>[1271206.111541] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 07 00 00 00 00 00 00 00 00 00 00
<7>[1271206.111572] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1271206.111602] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1271206.111602] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1271206.135528] wlan0: authenticate with 00:27:22:94:7d:73 (try 1)
<7>[1271206.160186] wlan0: authenticated
<7>[1271206.205596] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 07 00 00 00 00 00 00 00 00 00 00
<7>[1271206.205627] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1271206.205657] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1271206.205657] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1271206.225494] wlan0: associate with 00:27:22:94:7d:73 (try 1)
<7>[1271206.241241] wlan0: RX ReassocResp from 00:27:22:94:7d:73 (capab=0x431 status=0 aid=3)
<7>[1271206.241271] wlan0: associated
<6>[1271206.305969] ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
<6>[1271206.335571] wl1271: Association completed.
<7>[1271216.535369] wlan0: no IPv6 routers present
<6>[1273351.494659] wl1271: Beacon loss detected.
<7>[1273351.499176] wlan0: Connection to AP 00:27:22:94:7d:73 lost.
<7>[1273351.511535] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 01 00 00 00 00 00 00 00 00 00 00
<7>[1273351.511535] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1273351.511566] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1273351.511566] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<6>[1273351.589263] cfg80211: Calling CRDA to update world regulatory domain
<3>[1273351.615203] wl1271: ERROR invalid hlid. dropping skb 0xc3e3b980
<7>[1273353.362060] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 01 00 00 00 00 00 00 00 00 00 00
<7>[1273353.362091] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1273353.362121] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1273353.362121] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1273353.385559] wlan0: authenticate with 00:27:22:80:f2:02 (try 1)
<7>[1273353.400634] wlan0: authenticated
<7>[1273353.426971] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 01 00 00 00 00 00 00 00 00 00 00
<7>[1273353.427001] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1273353.427032] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1273353.427032] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1273353.445495] wlan0: associate with 00:27:22:80:f2:02 (try 1)
<7>[1273353.459716] wlan0: RX ReassocResp from 00:27:22:80:f2:02 (capab=0x431 status=0 aid=2)
<7>[1273353.459716] wlan0: associated
<6>[1273353.530273] ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
<6>[1273353.565551] wl1271: Association completed.
<7>[1273364.575408] wlan0: no IPv6 routers present
<6>[1289086.627807] wl1271: Beacon loss detected.
<7>[1289086.632293] wlan0: Connection to AP 00:27:22:80:f2:02 lost.
<7>[1289086.644866] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 02 00 00 00 00 00 00 00 00 00 00
<7>[1289086.644866] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1289086.644897] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1289086.644897] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<6>[1289086.743408] cfg80211: Calling CRDA to update world regulatory domain
<3>[1289086.765411] wl1271: ERROR invalid hlid. dropping skb 0xc5dae200
<7>[1289088.544006] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 02 00 00 00 00 00 00 00 00 00 00
<7>[1289088.544036] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1289088.544036] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1289088.544067] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1289088.555511] wlan0: authenticate with 00:27:22:94:7d:73 (try 1)
<7>[1289088.565582] wlan0: authenticated
<7>[1289088.608856] wl1271: CMD_ROLE_START: 00000000: 00 00 05 00 01 02 00 00 00 00 00 00 00 00 00 00
<7>[1289088.608886] wl1271: CMD_ROLE_START: 00000010: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1289088.608917] wl1271: CMD_ROLE_START: 00000020: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1289088.608917] wl1271: CMD_ROLE_START: 00000030: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
<7>[1289088.625457] wlan0: associate with 00:27:22:94:7d:73 (try 1)
<7>[1289088.641571] wlan0: RX ReassocResp from 00:27:22:94:7d:73 (capab=0x431 status=0 aid=3)
<7>[1289088.641601] wlan0: associated
<6>[1289088.706298] ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
<6>[1289088.745513] wl1271: Association completed.
<7>[1289098.955383] wlan0: no IPv6 routers present