Figure 1 is the OVP circuit modified from the one shown in AN1533. The circuit trips at 40V, turning Q1 OFF to disconnect the Cload from VIN. DIN, Q1 and Q2 have to be selected according to transient voltage and the load current. Refer to AN1533 for details of theory of operation.



Jimmy – TI - SVA