

1,According to the schematic diagram and PCB, using the net line flying out of the test




2, Use an on-board Ethernet converter for conversion to an RJ45 interface 

3,Link with computer, load driver



4,The computer displays a yellow icon



5,Ping does not have access to the computer, even if it is changed to the same network segment

