***Dlp3010evm-LC(projector) 與 acA1300-30gm(camera) synchronized problem***

* Dlp3010 set up



[J3] : pin2↔pin3(connector for selecting 3DR signal usage)

[J11]: pin2↔pin3(Header for voltage level selection for trigger-in/out for 3.3V)

|  |  |  |
| --- | --- | --- |
| Projector pin | connect | Camera pin |
| 4(output) | ↔ | 2(input) |
| 5(input) | ↔ | 4(output) |
| 1(GND) | ↔ | 5(GND) |

[J4]:

 (connector in for trigger-in/out selection for light control application)





* Software set up
1. Dlp3010



