# Communications Examples

## Files
file | example_basic_comms_coordinator_afzdo.c

| Resets Radio, configures this device to be a Zigbee Coordinator, and displays any messages that are received. Uses the AF/ZDO interface.
file | example_basic_comms_coordinator_sapi.c

| Resets Radio, configures this device to be a Zigbee Coordinator, and displays any messages that are received. Uses the SIMPLE API.
file | example_basic_comms_end_device_afzdo.c

| Resets Radio, configures this device to be a Zigbee End Device, joins a network, then sends a message to the coordinator every few seconds. Sleeps inbetween transmissions.
file | example_basic_comms_router_afzdo.c

| Resets Radio, configures this device to be a Zigbee Router, joins a network, then sends a message to the coordinator once per second. Uses the AF/ZDO interface. Pressing the button will display device information.
file | example_basic_comms_router_sapi.c

| Resets Radio, configures this device to be a Zigbee Router, joins a network, then sends a message to the coordinator once per second. Uses the SIMPLE API.
file | example_per_tester_coordinator_afzdo.c

| Packet Error Rate Tester: configures this device to be a Zigbee Coordinator and displays how many messages were received. Uses the AF/ZDO interface.
file | example_per_tester_router_afzdo.c

| Packet Error Rate Tester: Resets Radio, configures this device to be a Zigbee Router, joins a network, then sends 1000 messages to coordinator.
file | example_basic_comms_router_afzdo.c

| Resets Radio, configures this device to be a Zigbee Router, joins a network, then sends a message to the coordinator once per second. Uses the AF/ZDO interface. Pressing the button will display device information.
file | example_secure_comms_coordinator_afzdo.c

| Resets Radio, configures this device to be a Zigbee Coordinator, and displays any messages that are received. Uses the AF/ZDO interface.
file | example_secure_comms_router_afzdo.c

| Resets Radio, configures this device to be a Zigbee Router, joins a network, then sends a message to the coordinator once per second. Uses the AF/ZDO interface.

All Data Structures Files Functions Variables Defines