# Hardware Driver Examples

## Files
file | example_accelerometer_interrupt.c

| Configures accelerometer to generate an interrupt when motion is detected.
file | example_button_blink.c

| Toggles LED0 when button pressed.
file | example_hello_world.c

| Outputs "Hello World" to console and toggles LED1 approximately once per second.
file | example_read_accelerometer.c

| Reads accelerometer values in the X-axis, Y-axis, and Z-axis and outputs to console regularly.
file | example_read_light_sensor.c

| Uses the MSP430's internal Analog to Digital Converter (ADC) to read the ambient light sensor value and supply voltage and outputs to console approximately once per second.

All Data Structures Files Functions Variables Defines