# Simple Applications

## Files
file | example_polling_application_coordinator_afzdo.c

| Resets Radio, configures this device to be a Zigbee Coordinator, and waits When button is pressed, sends a message to the end device. Demonstrates how end device automatically polls.
file | example_simple_application_coordinator_afzdo.c

| Resets Radio, configures this device to be a Zigbee Coordinator, and displays any messages that are received. Uses the AF/ZDO interface.
file | example_basic_comms_router_afzdo.c

| Resets Radio, configures this device to be a Zigbee Router, joins a network, then sends a message to the coordinator once per second. Uses the AF/ZDO interface. Pressing the button will display device information.
file | example_basic_comms_router_afzdo.c

| Resets Radio, configures this device to be a Zigbee Router, joins a network, then sends a message to the coordinator once per second. Uses the AF/ZDO interface. Pressing the button will display device information.

## Detailed Description

Note:
  Projects compiled with IAR Embedded Workbench for IAR version 4.21.2

All Data Structures Files Functions Variables Defines