# example_simple_application_router_afzdo.c File Reference

Resets Radio, configures this device to be a Zigbee Router, joins a network, then sends a message to the coordinator. Uses the AF/ZDO interface. More...

`#include "../HAL/hal_mdb1.h"`
`#include "../ZNP/znp_interface.h"`
`#include "../ZNP/application_configuration.h"`
`#include "../ZNP/af_zdo.h"`
`#include "../Common/printf.h"`
`#include "../Common/utilities.h"`
`#include "znp_example_utils.h"`
`#include "Messages/header.h"`
`#include "header.h"`

## Defines
#define | TEST_CLUSTER 0x77
signed int | returnValue
int | main (void)

## Detailed Description

Resets Radio, configures this device to be a Zigbee Router, joins a network, then sends a message to the coordinator. Uses the AF/ZDO interface.

This matches example_simple_application_COORDINATOR.c Get the coordinator running first, or else the router won't have anything to join to.

It is recommended that you get the basic communications examples working first

Rev
  480

Author
  dsmith

Date
  2010-05-03 15:49:48 -0700 (Mon, 03 May 2010)

All Data Structures Files Functions Variables Defines