# pcieLegacyIrqStatusRawReg_s Struct Reference
[PCIE LLD Application Register Definitions]

Specification of the Legacy Raw Interrupt Status Register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
uint8_t | legacyRawStatus
| [rw] Legacy Interrupt Raw Status, RC mode only

## Detailed Description

Specification of the Legacy Raw Interrupt Status Register.

There are multiple instances A-D (0-3) of this register.

## Field Documentation

uint8_t pcieLegacyIrqStatusRawReg_s::legacyRawStatus

[rw] Legacy Interrupt Raw Status, RC mode only

Field size: 1 bit

uint32_t pcieLegacyIrqStatusRawReg_s::raw

[ro] Raw image of register on read; actual value on write

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated