# pcieEpIrqSetReg_s Struct Reference
[PCIE LLD Application Register Definitions]

Specification of the Endpoint Interrupt Request Set Register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
uint8_t | epIrqSet
| [rw] Write 1 to generate assert interrupt message

## Detailed Description

Specification of the Endpoint Interrupt Request Set Register.

## Field Documentation

uint8_t pcieEpIrqSetReg_s::epIrqSet

[rw] Write 1 to generate assert interrupt message

If MSI is disabled, legacy interrupt assert message will be generated. On read, a 1 indicates currently asserted interrupt.

Field size: 1 bit

uint32_t pcieEpIrqSetReg_s::raw

[ro] Raw image of register on read; actual value on write

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated