# pciePcsStatusReg_s Struct Reference
[PCIE LLD Application Register Definitions]

Specification of the PCS Status Register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint8_t | pcsRev
| [ro] PCS RTL Revision.
uint8_t | pcsLnEn
| [ro] PCS lanes enabled status.
uint8_t | pcsTxEn
| [ro] PCS transmitters enabled status.
uint8_t | pcsRxEn
| [ro] PCS receivers enabled status.

## Detailed Description

Specification of the PCS Status Register.

## Field Documentation

uint8_t pciePcsStatusReg_s::pcsLnEn

[ro] PCS lanes enabled status.

Field size: 2 bits

uint8_t pciePcsStatusReg_s::pcsRev

[ro] PCS RTL Revision.

Field size: 3 bits

uint8_t pciePcsStatusReg_s::pcsRxEn

[ro] PCS receivers enabled status.

Field size: 2 bits

uint8_t pciePcsStatusReg_s::pcsTxEn

[ro] PCS transmitters enabled status.

Field size: 2 bits

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated