# CSL_Edma3CfgInfo Struct Reference
[EDMA3 Data Structures]

EDMA3 Configuration Information This describes the configuration information for each EDMA instance. This is populated by the SOC layer for each instance. More...

`#include <csl_edma3.h>`

## Data Fields

Uint8 | numDMAChannel
Uint8 | numQDMAChannel
Uint8 | numINTChannel
Uint16 | numParamsets
Uint8 | numEvque
Uint8 | numRegions
Bool | IsChannelMapping
Bool | IsMemoryProtection

## Detailed Description

EDMA3 Configuration Information This describes the configuration information for each EDMA instance. This is populated by the SOC layer for each instance.

## Field Documentation

Bool CSL_Edma3CfgInfo::IsChannelMapping

This indicates if the instance supports Channel Mapping.

Bool CSL_Edma3CfgInfo::IsMemoryProtection

This indicates if the instance supports Memory Protection.

Uint8 CSL_Edma3CfgInfo::numDMAChannel

This is the number of DMA channels supported by this instance

Uint8 CSL_Edma3CfgInfo::numEvque

This is the number of Event Queues supported by this instance

Uint8 CSL_Edma3CfgInfo::numINTChannel

This is the number of Interrupt Channels supported by this instance

Uint16 CSL_Edma3CfgInfo::numParamsets

This is the number of PARAM Sets supported by this instance

Uint8 CSL_Edma3CfgInfo::numQDMAChannel

This is the number of QDMA channels supported by this instance

Uint8 CSL_Edma3CfgInfo::numRegions

This is the number of regions supported by this instance

The documentation for this struct was generated from the following file:

- csl_edma3.h

Copyright 2012, Texas Instruments Incorporated