# hyplnkIntCtrlIdxReg_s Struct Reference
[HYPLNK LLD Register Definitions]

Specification of the Interupt Control Index Register. More...

`#include <hyplnk.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint8_t | intCtrlIdx
| [rw] Selects interrupt control value register

## Detailed Description

Specification of the Interupt Control Index Register.

The Interrupt Control Index Register is used to control which hardware or software internal control register is read or written via hyplnkIntCtrlValReg_s.

## Field Documentation

uint8_t hyplnkIntCtrlIdxReg_s::intCtrlIdx

[rw] Selects interrupt control value register

Field size: 8 bits

The specified array element can be read or written via hyplnkIntCtrlValReg_s after the index is written.

The documentation for this struct was generated from the following file:

- hyplnk.h

Copyright 2012, Texas Instruments Incorporated