# pcieCfgTransReg_s Struct Reference
[PCIE LLD Application Register Definitions]

Specification of the Configuration Transaction Setup Register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint8_t | type
| [rw] Configuration type for outbound configuration accesses
uint8_t | bus
| [rw] PCIe bus number for outbound configuration accesses
uint8_t | device
| [rw] PCIe device number for outbound configuration accesses
uint8_t | func
| [rw] PCIe function number for outbound configuration accesses

## Detailed Description

Specification of the Configuration Transaction Setup Register.

## Field Documentation

uint8_t pcieCfgTransReg_s::bus

[rw] PCIe bus number for outbound configuration accesses

Field size: 8 bits

uint8_t pcieCfgTransReg_s::device

[rw] PCIe device number for outbound configuration accesses

Field size: 5 bit

uint8_t pcieCfgTransReg_s::func

[rw] PCIe function number for outbound configuration accesses

Field size: 3 bits

uint8_t pcieCfgTransReg_s::type

[rw] Configuration type for outbound configuration accesses

0 = Type 0 access. 1 = Type 1 access.

Field size: 1 bit

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated