# pciePmCmdReg_s Struct Reference
[PCIE LLD Application Register Definitions]

Specification of the Power Management Command Register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint8_t | turnOff
| [w1] PM Turn off
uint8_t | pme
| [w1] Transmit PM PME message

## Detailed Description

Specification of the Power Management Command Register.

## Field Documentation

uint8_t pciePmCmdReg_s::pme

[w1] Transmit PM PME message

Write 1 to transmit a PM_PME message. Reads 0. Applicable to EP mode only.

0 = No effect
1 = Transmit a PM_PME message

Field size: 1 bit

uint8_t pciePmCmdReg_s::turnOff

[w1] PM Turn off

Write 1 to transmit a PM_TURNOFF message. Reads 0. Applicable in RC mode only.

0 = No effect
1 = Transmit a PM_TURNOFF message

Field size: 1 bit

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated