# QMSS Low Level Driver Data Structures
[QMSS, QMSS Low Level Driver Symbols Defined]

## Data Structures

struct | Qmss_AccCmdCfg
| Accumulator Command interface structure. More...
struct | Qmss_StartCfg
| QMSS start configuration structure. More...
struct | Qmss_Queue
| Queue definition. More...
struct | Qmss_QueueNumRange
| Queue definition. More...
struct | Qmss_DescCfg
| descriptor configuration structure More...
struct | Qmss_MemRegInfo
| Memory region configuration information structure. More...
struct | Qmss_MemRegCfg
| Memory region configuration information structure of all memory regions. More...
struct | Qmss_PdspCfg
| QMSS PDSP firmware download information structure. More...
struct | Qmss_InitCfg
| QMSS configuration structure. More...
struct | Qmss_GlobalConfigParams
| QMSS Global configuration structure definition. More...
struct | Qmss_QosQueueCfg
| QoS queue configuration structure. More...
struct | Qmss_QosClusterCfgTB
| QoS cluster configuration structure for Modified Token Bucket. More...
struct | Qmss_QosSchedQueueCfg
| QoS scheduler queue configuration structure. More...
struct | Qmss_QosSchedGroupCfg
| QoS scheduler group configuration. More...
struct | Qmss_QosSchedPortCfg
| QoS scheduler port configuration. More...

## Typedefs

typedef void * | Qmss_RmHnd
| QMSS RM Handle.
typedef int32_t | Qmss_QueueHnd
| Queue handle.
typedef int32_t | Qmss_Result
| QMSS return result.
typedef uint32_t * | Qmss_QueuePushHnd
| Handle used in the "Fast Push" set of APIs.

## Variables

Qmss_GlobalConfigParams | sample_qmssGblCfgParams []
| QMSS LLD initialization parameters.
Qmss_GlobalConfigParams | qmssGblCfgParams []
| QMSS LLD initialization parameters.
uint8_t | Qmss_cdmaEoiVector []
| INTD EOI vector map for CDMA interrupt.
uint8_t | Qmss_highEoiVector []
| INTD EOI vector map for each high priority interrupt.
uint8_t | Qmss_lowEoiVector []
| INTD EOI vector map for each low priority interrupt.
const unsigned int | acc32_le []
| PDSP Firmware symbols.
const unsigned int | acc32_be []
| 32 channel high priority accumulation big endian firmware
const unsigned int | acc16_le []
| 16 channel low priority accumulation little endian firmware
const unsigned int | acc16_be []
| 16 channel low priority accumulation big endian firmware
const unsigned int | acc48_le []
| 48 channel combined high and low priority accumulation little endian firmware
const unsigned int | acc48_be []
| 48 channel combined high and low priority accumulation big endian firmware
const unsigned int | qos_le []
| QoS little endian firmware.
const unsigned int | qos_be []
| QoS big endian firmware.
const unsigned int | qos_sched_le []
| QoS scheduler little endian firmware.
const unsigned int | qos_sched_be []
| QoS scheduler big endian firmware.

## Variable Documentation

const unsigned int acc32_le[]

PDSP Firmware symbols.

32 channel high priority accumulation little endian firmware

Copyright 2012, Texas Instruments Incorporated