# pcieRootStatusReg_s Struct Reference
[PCIE LLD Capabilities Register Definitions]

Specification of the Root Status and Control register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
uint8_t | pmePend
| [ro] Indicates that another PME is pending when the PME Status bit is Set.
uint8_t | pmeStatus
| [rw] Indicates that PME was asserted by the PME Requester.
uint16_t | pmeReqID
| [ro] ID of the last PME Requester.

## Detailed Description

Specification of the Root Status and Control register.

This register may only be used for root complex mode.

## Field Documentation

uint8_t pcieRootStatusReg_s::pmePend

[ro] Indicates that another PME is pending when the PME Status bit is Set.

Field size: 1 bit

uint16_t pcieRootStatusReg_s::pmeReqID

[ro] ID of the last PME Requester.

This field is only valid when the PME Status bit is Set.

Field size: 16 bits

uint8_t pcieRootStatusReg_s::pmeStatus

[rw] Indicates that PME was asserted by the PME Requester.

Write 1 to clear

Field size: 1 bit

uint32_t pcieRootStatusReg_s::raw

[ro] Raw image of register on read; actual value on write

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated