# hyplnkIntPtrValReg_s Struct Reference
[HYPLNK LLD Register Definitions]

Specification of the Interrupt Control Value Register. More...

`#include <hyplnk.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint32_t | intPtr
| [rw] Specifies an interrupt pointer

## Detailed Description

Specification of the Interrupt Control Value Register.

The Interrupt Pointer Value is used to write or read to the interrupt pointer number (intPtrIdx) This allows the remote interrupts to interrupt any MicroProcessor. Values written are stored in the Interrupt Pointer for that MicroProcessor.

## Field Documentation

uint32_t hyplnkIntPtrValReg_s::intPtr

[rw] Specifies an interrupt pointer

Field size: 30 bits

This allows the remote interrupts to interrupt any MicroProcessor. Values written are stored in the Interrupt Pointer for that MicroProcessor.

The documentation for this struct was generated from the following file:

- hyplnk.h

Copyright 2012, Texas Instruments Incorporated