# _EMAC_Config Struct Reference
[EMAC Data Structures]

EMAC_Config. More...

`#include <csl_emac.h>`

## Data Fields

EMAC_Common_Config | EMACCommonConfig
EMAC_Core_Config | EMACCoreConfig

## Detailed Description

EMAC_Config.

The EMAC_Config structure defines how the EMAC device should operate. It is passed to the device when the device is opened (EMAC_open()), and remains in effect until the device is closed (EMAC_close).

The following is a short description of the configuration fields:

EMACCommonConfig - Specify configurations common to all the cores

EMACCoreConfig - Specify configurations specific to individual cores

## Field Documentation

EMAC_Common_Config _EMAC_Config::EMACCommonConfig

Configurations common to all the cores

EMAC_Core_Config _EMAC_Config::EMACCoreConfig

Configurations specific to individual cores

The documentation for this struct was generated from the following file:

- csl_emac.h

Copyright 2012, Texas Instruments Incorporated