- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

# EMAC_CONFIG_INFO_tag Struct Reference

EMAC configuration data structure. More...

`#include <emac_drv.h>`

## Data Fields

EMAC_PKT_FILTER_T | rx_filter
Uint32 | mcast_cnt
Uint8 * | p_mcast_list

## Detailed Description

EMAC configuration data structure.

## Field Documentation

EMAC_PKT_FILTER_T EMAC_CONFIG_INFO_tag::rx_filter

EMAC RX filter, e.g. broadcast, multicast, etc.

Uint32 EMAC_CONFIG_INFO_tag::mcast_cnt

Multicast address count, if mcast_cnt=0, p_mcast_list can be NULL

Uint8* EMAC_CONFIG_INFO_tag::p_mcast_list

Pointer to the multicast list of which size is mcast_cnt*6 in bytes

The documentation for this struct was generated from the following file:

- emac_drv.h

Copyright 2012, Texas Instruments Incorporated