# Cppi_RxChInitCfg Struct Reference
[CPPI Low Level Driver Data Structures]

CPPI receive channel configuration structure. More...

`#include <cppi_drv.h>`

## Data Fields

int32_t | channelNum
Cppi_ChState | rxEnable

## Detailed Description

CPPI receive channel configuration structure.

## Field Documentation

int32_t Cppi_RxChInitCfg::channelNum

Channel number If channelNum is set to CPPI_PARAM_NOT_SPECIFIED then the next available channel will be allocated

Cppi_ChState Cppi_RxChInitCfg::rxEnable

Enable Rx Channel on creation. If not set use CPPI_channelEnable() API to enable it later

The documentation for this struct was generated from the following file:

- cppi_drv.h

Copyright 2012, Texas Instruments Incorporated