# EDMA3 Functions
[EDMA3]

## Functions

CSL_Status | CSL_edma3Init (CSL_Edma3Context *pContext)
CSL_Edma3Handle | CSL_edma3Open (CSL_Edma3Obj *edmaObj, CSL_InstNum edmaNum, CSL_Edma3ModuleAttr *attr, CSL_Status *status)
CSL_Status | CSL_edma3Close (CSL_Edma3Handle hEdma)
CSL_Status | CSL_edma3HwSetup (CSL_Edma3Handle hMod, CSL_Edma3HwSetup *setup)
CSL_Status | CSL_edma3GetHwSetup (CSL_Edma3Handle hMod, CSL_Edma3HwSetup *setup)
CSL_Status | CSL_edma3HwControl (CSL_Edma3Handle hMod, CSL_Edma3HwControlCmd cmd, void *cmdArg)
CSL_Status | CSL_edma3ccGetModuleBaseAddr (CSL_InstNum edmaNum, CSL_Edma3ModuleAttr *pAttr, CSL_Edma3ModuleBaseAddress *pBaseAddress, CSL_Edma3CfgInfo *pCfgInfo)
CSL_Status | CSL_edma3GetHwStatus (CSL_Edma3Handle hMod, CSL_Edma3HwStatusQuery myQuery, void *response)
CSL_Edma3ChannelHandle | CSL_edma3ChannelOpen (CSL_Edma3ChannelObj *edmaObj, CSL_InstNum edmaNum, CSL_Edma3ChannelAttr *chAttr, CSL_Status *status)
CSL_Status | CSL_edma3ChannelClose (CSL_Edma3ChannelHandle hEdma)
CSL_Status | CSL_edma3HwChannelSetupParam (CSL_Edma3ChannelHandle hEdma, Uint16 paramNum)
CSL_Status | CSL_edma3HwChannelSetupTriggerWord (CSL_Edma3ChannelHandle hEdma, Uint8 triggerWord)
CSL_Status | CSL_edma3HwChannelSetupQue (CSL_Edma3ChannelHandle hEdma, CSL_Edma3Que que)
CSL_Status | CSL_edma3GetHwChannelSetupParam (CSL_Edma3ChannelHandle hEdma, Uint16 *paramNum)
CSL_Status | CSL_edma3GetHwChannelSetupTriggerWord (CSL_Edma3ChannelHandle hEdma, Uint8 *triggerWord)
CSL_Status | CSL_edma3GetHwChannelSetupQue (CSL_Edma3ChannelHandle hEdma, CSL_Edma3Que *que)
CSL_Status | CSL_edma3HwChannelControl (CSL_Edma3ChannelHandle hCh, CSL_Edma3HwChannelControlCmd cmd, void *cmdArg)
CSL_Status | CSL_edma3GetHwChannelStatus (CSL_Edma3ChannelHandle hCh, CSL_Edma3HwChannelStatusQuery myQuery, void *response)
CSL_Edma3ParamHandle | CSL_edma3GetParamHandle (CSL_Edma3ChannelHandle hEdma, Int16 paramNum, CSL_Status *status)
CSL_Status | CSL_edma3ParamSetup (CSL_Edma3ParamHandle hParam, CSL_Edma3ParamSetup *pSetup)
CSL_Status | CSL_edma3ParamWriteWord (CSL_Edma3ParamHandle hParamHndl, Uint16 wordOffset, Uint32 word)
CSL_IDEF_INLINE void | CSL_edma3GetInfo (CSL_Edma3Handle hModule, CSL_Edma3QueryInfo *response)
CSL_IDEF_INLINE void | CSL_edma3MapDMAChannelToParamBlock (CSL_Edma3Handle hModule, Uint8 dmaChannel, Uint16 paramId)
CSL_IDEF_INLINE Uint16 | CSL_edma3GetDMAChannelToParamBlockMapping (CSL_Edma3Handle hModule, Uint8 dmaChannel)
CSL_IDEF_INLINE void | CSL_edma3MapQDMAChannelToParamBlock (CSL_Edma3Handle hModule, Uint8 qdmaChannel, Uint16 paramId)
CSL_IDEF_INLINE Uint16 | CSL_edma3GetQDMAChannelToParamBlockMapping (CSL_Edma3Handle hModule, Uint8 qdmaChannel)
CSL_IDEF_INLINE void | CSL_edma3SetQDMATriggerWord (CSL_Edma3Handle hModule, Uint8 qdmaChannel, Uint8 trword)
CSL_IDEF_INLINE void | CSL_edma3GetQDMATriggerWord (CSL_Edma3Handle hModule, Uint8 qdmaChannel, Uint8 *trword)
CSL_IDEF_INLINE void | CSL_edma3MapDMAChannelToEventQueue (CSL_Edma3Handle hModule, Uint8 dmaChannel, Uint8 eventQueue)
CSL_IDEF_INLINE Uint8 | CSL_edma3GetDMAChannelToEventQueueMapping (CSL_Edma3Handle hModule, Uint8 dmaChannel)
CSL_IDEF_INLINE void | CSL_edma3MapQDMAChannelToEventQueue (CSL_Edma3Handle hModule, Uint8 qdmaChannel, Uint8 eventQueue)
CSL_IDEF_INLINE Uint8 | CSL_edma3GetQDMAChannelToEventQueueMapping (CSL_Edma3Handle hModule, Uint8 qdmaChannel)
CSL_IDEF_INLINE void | CSL_edma3MapEventQueueToTC (CSL_Edma3Handle hModule, Uint8 eventQueue, Uint8 tcNum)
CSL_IDEF_INLINE Uint8 | CSL_edma3GetEventQueueToTCMapping (CSL_Edma3Handle hModule, Uint8 eventQueue)
CSL_IDEF_INLINE void | CSL_edma3SetEventQueuePriority (CSL_Edma3Handle hModule, Uint8 eventQueue, Uint8 priority)
CSL_IDEF_INLINE Uint8 | CSL_edma3GetEventQueuePriority (CSL_Edma3Handle hModule, Uint8 eventQueue)
CSL_IDEF_INLINE void | CSL_edma3GetEventMissed (CSL_Edma3Handle hModule, CSL_BitMask32 *missedLo, CSL_BitMask32 *missedHi, CSL_BitMask32 *missedQdma)
CSL_IDEF_INLINE void | CSL_edma3IsDMAChannelMissedEventSet (CSL_Edma3Handle hModule, Uint8 dmaChannel, Bool *response)
CSL_IDEF_INLINE void | CSL_edma3IsQDMAChannelMissedEventSet (CSL_Edma3Handle hModule, Uint8 qdmaChannel, Bool *response)
CSL_IDEF_INLINE void | CSL_edma3EventsMissedClear (CSL_Edma3Handle hModule, CSL_BitMask32 missedLo, CSL_BitMask32 missedHi, CSL_BitMask32 missedQdma)
CSL_IDEF_INLINE void | CSL_edma3ClearDMAMissedEvent (CSL_Edma3Handle hModule, Uint8 dmaChannel)
CSL_IDEF_INLINE void | CSL_edma3ClearQDMAMissedEvent (CSL_Edma3Handle hModule, Uint8 qdmaChannel)
CSL_IDEF_INLINE void | CSL_edma3GetControllerError (CSL_Edma3Handle hModule, CSL_Edma3CtrlErrStat *ccStat)
CSL_IDEF_INLINE void | CSL_edma3ClearControllerError (CSL_Edma3Handle hModule, CSL_Edma3CtrlErrStat *ccStat)
CSL_IDEF_INLINE void | CSL_edma3ErrorEval (CSL_Edma3Handle hModule)
CSL_IDEF_INLINE void | CSL_edma3DmaRegionAccessEnable (CSL_Edma3Handle hModule, Int edmaRegion, CSL_BitMask32 drae, CSL_BitMask32 draeh)
CSL_IDEF_INLINE void | CSL_edma3DmaRegionAccessDisable (CSL_Edma3Handle hModule, Int edmaRegion, CSL_BitMask32 drae, CSL_BitMask32 draeh)
CSL_IDEF_INLINE void | CSL_edma3QdmaRegionAccessEnable (CSL_Edma3Handle hModule, Int edmaRegion, CSL_BitMask32 qrae)
CSL_IDEF_INLINE void | CSL_edma3QdmaRegionAccessDisable (CSL_Edma3Handle hModule, Int edmaRegion, CSL_BitMask32 qrae)
CSL_IDEF_INLINE void | CSL_edma3GetWaterMark (CSL_Edma3Handle hModule, Uint8 eventQueue, Uint8 *waterMark)
CSL_IDEF_INLINE void | CSL_edma3GetNumberValidEntries (CSL_Edma3Handle hModule, Uint8 eventQueue, Uint8 *numValidEntries)
CSL_IDEF_INLINE void | CSL_edma3GetStartPointer (CSL_Edma3Handle hModule, Uint8 eventQueue, Uint8 *startPtr)
CSL_IDEF_INLINE void | CSL_edma3GetThresholdExceeded (CSL_Edma3Handle hModule, Uint8 eventQueue, Bool *thresholdExceeded)
CSL_IDEF_INLINE void | CSL_edma3EventQueueThresholdSet (CSL_Edma3Handle hModule, Uint8 eventQueue, Uint8 threshold)
CSL_IDEF_INLINE void | CSL_edma3GetActivityStatus (CSL_Edma3Handle hModule, CSL_Edma3ActivityStat *activityStat)
CSL_IDEF_INLINE void | CSL_edma3GetMemoryFaultError (CSL_Edma3Handle hModule, CSL_Edma3MemFaultStat *memFault)
CSL_IDEF_INLINE void | CSL_edma3MemFaultClear (CSL_Edma3Handle hModule)
CSL_IDEF_INLINE void | CSL_edma3GetMemoryProtectionAttrib (CSL_Edma3Handle hModule, Int region, CSL_BitMask32 *mppa)
CSL_IDEF_INLINE void | CSL_edma3SetMemoryProtectionAttrib (CSL_Edma3Handle hModule, Int region, CSL_BitMask32 mppa)
CSL_IDEF_INLINE void | CSL_edma3IsDMAChannelEventPending (CSL_Edma3Handle hModule, Uint8 dmaChannel, Bool *response)
CSL_IDEF_INLINE void | CSL_edma3ClearDMAChannelEvent (CSL_Edma3Handle hModule, Int region, Uint8 dmaChannel)
CSL_IDEF_INLINE void | CSL_edma3SetDMAChannelEvent (CSL_Edma3Handle hModule, Int region, Uint8 dmaChannel)
CSL_IDEF_INLINE void | CSL_edma3DMAChannelDisable (CSL_Edma3Handle hModule, Int region, Uint8 dmaChannel)
CSL_IDEF_INLINE void | CSL_edma3DMAChannelEnable (CSL_Edma3Handle hModule, Int region, Uint8 dmaChannel)
CSL_IDEF_INLINE void | CSL_edma3GetDMASecondaryEvents (CSL_Edma3Handle hModule, CSL_BitMask32 *secEventLo, CSL_BitMask32 *secEventHi)
CSL_IDEF_INLINE void | CSL_edma3IsDMAChannelSecondaryEventSet (CSL_Edma3Handle hModule, Uint8 dmaChannel, Bool *response)
CSL_IDEF_INLINE void | CSL_edma3ClearDMASecondaryEvents (CSL_Edma3Handle hModule, CSL_BitMask32 secEventLo, CSL_BitMask32 secEventHi)
CSL_IDEF_INLINE void | CSL_edma3ClearDMAChannelSecondaryEvents (CSL_Edma3Handle hModule, Uint8 dmaChannel)
CSL_IDEF_INLINE void | CSL_edma3InterruptLoDisable (CSL_Edma3Handle hModule, Int region, CSL_BitMask32 intrLo)
CSL_IDEF_INLINE void | CSL_edma3InterruptHiDisable (CSL_Edma3Handle hModule, Int region, CSL_BitMask32 intrHi)
CSL_IDEF_INLINE void | CSL_edma3InterruptLoEnable (CSL_Edma3Handle hModule, Int region, CSL_BitMask32 intrLo)
CSL_IDEF_INLINE void | CSL_edma3InterruptHiEnable (CSL_Edma3Handle hModule, Int region, CSL_BitMask32 intrHi)
CSL_IDEF_INLINE void | CSL_edma3GetLoPendingInterrupts (CSL_Edma3Handle hModule, Int region, CSL_BitMask32 *intrLo)
CSL_IDEF_INLINE void | CSL_edma3GetHiPendingInterrupts (CSL_Edma3Handle hModule, Int region, CSL_BitMask32 *intrHi)
CSL_IDEF_INLINE void | CSL_edma3ClearLoPendingInterrupts (CSL_Edma3Handle hModule, Int region, CSL_BitMask32 intrLo)
CSL_IDEF_INLINE void | CSL_edma3ClearHiPendingInterrupts (CSL_Edma3Handle hModule, Int region, CSL_BitMask32 intrHi)
CSL_IDEF_INLINE void | CSL_edma3InterruptEval (CSL_Edma3Handle hModule, Int region)
CSL_IDEF_INLINE void | CSL_edma3IsQDMAChannelEventPending (CSL_Edma3Handle hModule, Uint8 qdmaChannel, Bool *response)
CSL_IDEF_INLINE void | CSL_edma3QDMAChannelEnable (CSL_Edma3Handle hModule, Int region, Uint8 qdmaChannel)
CSL_IDEF_INLINE void | CSL_edma3QDMAChannelDisable (CSL_Edma3Handle hModule, Int region, Uint8 qdmaChannel)
CSL_IDEF_INLINE void | CSL_edma3GetQDMASecondaryEvents (CSL_Edma3Handle hModule, Uint32 *qdmaSecEvent)
CSL_IDEF_INLINE void | CSL_edma3IsQDMAChannelSecondaryEventSet (CSL_Edma3Handle hModule, Uint8 qdmaChannel, Bool *response)
CSL_IDEF_INLINE void | CSL_edma3ClearQDMASecondaryEvents (CSL_Edma3Handle hModule, Uint32 qdmaSecEvent)
CSL_IDEF_INLINE void | CSL_edma3ClearQDMAChannelSecondaryEvents (CSL_Edma3Handle hModule, Uint8 qdmaChannel)

## Function Documentation

CSL_Status CSL_edma3ccGetModuleBaseAddr | ( | CSL_InstNum | edmaNum,
|  | CSL_Edma3ModuleAttr * | pParam,
|  | CSL_Edma3ModuleBaseAddress * | pBaseAddress,
|  | CSL_Edma3CfgInfo * | pCfgInfo |
| ) |  |  |

============================================================================
CSL_edma3ccGetModuleBaseAddr

Description
This function is used for getting the base-address of the peripheral instance. This function will be called inside the @ CSL_edma3Open()/ CSL_edma3ChannelOpen() function call.

Note: This function is open for re-implementing if the user wants to modify the base address of the peripheral object to point to a different location and there by allow CSL initiated write/reads into peripheral MMR's go to an alternate location.

Arguments

                edmaNum         Specifies the instance of the edma to be opened.
                pParam          Module specific parameters.
                pBaseAddress    Pointer to baseaddress structure containing base
                                address details.
                pCfgInfo        Pointer to the EDMA CC Instance information populated
                                by this API.

Return Value
Success - CSL_SOK
Error - CSL_ESYS_FAIL (Timer Instance is invalid)
Error - CSL_ESYS_INVPARAMS (The parameter passed is invalid)

Pre Condition
None

Post Condition
Base Address structure is populated

Affects
None.

Example

            CSL_Status                   status;
            CSL_Edma3ModuleBaseAddress   baseAddress;
            CSL_Edma3CfgInfo             cfgInfo;

            // Get the EDMA CC Instance 0 Information
            status = CSL_edma3ccGetModuleBaseAddr(0, NULL, &baseAddress, &cfgInfo);

===========================================================================

CSL_Status CSL_edma3ChannelClose | ( | CSL_Edma3ChannelHandle | hEdma | ) |

============================================================================
csl_edma3ChannelClose.c

Description
This function marks the channel cannot be accessed anymore using the handle. CSL for the EDMA channel need to be reopened before using any edma channel.

Arguments

                hEdma           Handle to the channel to be closed.

Return Value
Success - CSL_SOK
Error - CSL_ESYS_BADHANDLE (The handle passed is invalid)

Pre Condition
Functions CSL_edma3Init(), CSL_edma3Open(), CSL_edma3ChannelOpen() must be invoked successfully in that order before this API can be invoked.

Post Condition
The edma channel related CSL APIs can not be called until the edma channel is reopened again using CSL_edma3ChannelOpen()

Example

                CSL_Edma3Handle             hModule;
                CSL_Edma3Obj                edmaObj;
                CSL_Edma3ChannelObj         chObj;
                CSL_Edma3ChannelHandle      hChannel;
                CSL_Edma3ChannelAttr        chAttr;
                CSL_Status                  status;

                // Module Initialization
                CSL_edma3Init(NULL);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, 0, NULL,&status);

                // Channel 0 Open in context of Shadow region 0
                chAttr.regionNum = CSL_EDMA3_REGION_0;
                chAttr.chaNum    = 0;
                hChannel = CSL_edma3ChannelOpen(&chObj, 0, &chAttr, &status);
                ...
                // Close Channel
                CSL_edma3ChannelClose(hChannel);
                ...

=============================================================================

CSL_Edma3ChannelHandle CSL_edma3ChannelOpen | ( | CSL_Edma3ChannelObj * | pEdmaObj,
|  | CSL_InstNum | edmaNum,
|  | CSL_Edma3ChannelAttr * | pChAttr,
|  | CSL_Status * | pStatus |
| ) |  |  |

============================================================================
CSL_edma3ChannelOpen

Description
The API returns a handle for the specified EDMA Channel for use. The channel can be re-opened anytime after it has been normally closed if so required. The handle returned by this call is input as an essential argument for many of the APIs described for this module.

Arguments

                pEdmaObj         pointer to the object that holds reference to the
                                 channel instance of the Specified DMA
                edmaNum          Instance of EDMA whose channel is requested
                pChAttr          Channel Attributes which describe the channel to
                                 be opened.
                status           Status of the function call

Return Value
Success - Channel Handle
Error - NULL

Pre Condition
CSL_edma3Init(), CSL_edma3Open() must be invoked successfully in that order before this API can be invoked

Post Condition EDMA channel object structure is populated

Affects
None

Example

                CSL_Edma3Handle             hModule;
                CSL_Edma3Obj                edmaObj;
                CSL_Edma3ChannelObj         chObj;
                CSL_Edma3ChannelHandle      hChannel;
                CSL_Edma3ChannelAttr        chAttr;
                CSL_Status                  status;

                // Module Initialization
                CSL_edma3Init(NULL);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, 0, NULL,&status);

                // Channel 0 Open in context of Shadow region 0
                chAttr.regionNum = CSL_EDMA3_REGION_0;
                chAttr.chaNum    = 0;
                hChannel = CSL_edma3ChannelOpen(&chObj, 0, &chAttr, &status);
                ...

=============================================================================

CSL_IDEF_INLINE void CSL_edma3ClearControllerError | ( | CSL_Edma3Handle | hModule,
|  | CSL_Edma3CtrlErrStat * | ccStat |
| ) |  |  |

============================================================================
CSL_edma3ClearControllerError

Description
Channel Controller Error Fault.

Arguments

            hModule           Module Handle
            ccStat            Error Status which is to be cleared.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_CCERRCLR_QTHRXD0;TPCC_TPCC_CCERRCLR_QTHRXD1;TPCC_TPCC_CCERRCLR_QTHRXD2; TPCC_TPCC_CCERRCLR_QTHRXD3;TPCC_TPCC_CCERRCLR_QTHRXD4;TPCC_TPCC_CCERRCLR_QTHRXD5; TPCC_TPCC_CCERRCLR_QTHRXD6;TPCC_TPCC_CCERRCLR_QTHRXD7, TPCC_TPCC_CCERR_TCCERR

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                CSL_Edma3CtrlErrStat    ccError;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Get Controller Error
                status = CSL_edma3GetControllerError(hModule,&ccError);
                ...
                // Clear the error.
                CSL_edma3ClearControllerError(hModule,&ccError);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3ClearDMAChannelEvent | ( | CSL_Edma3Handle | hModule,
|  | Int | region,
|  | Uint8 | dmaChannel |
| ) |  |  |

============================================================================
CSL_edma3ClearDMAChannelEvent

Description
This API clears the event for the specific DMA channel.

Arguments

            hModule         Module Handle
            region          Region (Shadow or Global)
            dmaChannel      DMA Channel for which the event is cleared.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_ECR_E0=1;TPCC_TPCC_ECR_E1=1;TPCC_TPCC_ECR_E2=1;TPCC_TPCC_ECR_E3=1; TPCC_TPCC_ECR_E4=1;TPCC_TPCC_ECR_E5=1;TPCC_TPCC_ECR_E6=1;TPCC_TPCC_ECR_E7=1; TPCC_TPCC_ECR_E8=1;TPCC_TPCC_ECR_E9=1;TPCC_TPCC_ECR_E10=1;TPCC_TPCC_ECR_E11=1; TPCC_TPCC_ECR_E12=1;TPCC_TPCC_ECR_E13=1;TPCC_TPCC_ECR_E14=1;TPCC_TPCC_ECR_E15=1; TPCC_TPCC_ECR_E16=1;TPCC_TPCC_ECR_E17=1;TPCC_TPCC_ECR_E18=1;TPCC_TPCC_ECR_E19=1; TPCC_TPCC_ECR_E20=1;TPCC_TPCC_ECR_E21=1;TPCC_TPCC_ECR_E22=1;TPCC_TPCC_ECR_E23=1; TPCC_TPCC_ECR_E24=1;TPCC_TPCC_ECR_E25=1;TPCC_TPCC_ECR_E26=1;TPCC_TPCC_ECR_E27=1; TPCC_TPCC_ECR_E28=1;TPCC_TPCC_ECR_E29=1;TPCC_TPCC_ECR_E30=1;TPCC_TPCC_ECR_E31=1;
TPCC_TPCC_ECRH_E32=1;TPCC_TPCC_ECRH_E33=1;TPCC_TPCC_ECRH_E34=1;TPCC_TPCC_ECRH_E35=1; TPCC_TPCC_ECRH_E36=1;TPCC_TPCC_ECRH_E37=1;TPCC_TPCC_ECRH_E38=1;TPCC_TPCC_ECRH_E39=1; TPCC_TPCC_ECRH_E40=1;TPCC_TPCC_ECRH_E41=1;TPCC_TPCC_ECRH_E42=1;TPCC_TPCC_ECRH_E43=1; TPCC_TPCC_ECRH_E44=1;TPCC_TPCC_ECRH_E45=1;TPCC_TPCC_ECRH_E46=1;TPCC_TPCC_ECRH_E47=1; TPCC_TPCC_ECRH_E48=1;TPCC_TPCC_ECRH_E49=1;TPCC_TPCC_ECRH_E50=1;TPCC_TPCC_ECRH_E51=1; TPCC_TPCC_ECRH_E52=1;TPCC_TPCC_ECRH_E53=1;TPCC_TPCC_ECRH_E54=1;TPCC_TPCC_ECRH_E55=1; TPCC_TPCC_ECRH_E56=1;TPCC_TPCC_ECRH_E57=1;TPCC_TPCC_ECRH_E58=1;TPCC_TPCC_ECRH_E59=1; TPCC_TPCC_ECRH_E60=1;TPCC_TPCC_ECRH_E61=1;TPCC_TPCC_ECRH_E62=1;TPCC_TPCC_ECRH_E63=1;

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                Bool                    dmaStatus;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Get DMA Channel 0 Status
                CSL_edma3GetDMAChannelEvent(hModule, 0, &dmaStatus);
                if (dmaStatus == TRUE)
                {
                    // DMA Channel 0 is active...
                    ...
                    // Clear DMA Channel 0.
                    CSL_edma3ClearDMAChannelEvent (hModule, CSL_EDMA3_REGION_GLOBAL, 0);
                }

===========================================================================

CSL_IDEF_INLINE void CSL_edma3ClearDMAChannelSecondaryEvents | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | dmaChannel |
| ) |  |  |

============================================================================
CSL_edma3ClearDMAChannelSecondaryEvents

Description
This API clears the DMA Secondary Event for a specific DMA Channel.

Arguments

            hModule         Module Handle
            qdmaChannel     DMA Channel for which the secondary event is to be cleared.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_SECR_SECR0=1;TPCC_TPCC_SECR_SECR1=1;TPCC_TPCC_SECR_SECR2=1; TPCC_TPCC_SECR_SECR3=1;TPCC_TPCC_SECR_SECR4=1;TPCC_TPCC_SECR_SECR5=1; TPCC_TPCC_SECR_SECR6=1;TPCC_TPCC_SECR_SECR7=1;TPCC_TPCC_SECR_SECR8=1; TPCC_TPCC_SECR_SECR9=1;TPCC_TPCC_SECR_SECR10=1;TPCC_TPCC_SECR_SECR11=1; TPCC_TPCC_SECR_SECR12=1;TPCC_TPCC_SECR_SECR13=1;TPCC_TPCC_SECR_SECR14=1; TPCC_TPCC_SECR_SECR15=1;TPCC_TPCC_SECR_SECR16=1;TPCC_TPCC_SECR_SECR17=1; TPCC_TPCC_SECR_SECR18=1;TPCC_TPCC_SECR_SECR19=1;TPCC_TPCC_SECR_SECR20=1; TPCC_TPCC_SECR_SECR21=1;TPCC_TPCC_SECR_SECR22=1;TPCC_TPCC_SECR_SECR23=1; TPCC_TPCC_SECR_SECR24=1;TPCC_TPCC_SECR_SECR25=1;TPCC_TPCC_SECR_SECR26=1; TPCC_TPCC_SECR_SECR27=1;TPCC_TPCC_SECR_SECR28=1;TPCC_TPCC_SECR_SECR29=1; TPCC_TPCC_SECR_SECR30=1;TPCC_TPCC_SECR_SECR31=1;
TPCC_TPCC_SECRH_SECR32=1;TPCC_TPCC_SECRH_SECR33=1;TPCC_TPCC_SECRH_SECR34=1; TPCC_TPCC_SECRH_SECR35=1;TPCC_TPCC_SECRH_SECR36=1;TPCC_TPCC_SECRH_SECR37=1; TPCC_TPCC_SECRH_SECR38=1;TPCC_TPCC_SECRH_SECR39=1;TPCC_TPCC_SECRH_SECR40=1; TPCC_TPCC_SECRH_SECR41=1;TPCC_TPCC_SECRH_SECR42=1;TPCC_TPCC_SECRH_SECR43=1; TPCC_TPCC_SECRH_SECR44=1;TPCC_TPCC_SECRH_SECR45=1;TPCC_TPCC_SECRH_SECR46=1; TPCC_TPCC_SECRH_SECR47=1;TPCC_TPCC_SECRH_SECR48=1;TPCC_TPCC_SECRH_SECR49=1; TPCC_TPCC_SECRH_SECR50=1;TPCC_TPCC_SECRH_SECR51=1;TPCC_TPCC_SECRH_SECR52=1; TPCC_TPCC_SECRH_SECR53=1;TPCC_TPCC_SECRH_SECR54=1;TPCC_TPCC_SECRH_SECR55=1; TPCC_TPCC_SECRH_SECR56=1;TPCC_TPCC_SECRH_SECR57=1;TPCC_TPCC_SECRH_SECR58=1; TPCC_TPCC_SECRH_SECR59=1;TPCC_TPCC_SECRH_SECR60=1;TPCC_TPCC_SECRH_SECR61=1; TPCC_TPCC_SECRH_SECR62=1;TPCC_TPCC_SECRH_SECR63=1;

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                Uint32                  qdmaSecEvent;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Clear the DMA Secondary Event for DMA channel 1
                CSL_edma3ClearDMAChannelSecondaryEvents(hModule, 1);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3ClearDMAMissedEvent | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | dmaChannel |
| ) |  |  |

============================================================================
CSL_edma3ClearDMAMissedEvent

Description
The API clears the missed event for the specific DMA Channel.

Arguments

            hModule         Module Handle
            dmaChannel      DMA Channel for which the event is cleared.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
Clears all the missed events

Writes
TPCC_TPCC_EMCR_EMCR0;TPCC_TPCC_EMCR_EMCR1;TPCC_TPCC_EMCR_EMCR2; TPCC_TPCC_EMCR_EMCR3;TPCC_TPCC_EMCR_EMCR4;TPCC_TPCC_EMCR_EMCR5; TPCC_TPCC_EMCR_EMCR6;TPCC_TPCC_EMCR_EMCR7;TPCC_TPCC_EMCR_EMCR8; TPCC_TPCC_EMCR_EMCR9;TPCC_TPCC_EMCR_EMCR10;TPCC_TPCC_EMCR_EMCR11; TPCC_TPCC_EMCR_EMCR12;TPCC_TPCC_EMCR_EMCR13;TPCC_TPCC_EMCR_EMCR14; TPCC_TPCC_EMCR_EMCR15;TPCC_TPCC_EMCR_EMCR16;TPCC_TPCC_EMCR_EMCR17; TPCC_TPCC_EMCR_EMCR18;TPCC_TPCC_EMCR_EMCR19;TPCC_TPCC_EMCR_EMCR20; TPCC_TPCC_EMCR_EMCR21;TPCC_TPCC_EMCR_EMCR22;TPCC_TPCC_EMCR_EMCR23; TPCC_TPCC_EMCR_EMCR24;TPCC_TPCC_EMCR_EMCR25;TPCC_TPCC_EMCR_EMCR26; TPCC_TPCC_EMCR_EMCR27;TPCC_TPCC_EMCR_EMCR28;TPCC_TPCC_EMCR_EMCR29; TPCC_TPCC_EMCR_EMCR30;TPCC_TPCC_EMCR_EMCR31; TPCC_TPCC_EMCRH_EMCR32;TPCC_TPCC_EMCRH_EMCR33;TPCC_TPCC_EMCRH_EMCR34 TPCC_TPCC_EMCRH_EMCR35;TPCC_TPCC_EMCRH_EMCR36;TPCC_TPCC_EMCRH_EMCR37 TPCC_TPCC_EMCRH_EMCR38;TPCC_TPCC_EMCRH_EMCR39;TPCC_TPCC_EMCRH_EMCR40 TPCC_TPCC_EMCRH_EMCR41;TPCC_TPCC_EMCRH_EMCR42;TPCC_TPCC_EMCRH_EMCR43 TPCC_TPCC_EMCRH_EMCR44;TPCC_TPCC_EMCRH_EMCR45;TPCC_TPCC_EMCRH_EMCR46 TPCC_TPCC_EMCRH_EMCR47;TPCC_TPCC_EMCRH_EMCR48;TPCC_TPCC_EMCRH_EMCR49 TPCC_TPCC_EMCRH_EMCR50;TPCC_TPCC_EMCRH_EMCR51;TPCC_TPCC_EMCRH_EMCR52 TPCC_TPCC_EMCRH_EMCR53;TPCC_TPCC_EMCRH_EMCR54;TPCC_TPCC_EMCRH_EMCR55 TPCC_TPCC_EMCRH_EMCR56;TPCC_TPCC_EMCRH_EMCR57;TPCC_TPCC_EMCRH_EMCR58 TPCC_TPCC_EMCRH_EMCR59;TPCC_TPCC_EMCRH_EMCR60;TPCC_TPCC_EMCRH_EMCR61 TPCC_TPCC_EMCRH_EMCR62;TPCC_TPCC_EMCRH_EMCR63;

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                CSL_BitMask32           missedLo, missedHi, missedQdma;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Clear missed DMA 1 channel event.
                CSL_edma3ClearDMAMissedEvent(hModule, 1);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3ClearDMASecondaryEvents | ( | CSL_Edma3Handle | hModule,
|  | CSL_BitMask32 | secEventLo,
|  | CSL_BitMask32 | secEventHi |
| ) |  |  |

============================================================================
CSL_edma3ClearDMASecondaryEvents

Description
This API clears the DMA secondary events

Arguments

            hModule         Module Handle
            secEventLo      Lower order 32 bits of secondary events to be cleared
            secEventHi      Higher order 32 bits of secondary events to be cleared

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_SECR,TPCC_TPCC_SECRH

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                CSL_BitMask32           secEventLo;
                CSL_BitMask32           secEventHi;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Get the DMA Secondary Events.
                CSL_edma3GetDMASecondaryEvents(hModule, &secEventLo, &secEventHi);
                ...
                // Clear the DMA Secondary Events
                CSL_edma3ClearDMASecondaryEvents(hModule, secEventLo, secEventHi);

===========================================================================

CSL_IDEF_INLINE void CSL_edma3ClearHiPendingInterrupts | ( | CSL_Edma3Handle | hModule,
|  | Int | region,
|  | CSL_BitMask32 | intrHi |
| ) |  |  |

============================================================================
CSL_edma3ClearHiPendingInterrupts

Description
This API clears the High pending interrupts using the interrupt bitmasks provided

Arguments

            hModule           Module Handle
            region            Region (Shadown Region or Global)
            intrHi            Interrupt 32-63 (BitMask32) to be cleared

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_ICRH

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                CSL_BitMask32           edmaIntrHi;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Get all the pending interrupts for the global region.
                CSL_edma3GetHiPendingInterrupts(hModule, CSL_EDMA3_REGION_GLOBAL, &edmaIntrHi);
                ...
                // Clear the pending interrupts for the global region.
                CSL_edma3ClearHiPendingInterrupts(hModule, CSL_EDMA3_REGION_GLOBAL, edmaIntrHi);

===========================================================================

CSL_IDEF_INLINE void CSL_edma3ClearLoPendingInterrupts | ( | CSL_Edma3Handle | hModule,
|  | Int | region,
|  | CSL_BitMask32 | intrLo |
| ) |  |  |

============================================================================
CSL_edma3ClearLoPendingInterrupts

Description
This API clears the low pending interrupts using the interrupt bitmasks provided

Arguments

            hModule           Module Handle
            region            Region (Shadown Region or Global)
            intrLo            Interrupt 0-31 (BitMask32) to be cleared

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_ICR

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                CSL_BitMask32           edmaIntrLo;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Get all the pending interrupts for the global region.
                CSL_edma3GetLoPendingInterrupts(hModule, CSL_EDMA3_REGION_GLOBAL, &edmaIntrLo);
                ...
                // Clear the pending interrupts for the global region.
                CSL_edma3ClearLoPendingInterrupts(hModule, CSL_EDMA3_REGION_GLOBAL, edmaIntrLo);

===========================================================================

CSL_IDEF_INLINE void CSL_edma3ClearQDMAChannelSecondaryEvents | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | qdmaChannel |
| ) |  |  |

============================================================================
CSL_edma3ClearQDMAChannelSecondaryEvents

Description
This API clears the QDMA Secondary Event for a specific QDMA Channel.

Arguments

            hModule         Module Handle
            qdmaChannel     QDMA Channel for which the secondary event is to be cleared.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_QSECR_QSECR0=1;TPCC_TPCC_QSECR_QSECR1=1;TPCC_TPCC_QSECR_QSECR2=1; TPCC_TPCC_QSECR_QSECR3=1;TPCC_TPCC_QSECR_QSECR4=1;TPCC_TPCC_QSECR_QSECR5=1; TPCC_TPCC_QSECR_QSECR6=1;TPCC_TPCC_QSECR_QSECR7=1;

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                Uint32                  qdmaSecEvent;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Clear the QDMA Secondary Event for QDMA channel 1
                CSL_edma3ClearQDMAChannelSecondaryEvents(hModule, 1);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3ClearQDMAMissedEvent | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | qdmaChannel |
| ) |  |  |

============================================================================
CSL_edma3ClearQDMAMissedEvent

Description
The API clears the missed event for the specific QDMA Channel.

Arguments

            hModule         Module Handle
            qdmaChannel     QDMA Channel for which the event is cleared.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
Clears all the missed events

Writes
TPCC_TPCC_QEMCR_QEMCR0;TPCC_TPCC_QEMCR_QEMCR1;TPCC_TPCC_QEMCR_QEMCR2; TPCC_TPCC_QEMCR_QEMCR3;TPCC_TPCC_QEMCR_QEMCR4;TPCC_TPCC_QEMCR_QEMCR5; TPCC_TPCC_QEMCR_QEMCR6;TPCC_TPCC_QEMCR_QEMCR7

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                CSL_BitMask32           missedLo, missedHi, missedQdma;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Clear missed QDMA Channel 1 event.
                CSL_edma3ClearQDMAMissedEvent(hModule, 1);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3ClearQDMASecondaryEvents | ( | CSL_Edma3Handle | hModule,
|  | Uint32 | qdmaSecEvent |
| ) |  |  |

============================================================================
CSL_edma3ClearQDMASecondaryEvents

Description
This API clears the QDMA Secondary Event.

Arguments

            hModule         Module Handle
            qdmaSecEvent    QDMA Secondary Event to be cleared.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_QSECR

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                Uint32                  qdmaSecEvent;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Get the QDMA Secondary Event
                CSL_edma3GetQDMASecondaryEvents(hModule, &qdmaSecEvent);
                ...
                // Clear the QDMA Secondary Event
                CSL_edma3ClearQDMASecondaryEvents(hModule, qdmaSecEvent);
                ...

===========================================================================

CSL_Status CSL_edma3Close | ( | CSL_Edma3Handle | hEdma | ) |

============================================================================
CSL_edma3Close.c

Description
This is a module level close require to invalidate the module handle. The module handle must not be used after this API call.

Arguments

                hEdma           Handle to the Edma Instance

Return Value
Success - CSL_SOK
Error - CSL_ESYS_BADHANDLE (The handle passed is invalid)

Pre Condition
Functions CSL_edma3Init() and CSL_edma3Open() have to be called in that order successfully before calling this function.

Post Condition
The edma CSL APIs can not be called until the edma CSL is reopened again using CSL_edma3Open()

Example

                CSL_Edma3Handle     hModule;
                CSL_Edma3Obj        edmaObj;
                CSL_Status          status;

                // Module Initialization
                CSL_edma3Init(NULL);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, CSL_EDMA3, NULL, &status);
                ...
                // Close the Module.
                CSL_edma3Close(hModule);
                ...

=============================================================================

CSL_IDEF_INLINE void CSL_edma3DMAChannelDisable | ( | CSL_Edma3Handle | hModule,
|  | Int | region,
|  | Uint8 | dmaChannel |
| ) |  |  |

============================================================================
CSL_edma3DMAChannelDisable

Description
This API disables the specified DMA Channel.

Arguments

            hModule         Module Handle
            region          Region (Shadow or Global)
            dmaChannel      DMA Channel to be disabled.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_EECR_E0=1;TPCC_TPCC_EECR_E1=1;TPCC_TPCC_EECR_E2=1; TPCC_TPCC_EECR_E3=1;TPCC_TPCC_EECR_E4=1;TPCC_TPCC_EECR_E5=1; TPCC_TPCC_EECR_E6=1;TPCC_TPCC_EECR_E7=1;TPCC_TPCC_EECR_E8=1; TPCC_TPCC_EECR_E9=1;TPCC_TPCC_EECR_E10=1;TPCC_TPCC_EECR_E11=1; TPCC_TPCC_EECR_E12=1;TPCC_TPCC_EECR_E13=1;TPCC_TPCC_EECR_E14=1; TPCC_TPCC_EECR_E15=1;TPCC_TPCC_EECR_E16=1;TPCC_TPCC_EECR_E17=1; TPCC_TPCC_EECR_E18=1;TPCC_TPCC_EECR_E19=1;TPCC_TPCC_EECR_E20=1; TPCC_TPCC_EECR_E21=1;TPCC_TPCC_EECR_E22=1;TPCC_TPCC_EECR_E23=1; TPCC_TPCC_EECR_E24=1;TPCC_TPCC_EECR_E25=1;TPCC_TPCC_EECR_E26=1; TPCC_TPCC_EECR_E27=1;TPCC_TPCC_EECR_E28=1;TPCC_TPCC_EECR_E29=1; TPCC_TPCC_EECR_E30=1;TPCC_TPCC_EECR_E31=1;
TPCC_TPCC_EECRH_E32=1;TPCC_TPCC_EECRH_E33=1;TPCC_TPCC_EECRH_E34=1; TPCC_TPCC_EECRH_E35=1;TPCC_TPCC_EECRH_E36=1;TPCC_TPCC_EECRH_E37=1; TPCC_TPCC_EECRH_E38=1;TPCC_TPCC_EECRH_E39=1;TPCC_TPCC_EECRH_E40=1; TPCC_TPCC_EECRH_E41=1;TPCC_TPCC_EECRH_E42=1;TPCC_TPCC_EECRH_E43=1; TPCC_TPCC_EECRH_E44=1;TPCC_TPCC_EECRH_E45=1;TPCC_TPCC_EECRH_E46=1; TPCC_TPCC_EECRH_E47=1;TPCC_TPCC_EECRH_E48=1;TPCC_TPCC_EECRH_E49=1; TPCC_TPCC_EECRH_E50=1;TPCC_TPCC_EECRH_E51=1;TPCC_TPCC_EECRH_E52=1; TPCC_TPCC_EECRH_E53=1;TPCC_TPCC_EECRH_E54=1;TPCC_TPCC_EECRH_E55=1; TPCC_TPCC_EECRH_E56=1;TPCC_TPCC_EECRH_E57=1;TPCC_TPCC_EECRH_E58=1; TPCC_TPCC_EECRH_E59=1;TPCC_TPCC_EECRH_E60=1;TPCC_TPCC_EECRH_E61=1; TPCC_TPCC_EECRH_E62=1;TPCC_TPCC_EECRH_E63=1;

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Disables DMA Channel 0
                CSL_edma3DMAChannelDisable(hModule, 0);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3DMAChannelEnable | ( | CSL_Edma3Handle | hModule,
|  | Int | region,
|  | Uint8 | dmaChannel |
| ) |  |  |

============================================================================
CSL_edma3DMAChannelEnable

Description
This API enables the specified DMA Channel.

Arguments

            hModule         Module Handle
            region          Region (Shadow or Global)
            dmaChannel      DMA Channel to be enabled.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_EESR_E0=1;TPCC_TPCC_EESR_E1=1;TPCC_TPCC_EESR_E2=1; TPCC_TPCC_EESR_E3=1;TPCC_TPCC_EESR_E4=1;TPCC_TPCC_EESR_E5=1; TPCC_TPCC_EESR_E6=1;TPCC_TPCC_EESR_E7=1;TPCC_TPCC_EESR_E8=1; TPCC_TPCC_EESR_E9=1;TPCC_TPCC_EESR_E10=1;TPCC_TPCC_EESR_E11=1; TPCC_TPCC_EESR_E12=1;TPCC_TPCC_EESR_E13=1;TPCC_TPCC_EESR_E14=1; TPCC_TPCC_EESR_E15=1;TPCC_TPCC_EESR_E16=1;TPCC_TPCC_EESR_E17=1; TPCC_TPCC_EESR_E18=1;TPCC_TPCC_EESR_E19=1;TPCC_TPCC_EESR_E20=1; TPCC_TPCC_EESR_E21=1;TPCC_TPCC_EESR_E22=1;TPCC_TPCC_EESR_E23=1; TPCC_TPCC_EESR_E24=1;TPCC_TPCC_EESR_E25=1;TPCC_TPCC_EESR_E26=1; TPCC_TPCC_EESR_E27=1;TPCC_TPCC_EESR_E28=1;TPCC_TPCC_EESR_E29=1; TPCC_TPCC_EESR_E30=1;TPCC_TPCC_EESR_E31=1;
TPCC_TPCC_EESRH_E32=1;TPCC_TPCC_EESRH_E33=1;TPCC_TPCC_EESRH_E34=1; TPCC_TPCC_EESRH_E35=1;TPCC_TPCC_EESRH_E36=1;TPCC_TPCC_EESRH_E37=1; TPCC_TPCC_EESRH_E38=1;TPCC_TPCC_EESRH_E39=1;TPCC_TPCC_EESRH_E40=1; TPCC_TPCC_EESRH_E41=1;TPCC_TPCC_EESRH_E42=1;TPCC_TPCC_EESRH_E43=1; TPCC_TPCC_EESRH_E44=1;TPCC_TPCC_EESRH_E45=1;TPCC_TPCC_EESRH_E46=1; TPCC_TPCC_EESRH_E47=1;TPCC_TPCC_EESRH_E48=1;TPCC_TPCC_EESRH_E49=1; TPCC_TPCC_EESRH_E50=1;TPCC_TPCC_EESRH_E51=1;TPCC_TPCC_EESRH_E52=1; TPCC_TPCC_EESRH_E53=1;TPCC_TPCC_EESRH_E54=1;TPCC_TPCC_EESRH_E55=1; TPCC_TPCC_EESRH_E56=1;TPCC_TPCC_EESRH_E57=1;TPCC_TPCC_EESRH_E58=1; TPCC_TPCC_EESRH_E59=1;TPCC_TPCC_EESRH_E60=1;TPCC_TPCC_EESRH_E61=1; TPCC_TPCC_EESRH_E62=1;TPCC_TPCC_EESRH_E63=1;

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Enables DMA Channel 0 for the global region.
                CSL_edma3DMAChannelEnable(hModule, CSL_EDMA3_REGION_GLOBAL, 0);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3DmaRegionAccessDisable | ( | CSL_Edma3Handle | hModule,
|  | Int | edmaRegion,
|  | CSL_BitMask32 | drae,
|  | CSL_BitMask32 | draeh |
| ) |  |  |

============================================================================
CSL_edma3DmaRegionAccessDisable

Description
This API disables read/write access to the shadow regions for the specific DMA channels.

Arguments

            hModule           Module Handle
            edmaRegion        Shadow Region
            access            Region bits to be programmed
            drae              Bitmask to be disabled in DRAE
            draeh             Bitmask to be disabled in DRAEH

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_DRA_DRAE_E0=0;TPCC_TPCC_DRA_DRAE_E1=0;TPCC_TPCC_DRA_DRAE_E2=0; TPCC_TPCC_DRA_DRAE_E3=0;TPCC_TPCC_DRA_DRAE_E4=0;TPCC_TPCC_DRA_DRAE_E5=0; TPCC_TPCC_DRA_DRAE_E6=0;TPCC_TPCC_DRA_DRAE_E7=0;TPCC_TPCC_DRA_DRAE_E8=0; TPCC_TPCC_DRA_DRAE_E9=0;TPCC_TPCC_DRA_DRAE_E10=0;TPCC_TPCC_DRA_DRAE_E11=0; TPCC_TPCC_DRA_DRAE_E12=0;TPCC_TPCC_DRA_DRAE_E13=0;TPCC_TPCC_DRA_DRAE_E14=0; TPCC_TPCC_DRA_DRAE_E15=0;TPCC_TPCC_DRA_DRAE_E16=0;TPCC_TPCC_DRA_DRAE_E17=0; TPCC_TPCC_DRA_DRAE_E18=0;TPCC_TPCC_DRA_DRAE_E19=0;TPCC_TPCC_DRA_DRAE_E20=0; TPCC_TPCC_DRA_DRAE_E21=0;TPCC_TPCC_DRA_DRAE_E22=0;TPCC_TPCC_DRA_DRAE_E23=0; TPCC_TPCC_DRA_DRAE_E24=0;TPCC_TPCC_DRA_DRAE_E25=0;TPCC_TPCC_DRA_DRAE_E26=0; TPCC_TPCC_DRA_DRAE_E27=0;TPCC_TPCC_DRA_DRAE_E28=0;TPCC_TPCC_DRA_DRAE_E29=0; TPCC_TPCC_DRA_DRAE_E30=0;TPCC_TPCC_DRA_DRAE_E31=0;
TPCC_TPCC_DRA_DRAEH_E32=0;TPCC_TPCC_DRA_DRAEH_E33=0;TPCC_TPCC_DRA_DRAEH_E34=0; TPCC_TPCC_DRA_DRAEH_E35=0;TPCC_TPCC_DRA_DRAEH_E36=0;TPCC_TPCC_DRA_DRAEH_E37=0; TPCC_TPCC_DRA_DRAEH_E38=0;TPCC_TPCC_DRA_DRAEH_E39=0;TPCC_TPCC_DRA_DRAEH_E40=0; TPCC_TPCC_DRA_DRAEH_E41=0;TPCC_TPCC_DRA_DRAEH_E42=0;TPCC_TPCC_DRA_DRAEH_E43=0; TPCC_TPCC_DRA_DRAEH_E44=0;TPCC_TPCC_DRA_DRAEH_E45=0;TPCC_TPCC_DRA_DRAEH_E46=0; TPCC_TPCC_DRA_DRAEH_E47=0;TPCC_TPCC_DRA_DRAEH_E48=0;TPCC_TPCC_DRA_DRAEH_E49=0; TPCC_TPCC_DRA_DRAEH_E50=0;TPCC_TPCC_DRA_DRAEH_E51=0;TPCC_TPCC_DRA_DRAEH_E52=0; TPCC_TPCC_DRA_DRAEH_E53=0;TPCC_TPCC_DRA_DRAEH_E54=0;TPCC_TPCC_DRA_DRAEH_E55=0; TPCC_TPCC_DRA_DRAEH_E56=0;TPCC_TPCC_DRA_DRAEH_E57=0;TPCC_TPCC_DRA_DRAEH_E58=0; TPCC_TPCC_DRA_DRAEH_E59=0;TPCC_TPCC_DRA_DRAEH_E60=0;TPCC_TPCC_DRA_DRAEH_E61=0; TPCC_TPCC_DRA_DRAEH_E62=0;TPCC_TPCC_DRA_DRAEH_E63=0;

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Disable read/write access in Region 0 for DMA Channel 0 to 7
                CSL_edma3DmaRegionAccessDisable(hModule, 0, 0x000000FF, 0x0);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3DmaRegionAccessEnable | ( | CSL_Edma3Handle | hModule,
|  | Int | edmaRegion,
|  | CSL_BitMask32 | drae,
|  | CSL_BitMask32 | draeh |
| ) |  |  |

============================================================================
CSL_edma3DmaRegionAccessEnable

Description
This API enables read/write access to the shadow regions for the specific DMA channels.

Arguments

            hModule           Module Handle
            edmaRegion        Shadow Region
            access            Region bits to be programmed
            drae              Bitmask to be enabled in DRAE
            draeh             Bitmask to be enabled in DRAEH

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_DRA_DRAE_E0=1;TPCC_TPCC_DRA_DRAE_E1=1;TPCC_TPCC_DRA_DRAE_E2=1; TPCC_TPCC_DRA_DRAE_E3=1;TPCC_TPCC_DRA_DRAE_E4=1;TPCC_TPCC_DRA_DRAE_E5=1; TPCC_TPCC_DRA_DRAE_E6=1;TPCC_TPCC_DRA_DRAE_E7=1;TPCC_TPCC_DRA_DRAE_E8=1; TPCC_TPCC_DRA_DRAE_E9=1;TPCC_TPCC_DRA_DRAE_E10=1;TPCC_TPCC_DRA_DRAE_E11=1; TPCC_TPCC_DRA_DRAE_E12=1;TPCC_TPCC_DRA_DRAE_E13=1;TPCC_TPCC_DRA_DRAE_E14=1; TPCC_TPCC_DRA_DRAE_E15=1;TPCC_TPCC_DRA_DRAE_E16=1;TPCC_TPCC_DRA_DRAE_E17=1; TPCC_TPCC_DRA_DRAE_E18=1;TPCC_TPCC_DRA_DRAE_E19=1;TPCC_TPCC_DRA_DRAE_E20=1; TPCC_TPCC_DRA_DRAE_E21=1;TPCC_TPCC_DRA_DRAE_E22=1;TPCC_TPCC_DRA_DRAE_E23=1; TPCC_TPCC_DRA_DRAE_E24=1;TPCC_TPCC_DRA_DRAE_E25=1;TPCC_TPCC_DRA_DRAE_E26=1; TPCC_TPCC_DRA_DRAE_E27=1;TPCC_TPCC_DRA_DRAE_E28=1;TPCC_TPCC_DRA_DRAE_E29=1; TPCC_TPCC_DRA_DRAE_E30=1;TPCC_TPCC_DRA_DRAE_E31=1;
TPCC_TPCC_DRA_DRAEH_E32=1;TPCC_TPCC_DRA_DRAEH_E33=1;TPCC_TPCC_DRA_DRAEH_E34=1; TPCC_TPCC_DRA_DRAEH_E35=1;TPCC_TPCC_DRA_DRAEH_E36=1;TPCC_TPCC_DRA_DRAEH_E37=1; TPCC_TPCC_DRA_DRAEH_E38=1;TPCC_TPCC_DRA_DRAEH_E39=1;TPCC_TPCC_DRA_DRAEH_E40=1; TPCC_TPCC_DRA_DRAEH_E41=1;TPCC_TPCC_DRA_DRAEH_E42=1;TPCC_TPCC_DRA_DRAEH_E43=1; TPCC_TPCC_DRA_DRAEH_E44=1;TPCC_TPCC_DRA_DRAEH_E45=1;TPCC_TPCC_DRA_DRAEH_E46=1; TPCC_TPCC_DRA_DRAEH_E47=1;TPCC_TPCC_DRA_DRAEH_E48=1;TPCC_TPCC_DRA_DRAEH_E49=1; TPCC_TPCC_DRA_DRAEH_E50=1;TPCC_TPCC_DRA_DRAEH_E51=1;TPCC_TPCC_DRA_DRAEH_E52=1; TPCC_TPCC_DRA_DRAEH_E53=1;TPCC_TPCC_DRA_DRAEH_E54=1;TPCC_TPCC_DRA_DRAEH_E55=1; TPCC_TPCC_DRA_DRAEH_E56=1;TPCC_TPCC_DRA_DRAEH_E57=1;TPCC_TPCC_DRA_DRAEH_E58=1; TPCC_TPCC_DRA_DRAEH_E59=1;TPCC_TPCC_DRA_DRAEH_E60=1;TPCC_TPCC_DRA_DRAEH_E61=1; TPCC_TPCC_DRA_DRAEH_E62=1;TPCC_TPCC_DRA_DRAEH_E63=1;

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Enable read/write access in Region 0 for DMA Channel 0 to 7
                CSL_edma3DmaRegionAccessEnable(hModule, 0, 0x000000FF, 0x0);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3ErrorEval | ( | CSL_Edma3Handle | hModule | ) |

============================================================================
CSL_edma3ErrorEval

Description
This API enables enables evaluation of errros for the specified view/shadow region.Sets EVAL bit of the EEVAL register in the Global register space

Arguments

            hModule           Module Handle

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_EEVAL_EVAL=1

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Set the Error Interrupt Evaluation
                CSL_edma3ErrorEval(hModule);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3EventQueueThresholdSet | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | eventQueue,
|  | Uint8 | threshold |
| ) |  |  |

============================================================================
CSL_edma3EventQueueThresholdSet

Description
The function configures the queue threshold.

Arguments

            hModule           Module Handle
            eventQueue        Event queue for which the threshold is configured
            threshold         Target threshold value.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_QWMTHRA_Q0;TPCC_TPCC_QWMTHRA_Q1;TPCC_TPCC_QWMTHRA_Q2; TPCC_TPCC_QWMTHRA_Q3;
TPCC_TPCC_QWMTHRB_Q4;TPCC_TPCC_QWMTHRB_Q1;TPCC_TPCC_QWMTHRB_Q2; TPCC_TPCC_QWMTHRB_Q3

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Set the Queue threshold for Event Queue 0 to be 9
                CSL_edma3EventQueueThresholdSet(hModule, 0, 9);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3EventsMissedClear | ( | CSL_Edma3Handle | hModule,
|  | CSL_BitMask32 | missedLo,
|  | CSL_BitMask32 | missedHi,
|  | CSL_BitMask32 | missedQdma |
| ) |  |  |

============================================================================
CSL_edma3EventMissedClear

Description
Clear the Event missed errors

Arguments

            hModule           Module Handle
            missedLo          Lower 32 of of the Event Missed register needing to
                              be cleared (This is the same value as EMR)
            missedHi          Upper 32 of of the Event Missed register needing to
                              be cleared (This is the same value as EMRH)
            missedQdma        Bit mask of Qdma events missed needing to be cleared

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
Clears all the missed events

Writes
TPCC_TPCC_EMCR,TPCC_TPCC_EMCRH,TPCC_TPCC_QEMCR

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                CSL_BitMask32           missedLo, missedHi, missedQdma;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Get the missed events
                CSL_edma3GetEventMissed(hModule, &missedEdma, &missedEdmaHi, &missedQdma);
                ...
                // Clear the error
                CSL_edma3EventMissedClear(hModule,missedLo, missedHi,qdmamissed);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3GetActivityStatus | ( | CSL_Edma3Handle | hModule,
|  | CSL_Edma3ActivityStat * | activityStat |
| ) |  |  |

============================================================================
CSL_edma3GetActivityStatus

Description
Obtains the Channel Controller Activity Status

Arguments

            hModule           Module Handle
            activityStat      Activity Status populated by this API.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_CCSTAT_EVTACTV,TPCC_TPCC_CCSTAT_QEVTACTV,TPCC_TPCC_CCSTAT_TRACTV, TPCC_TPCC_CCSTAT_ACTV,TPCC_TPCC_CCSTAT_COMP_ACTV

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                CSL_Edma3ActivityStat   activityStat;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Get the CC activity status.
                CSL_edma3GetActivityStatus(hModule,&activityStat);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3GetControllerError | ( | CSL_Edma3Handle | hModule,
|  | CSL_Edma3CtrlErrStat * | ccStat |
| ) |  |  |

============================================================================
CSL_edma3GetControllerError

Description
The function gets the status of the controller error.

Arguments

            hModule     Module Handle
            ccStat      Controller Error populated by this API

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_CCERR_QTHRXD0;TPCC_TPCC_CCERR_QTHRXD1;TPCC_TPCC_CCERR_QTHRXD2; TPCC_TPCC_CCERR_QTHRXD3;TPCC_TPCC_CCERR_QTHRXD4;TPCC_TPCC_CCERR_QTHRXD5; TPCC_TPCC_CCERR_QTHRXD6;TPCC_TPCC_CCERR_QTHRXD7, TPCC_TPCC_CCERR_TCCERR

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                CSL_Edma3CtrlErrStat    ccError;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Get Controller Error
                status = CSL_edma3GetControllerError(hModule,&ccError);
                ...

===========================================================================

CSL_IDEF_INLINE Uint8 CSL_edma3GetDMAChannelToEventQueueMapping | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | dmaChannel |
| ) |  |  |

============================================================================
CSL_edma3GetDMAChannelToEventQueueMapping

Description
The function gets the mapping of the DMA Channel to the Event Queue

Arguments

            hModule     Module Handle
            dmaChannel  DMA Channel for which the mapping is to be retreived.

Return Value
Event Queue to which the DMA channel is mapped to

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_DMAQNUM_E0;TPCC_TPCC_DMAQNUM_E1;TPCC_TPCC_DMAQNUM_E2; TPCC_TPCC_DMAQNUM_E3;TPCC_TPCC_DMAQNUM_E4;TPCC_TPCC_DMAQNUM_E5; TPCC_TPCC_DMAQNUM_E6;TPCC_TPCC_DMAQNUM_E7

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                Uint8                   eventQueue;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, CSL_EDMA3, NULL, &status);

                // Get the Event Queue mapping of DMA Channel 1
                eventQueue = CSL_edma3GetDMAChannelToEventQueueMapping(hModule, 1);
                ...

===========================================================================

CSL_IDEF_INLINE Uint16 CSL_edma3GetDMAChannelToParamBlockMapping | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | dmaChannel |
| ) |  |  |

============================================================================
CSL_edma3GetDMAChannelToParamBlockMapping

Description
The function gets the PARAM Entry ID to which a specific DMA Channel is mapped.

Arguments

            hModule     Module Handle
            dmaChannel  DMA Channel Number whose mapping is to be found.

Return Value
Paramater ID to which the specific DMA Channel is mapped to.

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_DCHMAP_PAENTRY

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                Uint16                  paramId;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, CSL_EDMA3, NULL, &status);

                // Get the mapping information for DMA channel 1.
                paramId = CSL_edma3GetDMAChannelToParamBlockMapping(hModule, 1);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3GetDMASecondaryEvents | ( | CSL_Edma3Handle | hModule,
|  | CSL_BitMask32 * | secEventLo,
|  | CSL_BitMask32 * | secEventHi |
| ) |  |  |

============================================================================
CSL_edma3GetDMASecondaryEvents

Description
This API gets the DMA secondary events

Arguments

            hModule         Module Handle
            secEventLo      Lower order 32 bits of secondary events populated by the API
            secEventHi      Higher order 32 bits of secondary events populated by the API

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_SER,TPCC_TPCC_SERH

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                CSL_BitMask32           secEventLo;
                CSL_BitMask32           secEventHi;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Get the DMA Secondary Events.
                CSL_edma3GetDMASecondaryEvents(hModule, &secEventLo, &secEventHi);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3GetEventMissed | ( | CSL_Edma3Handle | hModule,
|  | CSL_BitMask32 * | missedLo,
|  | CSL_BitMask32 * | missedHi,
|  | CSL_BitMask32 * | missedQdma |
| ) |  |  |

============================================================================
CSL_edma3GetEventMissed

Description
Queries all the events missed.Since there may be upto 64 EDMA channels + upto 8 QDMA channels,this points to an array of 3, 32 bit elements.Gets the status of the missed events.

Arguments

            hModule           Module Handle
            missedLo          missed [0] - holds status from EMR
            missedHi          missed [1] - holds status from EMRH
            missedQdma        missed [2] - holds status from QEMR

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_EMR,TPCC_TPCC_EMRH,TPCC_TPCC_QEMR

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                CSL_BitMask32           missedLo, missedHi, missedQdma;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Get the missed events
                CSL_edma3GetEventMissed(hModule, &missedEdma, &missedEdmaHi, &missedQdma);
                ...

===========================================================================

CSL_IDEF_INLINE Uint8 CSL_edma3GetEventQueuePriority | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | eventQueue |
| ) |  |  |

============================================================================
CSL_edma3GetEventQueuePriority

Description
The function gets the priority of the specific event queue.

Arguments

            hModule     Module Handle
            eventQueue  Event Queue whose priority is to be retrieved.

Return Value
Priority to which the Event Queue is mapped to.

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
Event Queue is configured to the specific priority.

Reads
TPCC_TPCC_QUEPRI_PRIQ0;TPCC_TPCC_QUEPRI_PRIQ1;TPCC_TPCC_QUEPRI_PRIQ2; TPCC_TPCC_QUEPRI_PRIQ3;TPCC_TPCC_QUEPRI_PRIQ4;TPCC_TPCC_QUEPRI_PRIQ5; TPCC_TPCC_QUEPRI_PRIQ6;TPCC_TPCC_QUEPRI_PRIQ7

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                Uint8                   priority;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, CSL_EDMA3, NULL, &status);

                // Get the priority of Event Queue 2.
                priority = CSL_edma3GetEventQueuePriority(hModule, 2);
                ...

===========================================================================

CSL_IDEF_INLINE Uint8 CSL_edma3GetEventQueueToTCMapping | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | eventQueue |
| ) |  |  |

============================================================================
CSL_edma3GetEventQueueToTCMapping

Description
The function gets the TC mapping for the specific event queue.

Arguments

            hModule     Module Handle
            eventQueue  Event Queue which for which the mapping is needed.

Return Value
TC Number to which the event queue is mapped to

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
Event Queue is mapped to the specific TC

Reads
TPCC_TPCC_QUETCMAP_TCNUMQ0;TPCC_TPCC_QUETCMAP_TCNUMQ1;TPCC_TPCC_QUETCMAP_TCNUMQ2; TPCC_TPCC_QUETCMAP_TCNUMQ3;TPCC_TPCC_QUETCMAP_TCNUMQ4;TPCC_TPCC_QUETCMAP_TCNUMQ5; TPCC_TPCC_QUETCMAP_TCNUMQ6;TPCC_TPCC_QUETCMAP_TCNUMQ7

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                Uint8                   tcNum;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, CSL_EDMA3, NULL, &status);

                // Get the TC mapping for Event Queue 1
                tcNum = CSL_edma3GetEventQueueToTCMapping(hModule, 1, 0);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3GetHiPendingInterrupts | ( | CSL_Edma3Handle | hModule,
|  | Int | region,
|  | CSL_BitMask32 * | intrHi |
| ) |  |  |

============================================================================
CSL_edma3GetHiPendingInterrupts

Description
The API gets a bitmask of all high pending interrupts.

Arguments

            hModule           Module Handle
            region            Region (Shadown Region or Global)
            intrHi            Status 32-63 of the interrupts

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_IPRH

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                CSL_BitMask32           edmaIntrHi;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Get all the high pending interrupts for the global region.
                CSL_edma3GetHiPendingInterrupts(hModule, CSL_EDMA3_REGION_GLOBAL, &edmaIntrHi);
                ...

===========================================================================

CSL_Status CSL_edma3GetHwChannelSetupParam | ( | CSL_Edma3ChannelHandle | hEdma,
|  | Uint16 * | paramNum |
| ) |  |  |

============================================================================
CSL_edma3GetHwChannelSetupParam

Description
The function gets the DMA/QDMA Channel to PARAM Entry Mapping.

Arguments

                hEdma           Channel Handle
                paramNum        Pointer to parameter entry to which the channel
                                is mapped.

Return Value
Success - CSL_SOK
Error - CSL_ESYS_BADHANDLE (The handle passed is invalid)
Error - CSL_ESYS_INVPARAMS (The parameters passed is invalid)

Pre Condition
Functions CSL_edma3Init(), CSL_edma3Open() and CSL_edma3ChannelOpen() must be called successfully in that order before CSL_edma3GetHwChannelSetupParam() can be invoked.

Post Condition
None

Reads
TPCC_TPCC_DCHMAP_PAENTRY;
TPCC_TPCC_QCHMAP_PAENTRY

Example

                CSL_Edma3Handle             hModule;
                CSL_Edma3Obj                edmaObj;
                CSL_Edma3ChannelObj         chObj;
                CSL_Edma3ChannelHandle      hChannel;
                CSL_Edma3ChannelAttr        chAttr;
                CSL_Status                  status;
                Uint16                      paramNum;

                // Module Initialization
                CSL_edma3Init(NULL);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, 0, NULL,&status);

                // Channel 0 Open in context of Shadow region 0
                chAttr.regionNum = CSL_EDMA3_REGION_0;
                chAttr.chaNum    = 0;
                hChannel = CSL_edma3ChannelOpen(&chObj, 0, &chAttr, &status);
                ...
                // Get the parameter entry number to which a channel is mapped to
                CSL_edma3GetHwChannelSetupParam(hChannel,&paramNum);
                ...

=============================================================================

CSL_Status CSL_edma3GetHwChannelSetupQue | ( | CSL_Edma3ChannelHandle | hEdma,
|  | CSL_Edma3Que * | evtQue |
| ) |  |  |

============================================================================
CSL_edma3GetHwChannelSetupQue

Description
The function gets the event queue to which the specific DMA/QDMA channel is mapped.

Arguments

                hEdma           Channel Handle
                evtQue          Event Queue to which the DMA/QDMA channel is mapped.

Return Value
Success - CSL_SOK
Error - CSL_ESYS_BADHANDLE (The handle passed is invalid)
Error - CSL_ESYS_INVPARAMS (The parameters passed is invalid)

Pre Condition
Functions CSL_edma3Init(), CSL_edma3Open() and CSL_edma3ChannelOpen() must be called successfully in that order before CSL_edma3GetHwChannelSetupQue() can be called.

Post Condition
None

Reads
TPCC_TPCC_QDMAQNUM_E0;TPCC_TPCC_QDMAQNUM_E1;TPCC_TPCC_QDMAQNUM_E2; TPCC_TPCC_QDMAQNUM_E3;TPCC_TPCC_QDMAQNUM_E4;TPCC_TPCC_QDMAQNUM_E5; TPCC_TPCC_QDMAQNUM_E6;TPCC_TPCC_QDMAQNUM_E7;
TPCC_TPCC_DMAQNUM_E0;TPCC_TPCC_DMAQNUM_E1;TPCC_TPCC_DMAQNUM_E2; TPCC_TPCC_DMAQNUM_E3;TPCC_TPCC_DMAQNUM_E4;TPCC_TPCC_DMAQNUM_E5; TPCC_TPCC_DMAQNUM_E6;TPCC_TPCC_DMAQNUM_E7

Example

                CSL_Edma3Handle             hModule;
                CSL_Edma3Obj                edmaObj;
                CSL_Edma3ChannelObj         chObj;
                CSL_Edma3ChannelHandle      hChannel;
                CSL_Edma3ChannelAttr        chAttr;
                CSL_Status                  status;
                CSL_Edma3Que                evtQue;

                // Module Initialization
                CSL_edma3Init(NULL);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, 0, NULL,&status);

                // Channel 0 Open in context of Shadow region 0
                chAttr.regionNum = CSL_EDMA3_REGION_0;
                chAttr.chaNum    = 0;
                hChannel = CSL_edma3ChannelOpen(&chObj, 0, &chAttr, &status);
                ...
                // Get the trigger word programmed for the channel
                CSL_edma3GetHwChannelSetupQue(hChannel, &evtQue);
                ...

=============================================================================

CSL_Status CSL_edma3GetHwChannelSetupTriggerWord | ( | CSL_Edma3ChannelHandle | hEdma,
|  | Uint8 * | triggerWord |
| ) |  |  |

============================================================================
CSL_edma3GetHwChannelSetupTriggerWord

Description
The function gets the Trigger word for a specific QDMA Channel.

Arguments

                hEdma           Channel Handle (Only QDMA Channels)
                triggerWord     Pointer to Trigger word populated by this API.

Return Value
Success - CSL_SOK
Error - CSL_ESYS_BADHANDLE (The handle passed is invalid)
Error - CSL_ESYS_INVPARAMS (The parameters passed is invalid)

Pre Condition
Functions CSL_edma3Init(), CSL_edma3Open() and CSL_edma3ChannelOpen() must be called successfully in that order before CSL_edma3GetHwChannelSetupTriggerWord() can be called.

Post Condition
None

Reads
TPCC_TPCC_QCHMAP0_TRWORD

Example

                CSL_Edma3Handle             hModule;
                CSL_Edma3Obj                edmaObj;
                CSL_Edma3ChannelObj         chObj;
                CSL_Edma3ChannelHandle      hChannel;
                CSL_Edma3ChannelAttr        chAttr;
                CSL_Status                  status;
                Uint8                       triggerWord;

                // Module Initialization
                CSL_edma3Init(NULL);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, 0, NULL,&status);

                // Channel 0 Open in context of Shadow region 0
                chAttr.regionNum = CSL_EDMA3_REGION_0;
                chAttr.chaNum    = 0;
                hChannel = CSL_edma3ChannelOpen(&chObj, 0, &chAttr, &status);
                ...
                // Get the trigger word programmed for the channel
                CSL_edma3GetHwChannelSetupTriggerWord(hChannel,&triggerWord);
                ...

=============================================================================

CSL_Status CSL_edma3GetHwChannelStatus | ( | CSL_Edma3ChannelHandle | hEdma,
|  | CSL_Edma3HwChannelStatusQuery | myQuery,
|  | void * | response |
| ) |  |  |

============================================================================
CSL_edma3GetHwChannelStatus

Description
The function is to used to get the status of entities specific to an EDMA Channel. The channel specific entity to be queried is specified in the argument.

Arguments

                hEdma           Channel Handle
                myQuery         Query to be performed
                response        Pointer to buffer to return the data requested by
                                the query passed

See also:
  CSL_Edma3HwChannelStatusQuery

Return Value
Success - CSL_SOK
Error - CSL_ESYS_BADHANDLE (The handle passed is invalid)
Error - CSL_ESYS_INVQUERY (The query passed is invalid)

Pre Condition
Functions CSL_edma3Init(), CSL_edma3Open() and CSL_edma3ChannelOpen() must be called successfully in that order before this API can be invoked.If a Shadow region is used then care of the DRAE settings must be taken

Post Condition
None

Reads
TPCC_TPCC_ER_E0;TPCC_TPCC_ER_E1;TPCC_TPCC_ER_E2;TPCC_TPCC_ER_E3; TPCC_TPCC_ER_E4;TPCC_TPCC_ER_E5;TPCC_TPCC_ER_E6;TPCC_TPCC_ER_E7; TPCC_TPCC_ER_E8;TPCC_TPCC_ER_E9;TPCC_TPCC_ER_E10;TPCC_TPCC_ER_E11; TPCC_TPCC_ER_E12;TPCC_TPCC_ER_E13;TPCC_TPCC_ER_E14;TPCC_TPCC_ER_E15; TPCC_TPCC_ER_E16;TPCC_TPCC_ER_E17;TPCC_TPCC_ER_E18;TPCC_TPCC_ER_E19; TPCC_TPCC_ER_E20;TPCC_TPCC_ER_E21;TPCC_TPCC_ER_E22;TPCC_TPCC_ER_E23; TPCC_TPCC_ER_E24;TPCC_TPCC_ER_E25;TPCC_TPCC_ER_E26;TPCC_TPCC_ER_E27; TPCC_TPCC_ER_E28;TPCC_TPCC_ER_E29;TPCC_TPCC_ER_E30;TPCC_TPCC_ER_E31;
TPCC_TPCC_ERH_E32;TPCC_TPCC_ERH_E33;TPCC_TPCC_ERH_E34;TPCC_TPCC_ERH_E35; TPCC_TPCC_ERH_E36;TPCC_TPCC_ERH_E37;TPCC_TPCC_ERH_E38;TPCC_TPCC_ERH_E39; TPCC_TPCC_ERH_E40;TPCC_TPCC_ERH_E41;TPCC_TPCC_ERH_E42;TPCC_TPCC_ERH_E43; TPCC_TPCC_ERH_E44;TPCC_TPCC_ERH_E45;TPCC_TPCC_ERH_E46;TPCC_TPCC_ERH_E47; TPCC_TPCC_ERH_E48;TPCC_TPCC_ERH_E49;TPCC_TPCC_ERH_E50;TPCC_TPCC_ERH_E51; TPCC_TPCC_ERH_E52;TPCC_TPCC_ERH_E53;TPCC_TPCC_ERH_E54;TPCC_TPCC_ERH_E55; TPCC_TPCC_ERH_E56;TPCC_TPCC_ERH_E57;TPCC_TPCC_ERH_E58;TPCC_TPCC_ERH_E59; TPCC_TPCC_ERH_E60;TPCC_TPCC_ERH_E61;TPCC_TPCC_ERH_E62;TPCC_TPCC_ERH_E63;
TPCC_TPCC_QER_QER0;TPCC_TPCC_QER_QER1;TPCC_TPCC_QER_QER2;TPCC_TPCC_QER_QER3; TPCC_TPCC_QER_QER4;TPCC_TPCC_QER_QER5;TPCC_TPCC_QER_QER6;TPCC_TPCC_QER_QER7;
TPCC_TPCC_EMR_EMR0;TPCC_TPCC_EMR_EMR1;TPCC_TPCC_EMR_EMR2; TPCC_TPCC_EMR_EMR3;TPCC_TPCC_EMR_EMR4;TPCC_TPCC_EMR_EMR5; TPCC_TPCC_EMR_EMR6;TPCC_TPCC_EMR_EMR7;TPCC_TPCC_EMR_EMR8; TPCC_TPCC_EMR_EMR9;TPCC_TPCC_EMR_EMR10;TPCC_TPCC_EMR_EMR11; TPCC_TPCC_EMR_EMR12;TPCC_TPCC_EMR_EMR13;TPCC_TPCC_EMR_EMR14; TPCC_TPCC_EMR_EMR15;TPCC_TPCC_EMR_EMR16;TPCC_TPCC_EMR_EMR17; TPCC_TPCC_EMR_EMR18;TPCC_TPCC_EMR_EMR19;TPCC_TPCC_EMR_EMR20; TPCC_TPCC_EMR_EMR21;TPCC_TPCC_EMR_EMR22;TPCC_TPCC_EMR_EMR23; TPCC_TPCC_EMR_EMR24;TPCC_TPCC_EMR_EMR25;TPCC_TPCC_EMR_EMR26; TPCC_TPCC_EMR_EMR27;TPCC_TPCC_EMR_EMR28;TPCC_TPCC_EMR_EMR29; TPCC_TPCC_EMR_EMR30;TPCC_TPCC_EMR_EMR31;
TPCC_TPCC_EMRH_EMR32;TPCC_TPCC_EMRH_EMR33;TPCC_TPCC_EMRH_EMR34; TPCC_TPCC_EMRH_EMR35;TPCC_TPCC_EMRH_EMR36;TPCC_TPCC_EMRH_EMR37; TPCC_TPCC_EMRH_EMR38;TPCC_TPCC_EMRH_EMR39;TPCC_TPCC_EMRH_EMR40; TPCC_TPCC_EMRH_EMR41;TPCC_TPCC_EMRH_EMR42;TPCC_TPCC_EMRH_EMR43; TPCC_TPCC_EMRH_EMR44;TPCC_TPCC_EMRH_EMR45;TPCC_TPCC_EMRH_EMR46; TPCC_TPCC_EMRH_EMR47;TPCC_TPCC_EMRH_EMR48;TPCC_TPCC_EMRH_EMR49; TPCC_TPCC_EMRH_EMR50;TPCC_TPCC_EMRH_EMR51;TPCC_TPCC_EMRH_EMR52; TPCC_TPCC_EMRH_EMR53;TPCC_TPCC_EMRH_EMR54;TPCC_TPCC_EMRH_EMR55; TPCC_TPCC_EMRH_EMR56;TPCC_TPCC_EMRH_EMR57;TPCC_TPCC_EMRH_EMR58; TPCC_TPCC_EMRH_EMR59;TPCC_TPCC_EMRH_EMR60;TPCC_TPCC_EMRH_EMR61; TPCC_TPCC_EMRH_EMR62;TPCC_TPCC_EMRH_EMR63,
TPCC_TPCC_SER_SER0;TPCC_TPCC_SER_SER1;TPCC_TPCC_SER_SER2; TPCC_TPCC_SER_SER3;TPCC_TPCC_SER_SER4;TPCC_TPCC_SER_SER5; TPCC_TPCC_SER_SER6;TPCC_TPCC_SER_SER7;TPCC_TPCC_SER_SER8; TPCC_TPCC_SER_SER9;TPCC_TPCC_SER_SER10;TPCC_TPCC_SER_SER11; TPCC_TPCC_SER_SER12;TPCC_TPCC_SER_SER13;TPCC_TPCC_SER_SER14; TPCC_TPCC_SER_SER15;TPCC_TPCC_SER_SER16;TPCC_TPCC_SER_SER17; TPCC_TPCC_SER_SER18;TPCC_TPCC_SER_SER19;TPCC_TPCC_SER_SER20; TPCC_TPCC_SER_SER21;TPCC_TPCC_SER_SER22;TPCC_TPCC_SER_SER23; TPCC_TPCC_SER_SER24;TPCC_TPCC_SER_SER25;TPCC_TPCC_SER_SER26; TPCC_TPCC_SER_SER27;TPCC_TPCC_SER_SER28;TPCC_TPCC_SER_SER29; TPCC_TPCC_SER_SER30;TPCC_TPCC_SER_SER31;
TPCC_TPCC_SERH_SER32;TPCC_TPCC_SERH_SER33;TPCC_TPCC_SERH_SER34; TPCC_TPCC_SERH_SER35;TPCC_TPCC_SERH_SER36;TPCC_TPCC_SERH_SER37; TPCC_TPCC_SERH_SER38;TPCC_TPCC_SERH_SER39;TPCC_TPCC_SERH_SER40; TPCC_TPCC_SERH_SER41;TPCC_TPCC_SERH_SER42;TPCC_TPCC_SERH_SER43; TPCC_TPCC_SERH_SER44;TPCC_TPCC_SERH_SER45;TPCC_TPCC_SERH_SER46; TPCC_TPCC_SERH_SER47;TPCC_TPCC_SERH_SER48;TPCC_TPCC_SERH_SER49; TPCC_TPCC_SERH_SER50;TPCC_TPCC_SERH_SER51;TPCC_TPCC_SERH_SER52; TPCC_TPCC_SERH_SER53;TPCC_TPCC_SERH_SER54;TPCC_TPCC_SERH_SER55; TPCC_TPCC_SERH_SER56;TPCC_TPCC_SERH_SER57;TPCC_TPCC_SERH_SER58; TPCC_TPCC_SERH_SER59;TPCC_TPCC_SERH_SER60;TPCC_TPCC_SERH_SER61; TPCC_TPCC_SERH_SER62;TPCC_TPCC_SERH_SER63;
TPCC_TPCC_QEMR_QEMR0;TPCC_TPCC_QEMR_QEMR1;TPCC_TPCC_QEMR_QEMR2; TPCC_TPCC_QEMR_QEMR3;TPCC_TPCC_QEMR_QEMR4;TPCC_TPCC_QEMR_QEMR5; TPCC_TPCC_QEMR_QEMR6;TPCC_TPCC_QEMR_QEMR7,
TPCC_TPCC_QSER_QSER0;TPCC_TPCC_QSER_QSER1;TPCC_TPCC_QSER_QSER2; TPCC_TPCC_QSER_QSER3;TPCC_TPCC_QSER_QSER4;TPCC_TPCC_QSER_QSER5; TPCC_TPCC_QSER_QSER6;TPCC_TPCC_QSER_QSER7;

Example

                CSL_Edma3Handle             hModule;
                CSL_Edma3Obj                edmaObj;
                CSL_Edma3ChannelObj         chObj;
                CSL_Edma3ChannelHandle      hChannel;
                CSL_Edma3ChannelAttr        chAttr;
                CSL_Status                  status;
                CSL_Edma3ChannelErr         errStat;

                // Module Initialization
                CSL_edma3Init(NULL);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, 0, NULL,&status);

                // Channel 0 Open in context of Shadow region 0
                chAttr.regionNum = CSL_EDMA3_REGION_0;
                chAttr.chaNum    = 0;
                hChannel = CSL_edma3ChannelOpen(&chObj, 0, &chAttr, &status);
                ...
                // Get the Channel 0 Error Status
                CSL_edma3GetHwChannelStatus(hChannel, CSL_EDMA3_QUERY_CHANNEL_ERR, &errStat);
                ...

=============================================================================

CSL_Status CSL_edma3GetHwSetup | ( | CSL_Edma3Handle | hMod,
|  | CSL_Edma3HwSetup * | setup |
| ) |  |  |

============================================================================
CSL_edma3GetHwSetup

Description
The function gets the hardware setup for all DMA/QDMA Channels.

Arguments

                hMod            EDMA Handle
                setup           Setup structure which is populated by this API.

Return Value
Success - CSL_SOK
Error - CSL_ESYS_BADHANDLE (The handle passed is invalid)
Error - CSL_ESYS_INVPARAMS (The parameter passed is invalid)

Pre Condition
Functions CSL_edma3Init(), CSL_edma3Open() must be called successfully in that order before CSL_edma3GetHwSetup() can be called.

Post Condition
The hardware setup structure is populated with the hardware setup parameters

Reads
TPCC_TPCC_DCHMAP_PAENTRY,
TPCC_TPCC_DMAQNUM_E0;TPCC_TPCC_DMAQNUM_E1;TPCC_TPCC_DMAQNUM_E2; TPCC_TPCC_DMAQNUM_E3;TPCC_TPCC_DMAQNUM_E4;TPCC_TPCC_DMAQNUM_E5; TPCC_TPCC_DMAQNUM_E6;TPCC_TPCC_DMAQNUM_E7;
TPCC_TPCC_QCHMAP_PAENTRY,
TPCC_TPCC_QCHMAP_TRWORD,
TPCC_TPCC_QDMAQNUM_E0;TPCC_TPCC_QDMAQNUM_E1;TPCC_TPCC_QDMAQNUM_E2; TPCC_TPCC_QDMAQNUM_E3;TPCC_TPCC_QDMAQNUM_E4;TPCC_TPCC_QDMAQNUM_E5; TPCC_TPCC_QDMAQNUM_E6;TPCC_TPCC_QDMAQNUM_E7

Example

                CSL_Edma3Handle             hModule;
                CSL_Edma3Obj                edmaObj;
                CSL_Status                  status;
                CSL_Edma3QueryInfo          info;
                CSL_Edma3HwSetup            setup;
                CSL_Edma3HwDmaChannelSetup  dmahwSetup;

                // Module Initialization
                CSL_edma3Init(NULL);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Get DMA Channel Setup for all channels.
                setup.dmaChaSetup  = &dmahwSetup[0];
                setup.qdmaChaSetup = NULL;
                CSL_edma3GetHwSetup(hModule,&setup);
                ...

=============================================================================

CSL_Status CSL_edma3GetHwStatus | ( | CSL_Edma3Handle | hMod,
|  | CSL_Edma3HwStatusQuery | myQuery,
|  | void * | response |
| ) |  |  |

============================================================================
CSL_edma3GetHwStatus

Description
The function gets the status of various entities in the EDMA module. The entity whose status needs to be retreived is specified in the query and the response is populated in the 'response'.

Arguments

                hMod            Edma module handle
                myQuery         Query to be performed
                response        Pointer to buffer to return the data requested by
                                the query passed

See also:
  CSL_Edma3HwStatusQuery

Return Value
Success - CSL_SOK
Error - CSL_ESYS_BADHANDLE (The handle passed is invalid)
Error - CSL_ESYS_INVPARAMS (The parameter passed is invalid)
Error - CSL_ESYS_INVQUERY (The query is invalid)

Pre Condition
Functions CSL_edma3Init(), CSL_edma3Open() must be called successfully in that order before this API can be invoked.argument type that can be void* casted & passed with a particular command refer to CSL_Edma3HwStatusQuery

Post Condition
None

Reads
TPCC_TPCC_CFG,TPCC_TPCC_PID;

Example

                CSL_Edma3Handle             hModule;
                CSL_Edma3Obj                edmaObj;
                CSL_Status                  status;
                CSL_Edma3QueryInfo          info;

                // Module Initialization
                CSL_edma3Init(NULL);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Query Module Info
                CSL_edma3GetHwStatus(hModule,CSL_EDMA3_QUERY_INFO,&info);
                ...

=============================================================================

CSL_IDEF_INLINE void CSL_edma3GetInfo | ( | CSL_Edma3Handle | hModule,
|  | CSL_Edma3QueryInfo * | response |
| ) |  |  |

============================================================================
CSL_edma3GetInfo

Description
The function gets the EDMA Channel Controller Configuration Information which includes reading the peripheral revision register and configuration register.

Arguments

            hModule     Module Handle
            response    Output parameter populated with the configuration information.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_CFG,TPCC_TPCC_PID

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                CSL_Edma3QueryInfo      info;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, CSL_EDMA3, NULL, &status);

                // Get Module Info
                CSL_edma3GetInfo(hModule,&info);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3GetLoPendingInterrupts | ( | CSL_Edma3Handle | hModule,
|  | Int | region,
|  | CSL_BitMask32 * | intrLo |
| ) |  |  |

============================================================================
CSL_edma3GetLoPendingInterrupts

Description
The API gets a bitmask of all low pending interrupts.

Arguments

            hModule           Module Handle
            region            Region (Shadown Region or Global)
            intrLo            Status 0-31 of the interrupts

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_IPR

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                CSL_BitMask32           edmaIntrLo;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Get all low pending interrupts for the global region.
                CSL_edma3GetLoPendingInterrupts(hModule, CSL_EDMA3_REGION_GLOBAL, &edmaIntrLo);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3GetMemoryFaultError | ( | CSL_Edma3Handle | hModule,
|  | CSL_Edma3MemFaultStat * | memFault |
| ) |  |  |

============================================================================
CSL_edma3GetMemoryFaultError

Description
The function gets the Controllers memory fault error and the error attributes.

Arguments

            hModule           Module Handle
            memFault          The structure is populated by this API.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_MPFAR_FADDR,TPCC_TPCC_MPFSR_FID, TPCC_TPCC_MPFSR_UXE,TPCC_TPCC_MPFSR_UWE,TPCC_TPCC_MPFSR_URE, TPCC_TPCC_MPFSR_SXE,TPCC_TPCC_MPFSR_SWE,TPCC_TPCC_MPFSR_SRE, TPCC_TPCC_MPFSR_SECE

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                CSL_Edma3MemFaultStat   memFault;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Get memory protection fault
                CSL_edma3GetMemoryFaultError(hModule, &memFault);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3GetMemoryProtectionAttrib | ( | CSL_Edma3Handle | hModule,
|  | Int | region,
|  | CSL_BitMask32 * | mppa |
| ) |  |  |

============================================================================
CSL_edma3GetMemoryProtectionAttrib

Description
The function gets the memory access/protection attributes of the specific region.

Arguments

            hModule           Module Handle
            region            Region being queried.
            mppa              Memory Access/Protection Attributes populated by this API

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_MPPAG;TPCC_TPCC_MPPA

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                CSL_BitMask32           mppa;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Get memory protection attributes for the Global Region.
                CSL_edma3GetMemoryProtectionAttrib(hModule, -1, &mppa);
                ...
                // Get memory protection attributes for region 2
                CSL_edma3GetMemoryProtectionAttrib(hModule, 2, &mppa);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3GetNumberValidEntries | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | eventQueue,
|  | Uint8 * | numValidEntries |
| ) |  |  |

============================================================================
CSL_edma3GetNumberValidEntries

Description
The function gets the Number of valid entries for the specific event queue.

Arguments

            hModule           Module Handle
            eventQueue        Event queue number for which the watermark is retreived.
            numValidEntries   This is populated by the API to the number of valid entries

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_QSTAT_NUMVAL

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                Uint8                   numVal;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Get the Number of valid entries in event queue 0.
                CSL_edma3GetNumberValidEntries(hModule, 0, &numVal);
                ...

===========================================================================

CSL_Edma3ParamHandle CSL_edma3GetParamHandle | ( | CSL_Edma3ChannelHandle | hEdma,
|  | Int16 | paramNum,
|  | CSL_Status * | status |
| ) |  |  |

============================================================================
CSL_edma3GetParamHandle

Description
The function is used to get a specific PARAM Entry handle.

Arguments

                hEdma           Channel Handle
                paramNum        Parameter entry number
                status          Status of the function call

Return Value
Success - CSL_SOK
Error - CSL_ESYS_BADHANDLE (The handle passed is invalid)
Error - CSL_ESYS_INVPARAMS (The parameter passed is invalid)

Pre Condition
CSL_edma3Init(), CSL_edma3Open() and CSL_edma3ChannelOpen() must be called successfully in that order before this API can be invoked

Post Condition
None

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Status              status;
                CSL_Edma3ChannelHandle  hChannel;
                CSL_Edma3ChannelAttr    chAttr;
                CSL_Edma3ParamHandle    hParamBasic;

                // Module Initialization
                CSL_edma3Init(NULL);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Open DMA Channel 1.
                chAttr.regionNum = CSL_EDMA3_REGION_GLOBAL;
                chAttr.chaNum    = 1;
                hChannel = CSL_edma3ChannelOpen(&chObj, 0, &chAttr, &status);
                if ((hChannel == NULL) || (status != CSL_SOK))
                {
                    printf ("Error: Unable to open EDMA Channel:%d\n", channelNum);
                    return -1;
                }
                ...
                // Obtain a handle to PARAM Entry 0
                hParamBasic = CSL_edma3GetParamHandle(hChannel,0,&status);
                ...

=============================================================================

CSL_IDEF_INLINE Uint8 CSL_edma3GetQDMAChannelToEventQueueMapping | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | qdmaChannel |
| ) |  |  |

============================================================================
CSL_edma3GetQDMAChannelToEventQueueMapping

Description
The function gets the mapping of the QDMA Channel to the Event Queue

Arguments

            hModule     Module Handle
            qdmaChannel QDMA Channel for which the mapping is to be retreived.

Return Value
Event Queue to which the QDMA channel is mapped to

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_QDMAQNUM_E0;TPCC_TPCC_QDMAQNUM_E1;TPCC_TPCC_QDMAQNUM_E2; TPCC_TPCC_QDMAQNUM_E3;TPCC_TPCC_QDMAQNUM_E4;TPCC_TPCC_QDMAQNUM_E5; TPCC_TPCC_QDMAQNUM_E6;TPCC_TPCC_QDMAQNUM_E7

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                Uint8                   eventQueue;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, CSL_EDMA3, NULL, &status);

                // Get the Event Queue mapping of QDMA Channel 1
                eventQueue = CSL_edma3GetQDMAChannelToEventQueueMapping(hModule, 1);
                ...

===========================================================================

CSL_IDEF_INLINE Uint16 CSL_edma3GetQDMAChannelToParamBlockMapping | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | qdmaChannel |
| ) |  |  |

============================================================================
CSL_edma3GetQDMAChannelToParamBlockMapping

Description
The function gets the PARAM Entry ID to which a specific QDMA Channel is mapped.

Arguments

            hModule     Module Handle
            qdmaChannel QDMA Channel Number whose mapping is to be found.

Return Value
Paramater ID to which the specific QDMA Channel is mapped to.

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_QCHMAP_PAENTRY

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, CSL_EDMA3, NULL, &status);

                // Get the mapping information for QDMA channel 1.
                paramId = CSL_edma3GetQDMAChannelMap(hModule, 1);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3GetQDMASecondaryEvents | ( | CSL_Edma3Handle | hModule,
|  | Uint32 * | qdmaSecEvent |
| ) |  |  |

============================================================================
CSL_edma3GetQDMASecondaryEvents

Description
This API reads the QDMA Secondary Event.

Arguments

            hModule         Module Handle
            qdmaSecEvent    QDMA Secondary Event which is populated by this API

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_QSER

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                Uint32                  qdmaSecEvent;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Get the QDMA Secondary Event
                CSL_edma3GetQDMASecondaryEvents(hModule, &qdmaSecEvent);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3GetQDMATriggerWord | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | qdmaChannel,
|  | Uint8 * | trword |
| ) |  |  |

============================================================================
CSL_edma3GetQDMATriggerWord

Description
The function gets the trigger word of the PaRAM Entry block.

Arguments

            hModule     Module Handle
            qdmaChannel QDMA Channel Number which is to be configured.
            trword      Trigger Word to be retreived populated by this API.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
QDMA Channel is mapped to the specified PARAM Block.

Reads
TPCC_TPCC_QCHMAP_TRWORD

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                Uint8                   trWord;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, CSL_EDMA3, NULL, &status);

                // Get the QDMA Channel 1 Trigger Word
                trWord = CSL_edma3SetQDMATriggerWord(hModule, 1);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3GetStartPointer | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | eventQueue,
|  | Uint8 * | startPtr |
| ) |  |  |

============================================================================
CSL_edma3GetStartPointer

Description
The function gets the Number of valid entries for the specific event queue.

Arguments

            hModule           Module Handle
            eventQueue        Event queue number for which the watermark is retreived.
            startPtr          This is populated by the API to the start pointer

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_QSTAT_STRPTR

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                Uint8                   startPtr;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Get the Number of valid entries in event queue 0.
                CSL_edma3GetStartPointer(hModule, 0, &startPtr);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3GetThresholdExceeded | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | eventQueue,
|  | Bool * | thresholdExceeded |
| ) |  |  |

============================================================================
CSL_edma3GetThresholdExceeded

Description
The function gets the threshold exceeded flag for the specific event queue.

Arguments

            hModule           Module Handle
            eventQueue        Event queue number for which the watermark is retreived.
            thresholdExceeded This is populated by the API to the threshold exceeded flag
                              for the specific event queue.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_QSTAT_THRXCD

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                Uint8                   thresholdExceeded;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Determine if the threshold has been exceeded or not for Queue 1
                CSL_edma3GetThresholdExceeded(hModule, 1, &thresholdExceeded);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3GetWaterMark | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | eventQueue,
|  | Uint8 * | waterMark |
| ) |  |  |

============================================================================
CSL_edma3GetWaterMark

Description
The function gets the Queue Watermark for the specific event queue.

Arguments

            hModule           Module Handle
            eventQueue        Event queue number for which the watermark is retreived.
            waterMark         This is populated by the API to the configured water mark

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_QSTAT_WM

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                Uint8                   waterMark;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Get the Water Mark Queue for event queue 0
                CSL_edma3GetWaterMark(hModule, 0, &waterMark);
                ...

===========================================================================

CSL_Status CSL_edma3HwChannelControl | ( | CSL_Edma3ChannelHandle | hCh,
|  | CSL_Edma3HwChannelControlCmd | cmd,
|  | void * | cmdArg |
| ) |  |  |

============================================================================
CSL_edma3HwChannelControl

Description
This API is used to control the EDMA Channel. The function accepts a command as an argument on the type of operation which is to be performed on the specific channel.

Arguments

                hCh             Channel Handle
                cmd             Command/Action to be performed on the channel handle.
                cmdArg          Pointer to the argument specific to the command

Return Value
Success - CSL_SOK
Error - CSL_ESYS_BADHANDLE (The handle passed is invalid)
Error - CSL_ESYS_INVPARAMS (The parameter passed is invalid)

Pre Condition
Functions CSL_edma3Init(), CSL_edma3Open() and CSL_edma3ChannelOpen() must be called successfully in that order before this API can be invoked. If a Shadow region is used then care of the DRAE settings must be taken care of.

Post Condition
Edma registers are configured according to the command and the command arguements. The command determines which registers are modified.

Writes
TPCC_TPCC_QEESR_QEESR0=1;TPCC_TPCC_QEESR_QEESR1=1;TPCC_TPCC_QEESR_QEESR2=1; TPCC_TPCC_QEESR_QEESR3=1;TPCC_TPCC_QEESR_QEESR4=1;TPCC_TPCC_QEESR_QEESR5=1; TPCC_TPCC_QEESR_QEESR6=1;TPCC_TPCC_QEESR_QEESR7=1;
TPCC_TPCC_EESR_E0=1;TPCC_TPCC_EESR_E1=1;TPCC_TPCC_EESR_E2=1; TPCC_TPCC_EESR_E3=1;TPCC_TPCC_EESR_E4=1;TPCC_TPCC_EESR_E5=1; TPCC_TPCC_EESR_E6=1;TPCC_TPCC_EESR_E7=1;TPCC_TPCC_EESR_E8=1; TPCC_TPCC_EESR_E9=1;TPCC_TPCC_EESR_E10=1;TPCC_TPCC_EESR_E11=1; TPCC_TPCC_EESR_E12=1;TPCC_TPCC_EESR_E13=1;TPCC_TPCC_EESR_E14=1; TPCC_TPCC_EESR_E15=1;TPCC_TPCC_EESR_E16=1;TPCC_TPCC_EESR_E17=1; TPCC_TPCC_EESR_E18=1;TPCC_TPCC_EESR_E19=1;TPCC_TPCC_EESR_E20=1; TPCC_TPCC_EESR_E21=1;TPCC_TPCC_EESR_E22=1;TPCC_TPCC_EESR_E23=1; TPCC_TPCC_EESR_E24=1;TPCC_TPCC_EESR_E25=1;TPCC_TPCC_EESR_E26=1; TPCC_TPCC_EESR_E27=1;TPCC_TPCC_EESR_E28=1;TPCC_TPCC_EESR_E29=1; TPCC_TPCC_EESR_E30=1;TPCC_TPCC_EESR_E31=1;
TPCC_TPCC_EESRH_E32=1;TPCC_TPCC_EESRH_E33=1;TPCC_TPCC_EESRH_E34=1; TPCC_TPCC_EESRH_E35=1;TPCC_TPCC_EESRH_E36=1;TPCC_TPCC_EESRH_E37=1; TPCC_TPCC_EESRH_E38=1;TPCC_TPCC_EESRH_E39=1;TPCC_TPCC_EESRH_E40=1; TPCC_TPCC_EESRH_E41=1;TPCC_TPCC_EESRH_E42=1;TPCC_TPCC_EESRH_E43=1; TPCC_TPCC_EESRH_E44=1;TPCC_TPCC_EESRH_E45=1;TPCC_TPCC_EESRH_E46=1; TPCC_TPCC_EESRH_E47=1;TPCC_TPCC_EESRH_E48=1;TPCC_TPCC_EESRH_E49=1; TPCC_TPCC_EESRH_E50=1;TPCC_TPCC_EESRH_E51=1;TPCC_TPCC_EESRH_E52=1; TPCC_TPCC_EESRH_E53=1;TPCC_TPCC_EESRH_E54=1;TPCC_TPCC_EESRH_E55=1; TPCC_TPCC_EESRH_E56=1;TPCC_TPCC_EESRH_E57=1;TPCC_TPCC_EESRH_E58=1; TPCC_TPCC_EESRH_E59=1;TPCC_TPCC_EESRH_E60=1;TPCC_TPCC_EESRH_E61=1; TPCC_TPCC_EESRH_E62=1;TPCC_TPCC_EESRH_E63=1;
TPCC_TPCC_QEECR_QEECR0=1;TPCC_TPCC_QEECR_QEECR1=1;TPCC_TPCC_QEECR_QEECR2=1; TPCC_TPCC_QEECR_QEECR3=1;TPCC_TPCC_QEECR_QEECR4=1;TPCC_TPCC_QEECR_QEECR5=1; TPCC_TPCC_QEECR_QEECR6=1;TPCC_TPCC_QEECR_QEECR7=1;
TPCC_TPCC_EECR_E0=1;TPCC_TPCC_EECR_E1=1;TPCC_TPCC_EECR_E2=1; TPCC_TPCC_EECR_E3=1;TPCC_TPCC_EECR_E4=1;TPCC_TPCC_EECR_E5=1; TPCC_TPCC_EECR_E6=1;TPCC_TPCC_EECR_E7=1;TPCC_TPCC_EECR_E8=1; TPCC_TPCC_EECR_E9=1;TPCC_TPCC_EECR_E10=1;TPCC_TPCC_EECR_E11=1; TPCC_TPCC_EECR_E12=1;TPCC_TPCC_EECR_E13=1;TPCC_TPCC_EECR_E14=1; TPCC_TPCC_EECR_E15=1;TPCC_TPCC_EECR_E16=1;TPCC_TPCC_EECR_E17=1; TPCC_TPCC_EECR_E18=1;TPCC_TPCC_EECR_E19=1;TPCC_TPCC_EECR_E20=1; TPCC_TPCC_EECR_E21=1;TPCC_TPCC_EECR_E22=1;TPCC_TPCC_EECR_E23=1; TPCC_TPCC_EECR_E24=1;TPCC_TPCC_EECR_E25=1;TPCC_TPCC_EECR_E26=1; TPCC_TPCC_EECR_E27=1;TPCC_TPCC_EECR_E28=1;TPCC_TPCC_EECR_E29=1; TPCC_TPCC_EECR_E30=1;TPCC_TPCC_EECR_E31=1;
TPCC_TPCC_EECRH_E32=1;TPCC_TPCC_EECRH_E33=1;TPCC_TPCC_EECRH_E34=1; TPCC_TPCC_EECRH_E35=1;TPCC_TPCC_EECRH_E36=1;TPCC_TPCC_EECRH_E37=1; TPCC_TPCC_EECRH_E38=1;TPCC_TPCC_EECRH_E39=1;TPCC_TPCC_EECRH_E40=1; TPCC_TPCC_EECRH_E41=1;TPCC_TPCC_EECRH_E42=1;TPCC_TPCC_EECRH_E43=1; TPCC_TPCC_EECRH_E44=1;TPCC_TPCC_EECRH_E45=1;TPCC_TPCC_EECRH_E46=1; TPCC_TPCC_EECRH_E47=1;TPCC_TPCC_EECRH_E48=1;TPCC_TPCC_EECRH_E49=1; TPCC_TPCC_EECRH_E50=1;TPCC_TPCC_EECRH_E51=1;TPCC_TPCC_EECRH_E52=1; TPCC_TPCC_EECRH_E53=1;TPCC_TPCC_EECRH_E54=1;TPCC_TPCC_EECRH_E55=1; TPCC_TPCC_EECRH_E56=1;TPCC_TPCC_EECRH_E57=1;TPCC_TPCC_EECRH_E58=1; TPCC_TPCC_EECRH_E59=1;TPCC_TPCC_EECRH_E60=1;TPCC_TPCC_EECRH_E61=1; TPCC_TPCC_EECRH_E62=1;TPCC_TPCC_EECRH_E63=1;
TPCC_TPCC_ESR_E0=1;TPCC_TPCC_ESR_E1=1;TPCC_TPCC_ESR_E2=1;TPCC_TPCC_ESR_E3=1; TPCC_TPCC_ESR_E4=1;TPCC_TPCC_ESR_E5=1;TPCC_TPCC_ESR_E6=1;TPCC_TPCC_ESR_E7=1; TPCC_TPCC_ESR_E8=1;TPCC_TPCC_ESR_E9=1;TPCC_TPCC_ESR_E10=1;TPCC_TPCC_ESR_E11=1; TPCC_TPCC_ESR_E12=1;TPCC_TPCC_ESR_E13=1;TPCC_TPCC_ESR_E14=1;TPCC_TPCC_ESR_E15=1; TPCC_TPCC_ESR_E16=1;TPCC_TPCC_ESR_E17=1;TPCC_TPCC_ESR_E18=1;TPCC_TPCC_ESR_E19=1; TPCC_TPCC_ESR_E20=1;TPCC_TPCC_ESR_E21=1;TPCC_TPCC_ESR_E22=1;TPCC_TPCC_ESR_E23=1; TPCC_TPCC_ESR_E24=1;TPCC_TPCC_ESR_E25=1;TPCC_TPCC_ESR_E26=1;TPCC_TPCC_ESR_E27=1; TPCC_TPCC_ESR_E28=1;TPCC_TPCC_ESR_E29=1;TPCC_TPCC_ESR_E30=1;TPCC_TPCC_ESR_E31=1;
TPCC_TPCC_ESRH_E32=1;TPCC_TPCC_ESRH_E33=1;TPCC_TPCC_ESRH_E34=1;TPCC_TPCC_ESRH_E35=1; TPCC_TPCC_ESRH_E36=1;TPCC_TPCC_ESRH_E37=1;TPCC_TPCC_ESRH_E38=1;TPCC_TPCC_ESRH_E39=1; TPCC_TPCC_ESRH_E40=1;TPCC_TPCC_ESRH_E41=1;TPCC_TPCC_ESRH_E42=1;TPCC_TPCC_ESRH_E43=1; TPCC_TPCC_ESRH_E44=1;TPCC_TPCC_ESRH_E45=1;TPCC_TPCC_ESRH_E46=1;TPCC_TPCC_ESRH_E47=1; TPCC_TPCC_ESRH_E48=1;TPCC_TPCC_ESRH_E49=1;TPCC_TPCC_ESRH_E50=1;TPCC_TPCC_ESRH_E51=1; TPCC_TPCC_ESRH_E52=1;TPCC_TPCC_ESRH_E53=1;TPCC_TPCC_ESRH_E54=1;TPCC_TPCC_ESRH_E55=1; TPCC_TPCC_ESRH_E56=1;TPCC_TPCC_ESRH_E57=1;TPCC_TPCC_ESRH_E58=1;TPCC_TPCC_ESRH_E59=1; TPCC_TPCC_ESRH_E60=1;TPCC_TPCC_ESRH_E61=1;TPCC_TPCC_ESRH_E62=1;TPCC_TPCC_ESRH_E63=1;
TPCC_TPCC_ECR_E0=1;TPCC_TPCC_ECR_E1=1;TPCC_TPCC_ECR_E2=1;TPCC_TPCC_ECR_E3=1; TPCC_TPCC_ECR_E4=1;TPCC_TPCC_ECR_E5=1;TPCC_TPCC_ECR_E6=1;TPCC_TPCC_ECR_E7=1; TPCC_TPCC_ECR_E8=1;TPCC_TPCC_ECR_E9=1;TPCC_TPCC_ECR_E10=1;TPCC_TPCC_ECR_E11=1; TPCC_TPCC_ECR_E12=1;TPCC_TPCC_ECR_E13=1;TPCC_TPCC_ECR_E14=1;TPCC_TPCC_ECR_E15=1; TPCC_TPCC_ECR_E16=1;TPCC_TPCC_ECR_E17=1;TPCC_TPCC_ECR_E18=1;TPCC_TPCC_ECR_E19=1; TPCC_TPCC_ECR_E20=1;TPCC_TPCC_ECR_E21=1;TPCC_TPCC_ECR_E22=1;TPCC_TPCC_ECR_E23=1; TPCC_TPCC_ECR_E24=1;TPCC_TPCC_ECR_E25=1;TPCC_TPCC_ECR_E26=1;TPCC_TPCC_ECR_E27=1; TPCC_TPCC_ECR_E28=1;TPCC_TPCC_ECR_E29=1;TPCC_TPCC_ECR_E30=1;TPCC_TPCC_ECR_E31=1;
TPCC_TPCC_ECRH_E32=1;TPCC_TPCC_ECRH_E33=1;TPCC_TPCC_ECRH_E34=1;TPCC_TPCC_ECRH_E35=1; TPCC_TPCC_ECRH_E36=1;TPCC_TPCC_ECRH_E37=1;TPCC_TPCC_ECRH_E38=1;TPCC_TPCC_ECRH_E39=1; TPCC_TPCC_ECRH_E40=1;TPCC_TPCC_ECRH_E41=1;TPCC_TPCC_ECRH_E42=1;TPCC_TPCC_ECRH_E43=1; TPCC_TPCC_ECRH_E44=1;TPCC_TPCC_ECRH_E45=1;TPCC_TPCC_ECRH_E46=1;TPCC_TPCC_ECRH_E47=1; TPCC_TPCC_ECRH_E48=1;TPCC_TPCC_ECRH_E49=1;TPCC_TPCC_ECRH_E50=1;TPCC_TPCC_ECRH_E51=1; TPCC_TPCC_ECRH_E52=1;TPCC_TPCC_ECRH_E53=1;TPCC_TPCC_ECRH_E54=1;TPCC_TPCC_ECRH_E55=1; TPCC_TPCC_ECRH_E56=1;TPCC_TPCC_ECRH_E57=1;TPCC_TPCC_ECRH_E58=1;TPCC_TPCC_ECRH_E59=1; TPCC_TPCC_ECRH_E60=1;TPCC_TPCC_ECRH_E61=1;TPCC_TPCC_ECRH_E62=1;TPCC_TPCC_ECRH_E63=1;
TPCC_TPCC_EMCR_EMCR0;TPCC_TPCC_EMCR_EMCR1;TPCC_TPCC_EMCR_EMCR2; TPCC_TPCC_EMCR_EMCR3;TPCC_TPCC_EMCR_EMCR4;TPCC_TPCC_EMCR_EMCR5; TPCC_TPCC_EMCR_EMCR6;TPCC_TPCC_EMCR_EMCR7;TPCC_TPCC_EMCR_EMCR8; TPCC_TPCC_EMCR_EMCR9;TPCC_TPCC_EMCR_EMCR10;TPCC_TPCC_EMCR_EMCR11; TPCC_TPCC_EMCR_EMCR12;TPCC_TPCC_EMCR_EMCR13;TPCC_TPCC_EMCR_EMCR14; TPCC_TPCC_EMCR_EMCR15;TPCC_TPCC_EMCR_EMCR16;TPCC_TPCC_EMCR_EMCR17; TPCC_TPCC_EMCR_EMCR18;TPCC_TPCC_EMCR_EMCR19;TPCC_TPCC_EMCR_EMCR20; TPCC_TPCC_EMCR_EMCR21;TPCC_TPCC_EMCR_EMCR22;TPCC_TPCC_EMCR_EMCR23; TPCC_TPCC_EMCR_EMCR24;TPCC_TPCC_EMCR_EMCR25;TPCC_TPCC_EMCR_EMCR26; TPCC_TPCC_EMCR_EMCR27;TPCC_TPCC_EMCR_EMCR28;TPCC_TPCC_EMCR_EMCR29; TPCC_TPCC_EMCR_EMCR30;TPCC_TPCC_EMCR_EMCR31;
TPCC_TPCC_EMCRH_EMCR32;TPCC_TPCC_EMCRH_EMCR33;TPCC_TPCC_EMCRH_EMCR34 TPCC_TPCC_EMCRH_EMCR35;TPCC_TPCC_EMCRH_EMCR36;TPCC_TPCC_EMCRH_EMCR37 TPCC_TPCC_EMCRH_EMCR38;TPCC_TPCC_EMCRH_EMCR39;TPCC_TPCC_EMCRH_EMCR40 TPCC_TPCC_EMCRH_EMCR41;TPCC_TPCC_EMCRH_EMCR42;TPCC_TPCC_EMCRH_EMCR43 TPCC_TPCC_EMCRH_EMCR44;TPCC_TPCC_EMCRH_EMCR45;TPCC_TPCC_EMCRH_EMCR46 TPCC_TPCC_EMCRH_EMCR47;TPCC_TPCC_EMCRH_EMCR48;TPCC_TPCC_EMCRH_EMCR49 TPCC_TPCC_EMCRH_EMCR50;TPCC_TPCC_EMCRH_EMCR51;TPCC_TPCC_EMCRH_EMCR52 TPCC_TPCC_EMCRH_EMCR53;TPCC_TPCC_EMCRH_EMCR54;TPCC_TPCC_EMCRH_EMCR55 TPCC_TPCC_EMCRH_EMCR56;TPCC_TPCC_EMCRH_EMCR57;TPCC_TPCC_EMCRH_EMCR58 TPCC_TPCC_EMCRH_EMCR59;TPCC_TPCC_EMCRH_EMCR60;TPCC_TPCC_EMCRH_EMCR61 TPCC_TPCC_EMCRH_EMCR62;TPCC_TPCC_EMCRH_EMCR63,
TPCC_TPCC_SECR_SECR0=1;TPCC_TPCC_SECR_SECR1=1;TPCC_TPCC_SECR_SECR2=1; TPCC_TPCC_SECR_SECR3=1;TPCC_TPCC_SECR_SECR4=1;TPCC_TPCC_SECR_SECR5=1; TPCC_TPCC_SECR_SECR6=1;TPCC_TPCC_SECR_SECR7=1;TPCC_TPCC_SECR_SECR8=1; TPCC_TPCC_SECR_SECR9=1;TPCC_TPCC_SECR_SECR10=1;TPCC_TPCC_SECR_SECR11=1; TPCC_TPCC_SECR_SECR12=1;TPCC_TPCC_SECR_SECR13=1;TPCC_TPCC_SECR_SECR14=1; TPCC_TPCC_SECR_SECR15=1;TPCC_TPCC_SECR_SECR16=1;TPCC_TPCC_SECR_SECR17=1; TPCC_TPCC_SECR_SECR18=1;TPCC_TPCC_SECR_SECR19=1;TPCC_TPCC_SECR_SECR20=1; TPCC_TPCC_SECR_SECR21=1;TPCC_TPCC_SECR_SECR22=1;TPCC_TPCC_SECR_SECR23=1; TPCC_TPCC_SECR_SECR24=1;TPCC_TPCC_SECR_SECR25=1;TPCC_TPCC_SECR_SECR26=1; TPCC_TPCC_SECR_SECR27=1;TPCC_TPCC_SECR_SECR28=1;TPCC_TPCC_SECR_SECR29=1; TPCC_TPCC_SECR_SECR30=1;TPCC_TPCC_SECR_SECR31=1;
TPCC_TPCC_SECRH_SECR32=1;TPCC_TPCC_SECRH_SECR33=1;TPCC_TPCC_SECRH_SECR34=1; TPCC_TPCC_SECRH_SECR35=1;TPCC_TPCC_SECRH_SECR36=1;TPCC_TPCC_SECRH_SECR37=1; TPCC_TPCC_SECRH_SECR38=1;TPCC_TPCC_SECRH_SECR39=1;TPCC_TPCC_SECRH_SECR40=1; TPCC_TPCC_SECRH_SECR41=1;TPCC_TPCC_SECRH_SECR42=1;TPCC_TPCC_SECRH_SECR43=1; TPCC_TPCC_SECRH_SECR44=1;TPCC_TPCC_SECRH_SECR45=1;TPCC_TPCC_SECRH_SECR46=1; TPCC_TPCC_SECRH_SECR47=1;TPCC_TPCC_SECRH_SECR48=1;TPCC_TPCC_SECRH_SECR49=1; TPCC_TPCC_SECRH_SECR50=1;TPCC_TPCC_SECRH_SECR51=1;TPCC_TPCC_SECRH_SECR52=1; TPCC_TPCC_SECRH_SECR53=1;TPCC_TPCC_SECRH_SECR54=1;TPCC_TPCC_SECRH_SECR55=1; TPCC_TPCC_SECRH_SECR56=1;TPCC_TPCC_SECRH_SECR57=1;TPCC_TPCC_SECRH_SECR58=1; TPCC_TPCC_SECRH_SECR59=1;TPCC_TPCC_SECRH_SECR60=1;TPCC_TPCC_SECRH_SECR61=1; TPCC_TPCC_SECRH_SECR62=1;TPCC_TPCC_SECRH_SECR63=1;
TPCC_TPCC_QEMCR_QEMCR0;TPCC_TPCC_QEMCR_QEMCR1;TPCC_TPCC_QEMCR_QEMCR2; TPCC_TPCC_QEMCR_QEMCR3;TPCC_TPCC_QEMCR_QEMCR4;TPCC_TPCC_QEMCR_QEMCR5; TPCC_TPCC_QEMCR_QEMCR6;TPCC_TPCC_QEMCR_QEMCR7,
TPCC_TPCC_QSECR_QSECR0=1;TPCC_TPCC_QSECR_QSECR1=1;TPCC_TPCC_QSECR_QSECR2=1; TPCC_TPCC_QSECR_QSECR3=1;TPCC_TPCC_QSECR_QSECR4=1;TPCC_TPCC_QSECR_QSECR5=1; TPCC_TPCC_QSECR_QSECR6=1;TPCC_TPCC_QSECR_QSECR7=1;

Example

                CSL_Edma3Handle             hModule;
                CSL_Edma3Obj                edmaObj;
                CSL_Edma3ChannelObj         chObj;
                CSL_Edma3ChannelHandle      hChannel;
                CSL_Edma3ChannelAttr        chAttr;
                CSL_Status                  status;

                // Module Initialization
                CSL_edma3Init(NULL);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Channel 0 Open in context of Shadow region 0
                chAttr.regionNum = CSL_EDMA3_REGION_0;
                chAttr.chaNum    = 0;
                hChannel = CSL_edma3ChannelOpen(&chObj, CSL_EDMA3, &chAttr, &status);
                ...
                // Enable Channel
                CSL_edma3HwChannelControl(hChannel,CSL_EDMA3_CMD_CHANNEL_ENABLE,NULL);
                ...

=============================================================================

CSL_Status CSL_edma3HwChannelSetupParam | ( | CSL_Edma3ChannelHandle | hEdma,
|  | Uint16 | paramNum |
| ) |  |  |

============================================================================
CSL_edma3HwChannelSetupParam

Description
The function maps a DMA/QDMA channel to the specific PARAM Entry.

Arguments

                hEdma           Channel Handle
                paramNum        Parameter Entry

Return Value
Success - CSL_SOK
Error - CSL_ESYS_BADHANDLE (The handle passed is invalid)
Error - CSL_ESYS_INVPARAMS (The parameter passed is invalid)

Pre Condition
CSL_edma3Init(), CSL_edma3Open() and CSL_edma3ChannelOpen() must be called successfully in that order before this API can be invoked

Post Condition
Channel is mapped to the PARAM Entry.

Writes
TPCC_TPCC_DCHMAP_PAENTRY;
TPCC_TPCC_QCHMAP_PAENTRY

Example

                CSL_Edma3Handle             hModule;
                CSL_Edma3Obj                edmaObj;
                CSL_Status                  status;
                CSL_Edma3ChannelAttr        chAttr;
                CSL_Edma3ChannelObj         chObj;
                CSL_Edma3ChannelHandle      hChannel;

                // Module Initialization
                CSL_edma3Init(NULL);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Channel 0 Open in context of Shadow region 0
                chAttr.regionNum = CSL_EDMA3_REGION_0;
                chAttr.chaNum    = 0;
                hChannel = CSL_edma3ChannelOpen(&chObj, 0, &chAttr, &status);
                ...
                // Map the channel to PARAM Entry 1
                CSL_edma3HwChannelSetupParam(hChannel, 1);
                ...

=============================================================================

CSL_Status CSL_edma3HwChannelSetupQue | ( | CSL_Edma3ChannelHandle | hEdma,
|  | CSL_Edma3Que | evtQue |
| ) |  |  |

============================================================================
CSL_edma3HwChannelSetupQue

Description
The function maps the DMA/QDMA channels to the specified event queue.

Arguments

                hEdma           Channel Handle
                evtQue          Queue Setup

Return Value
Success - CSL_SOK
Error - CSL_ESYS_BADHANDLE (The handle passed is invalid)

Pre Condition
CSL_edma3Init(), CSL_edma3Open() and CSL_edma3ChannelOpen() must be called successfully in that order before this API can be invoked

Post Condition
Sets up the channel to Queue mapping

Writes
TPCC_TPCC_QDMAQNUM_E0;TPCC_TPCC_QDMAQNUM_E1;TPCC_TPCC_QDMAQNUM_E2; TPCC_TPCC_QDMAQNUM_E3;TPCC_TPCC_QDMAQNUM_E4;TPCC_TPCC_QDMAQNUM_E5; TPCC_TPCC_QDMAQNUM_E6;TPCC_TPCC_QDMAQNUM_E7;
TPCC_TPCC_DMAQNUM_E0;TPCC_TPCC_DMAQNUM_E1;TPCC_TPCC_DMAQNUM_E2; TPCC_TPCC_DMAQNUM_E3;TPCC_TPCC_DMAQNUM_E4;TPCC_TPCC_DMAQNUM_E5; TPCC_TPCC_DMAQNUM_E6;TPCC_TPCC_DMAQNUM_E7

Example

                CSL_Edma3Handle             hModule;
                CSL_Edma3Obj                edmaObj;
                CSL_Status                  status;
                CSL_Edma3ChannelAttr        chAttr;
                CSL_Edma3ChannelObj         chObj;
                CSL_Edma3ChannelHandle      hChannel;

                // Module Initialization
                CSL_edma3Init(NULL);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Channel 1 Open in context of Shadow region 0
                chAttr.regionNum = CSL_EDMA3_REGION_0;
                chAttr.chaNum = 16;
                hChannel = CSL_edma3ChannelOpen(&chObj, 0, &chAttr, &status);
                ...
                // Map the channel 1 to Event Queue 3.
                CSL_edma3HwChannelSetupQue(hChannel,CSL_EDMA3_QUE_3);
                ...

=============================================================================

CSL_Status CSL_edma3HwChannelSetupTriggerWord | ( | CSL_Edma3ChannelHandle | hEdma,
|  | Uint8 | triggerWord |
| ) |  |  |

============================================================================
CSL_edma3HwChannelSetupTriggerWord

Description
The function is used to setup the trigger word for QDMA Channels.

Arguments

                hEdma           Channel Handle
                triggerWord     Trigger Word to be configured.

Return Value
Success - CSL_SOK
Error - CSL_ESYS_BADHANDLE (The handle passed is invalid)
Error - CSL_ESYS_INVPARAMS (The parameter passed is invalid)

Pre Condition
CSL_edma3Init(), CSL_edma3Open() and CSL_edma3ChannelOpen() must be called successfully in that order before this API can be invoked

Post Condition
Sets up the QDMA Channel to trigger Word

Writes
TPCC_TPCC_QCHMAP_TRWORD

Example

                CSL_Edma3Handle             hModule;
                CSL_Edma3Obj                edmaObj;
                CSL_Status                  status;
                CSL_Edma3ChannelAttr        chAttr;
                CSL_Edma3ChannelObj         chObj;
                CSL_Edma3ChannelHandle      hChannel;

                // Module Initialization
                CSL_edma3Init(NULL);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Channel 16 Open in context of Shadow region 0 (This is a QDMA Channel)
                chAttr.regionNum = CSL_EDMA3_REGION_0;
                chAttr.chaNum = 16;
                hChannel = CSL_edma3ChannelOpen(&chObj, 0, &chAttr, &status);
                ...
                // Sets up the QDMA Channel 0 trigger Word to the 3rd trigger word.
                CSL_edma3HwChannelSetupTriggerWord(hChannel,3);
                ...

=============================================================================

CSL_Status CSL_edma3HwControl | ( | CSL_Edma3Handle | hMod,
|  | CSL_Edma3HwControlCmd | cmd,
|  | void * | cmdArg |
| ) |  |  |

============================================================================
CSL_edma3HwControl

Description
This API takes a command with an optional argument and performs the appropriate action. This can be used to perform various operations on the EDMA module.

Arguments

                hMod        EDMA Module Handle
                cmd         Command which needs to be executed.
                cmdArg      Pointer to the argument specific to the command

See also:
  CSL_Edma3HwControlCmd

Return Value
Success - CSL_SOK
Error - CSL_ESYS_BADHANDLE (The handle passed is invalid)
Error - CSL_ESYS_INVCMD (The command passed is invalid)

Pre Condition
Functions CSL_edma3Init(), CSL_edma3Open() must be called successfully in that order before this API can be invoked

Post Condition
EDMA registers are configured according to the command and the command arguments. The command determines which registers are modified.

Writes
TPCC_TPCC_MPPAG;TPCC_TPCC_MPPA;
TPCC_TPCC_MPFCR_MPFCLR=1;
TPCC_TPCC_DRA_DRAE_E0=1;TPCC_TPCC_DRA_DRAE_E1=1;TPCC_TPCC_DRA_DRAE_E2=1; TPCC_TPCC_DRA_DRAE_E3=1;TPCC_TPCC_DRA_DRAE_E4=1;TPCC_TPCC_DRA_DRAE_E5=1; TPCC_TPCC_DRA_DRAE_E6=1;TPCC_TPCC_DRA_DRAE_E7=1;TPCC_TPCC_DRA_DRAE_E8=1; TPCC_TPCC_DRA_DRAE_E9=1;TPCC_TPCC_DRA_DRAE_E10=1;TPCC_TPCC_DRA_DRAE_E11=1; TPCC_TPCC_DRA_DRAE_E12=1;TPCC_TPCC_DRA_DRAE_E13=1;TPCC_TPCC_DRA_DRAE_E14=1; TPCC_TPCC_DRA_DRAE_E15=1;TPCC_TPCC_DRA_DRAE_E16=1;TPCC_TPCC_DRA_DRAE_E17=1; TPCC_TPCC_DRA_DRAE_E18=1;TPCC_TPCC_DRA_DRAE_E19=1;TPCC_TPCC_DRA_DRAE_E20=1; TPCC_TPCC_DRA_DRAE_E21=1;TPCC_TPCC_DRA_DRAE_E22=1;TPCC_TPCC_DRA_DRAE_E23=1; TPCC_TPCC_DRA_DRAE_E24=1;TPCC_TPCC_DRA_DRAE_E25=1;TPCC_TPCC_DRA_DRAE_E26=1; TPCC_TPCC_DRA_DRAE_E27=1;TPCC_TPCC_DRA_DRAE_E28=1;TPCC_TPCC_DRA_DRAE_E29=1; TPCC_TPCC_DRA_DRAE_E30=1;TPCC_TPCC_DRA_DRAE_E31=1;
TPCC_TPCC_DRA_DRAEH_E32=1;TPCC_TPCC_DRA_DRAEH_E33=1;TPCC_TPCC_DRA_DRAEH_E34=1; TPCC_TPCC_DRA_DRAEH_E35=1;TPCC_TPCC_DRA_DRAEH_E36=1;TPCC_TPCC_DRA_DRAEH_E37=1; TPCC_TPCC_DRA_DRAEH_E38=1;TPCC_TPCC_DRA_DRAEH_E39=1;TPCC_TPCC_DRA_DRAEH_E40=1; TPCC_TPCC_DRA_DRAEH_E41=1;TPCC_TPCC_DRA_DRAEH_E42=1;TPCC_TPCC_DRA_DRAEH_E43=1; TPCC_TPCC_DRA_DRAEH_E44=1;TPCC_TPCC_DRA_DRAEH_E45=1;TPCC_TPCC_DRA_DRAEH_E46=1; TPCC_TPCC_DRA_DRAEH_E47=1;TPCC_TPCC_DRA_DRAEH_E48=1;TPCC_TPCC_DRA_DRAEH_E49=1; TPCC_TPCC_DRA_DRAEH_E50=1;TPCC_TPCC_DRA_DRAEH_E51=1;TPCC_TPCC_DRA_DRAEH_E52=1; TPCC_TPCC_DRA_DRAEH_E53=1;TPCC_TPCC_DRA_DRAEH_E54=1;TPCC_TPCC_DRA_DRAEH_E55=1; TPCC_TPCC_DRA_DRAEH_E56=1;TPCC_TPCC_DRA_DRAEH_E57=1;TPCC_TPCC_DRA_DRAEH_E58=1; TPCC_TPCC_DRA_DRAEH_E59=1;TPCC_TPCC_DRA_DRAEH_E60=1;TPCC_TPCC_DRA_DRAEH_E61=1; TPCC_TPCC_DRA_DRAEH_E62=1;TPCC_TPCC_DRA_DRAEH_E63=1;
TPCC_TPCC_DRA_DRAE_E0=0;TPCC_TPCC_DRA_DRAE_E1=0;TPCC_TPCC_DRA_DRAE_E2=0; TPCC_TPCC_DRA_DRAE_E3=0;TPCC_TPCC_DRA_DRAE_E4=0;TPCC_TPCC_DRA_DRAE_E5=0; TPCC_TPCC_DRA_DRAE_E6=0;TPCC_TPCC_DRA_DRAE_E7=0;TPCC_TPCC_DRA_DRAE_E8=0; TPCC_TPCC_DRA_DRAE_E9=0;TPCC_TPCC_DRA_DRAE_E10=0;TPCC_TPCC_DRA_DRAE_E11=0; TPCC_TPCC_DRA_DRAE_E12=0;TPCC_TPCC_DRA_DRAE_E13=0;TPCC_TPCC_DRA_DRAE_E14=0; TPCC_TPCC_DRA_DRAE_E15=0;TPCC_TPCC_DRA_DRAE_E16=0;TPCC_TPCC_DRA_DRAE_E17=0; TPCC_TPCC_DRA_DRAE_E18=0;TPCC_TPCC_DRA_DRAE_E19=0;TPCC_TPCC_DRA_DRAE_E20=0; TPCC_TPCC_DRA_DRAE_E21=0;TPCC_TPCC_DRA_DRAE_E22=0;TPCC_TPCC_DRA_DRAE_E23=0; TPCC_TPCC_DRA_DRAE_E24=0;TPCC_TPCC_DRA_DRAE_E25=0;TPCC_TPCC_DRA_DRAE_E26=0; TPCC_TPCC_DRA_DRAE_E27=0;TPCC_TPCC_DRA_DRAE_E28=0;TPCC_TPCC_DRA_DRAE_E29=0; TPCC_TPCC_DRA_DRAE_E30=0;TPCC_TPCC_DRA_DRAE_E31=0;
TPCC_TPCC_DRA_DRAEH_E32=0;TPCC_TPCC_DRA_DRAEH_E33=0;TPCC_TPCC_DRA_DRAEH_E34=0; TPCC_TPCC_DRA_DRAEH_E35=0;TPCC_TPCC_DRA_DRAEH_E36=0;TPCC_TPCC_DRA_DRAEH_E37=0; TPCC_TPCC_DRA_DRAEH_E38=0;TPCC_TPCC_DRA_DRAEH_E39=0;TPCC_TPCC_DRA_DRAEH_E40=0; TPCC_TPCC_DRA_DRAEH_E41=0;TPCC_TPCC_DRA_DRAEH_E42=0;TPCC_TPCC_DRA_DRAEH_E43=0; TPCC_TPCC_DRA_DRAEH_E44=0;TPCC_TPCC_DRA_DRAEH_E45=0;TPCC_TPCC_DRA_DRAEH_E46=0; TPCC_TPCC_DRA_DRAEH_E47=0;TPCC_TPCC_DRA_DRAEH_E48=0;TPCC_TPCC_DRA_DRAEH_E49=0; TPCC_TPCC_DRA_DRAEH_E50=0;TPCC_TPCC_DRA_DRAEH_E51=0;TPCC_TPCC_DRA_DRAEH_E52=0; TPCC_TPCC_DRA_DRAEH_E53=0;TPCC_TPCC_DRA_DRAEH_E54=0;TPCC_TPCC_DRA_DRAEH_E55=0; TPCC_TPCC_DRA_DRAEH_E56=0;TPCC_TPCC_DRA_DRAEH_E57=0;TPCC_TPCC_DRA_DRAEH_E58=0; TPCC_TPCC_DRA_DRAEH_E59=0;TPCC_TPCC_DRA_DRAEH_E60=0;TPCC_TPCC_DRA_DRAEH_E61=0; TPCC_TPCC_DRA_DRAEH_E62=0;TPCC_TPCC_DRA_DRAEH_E63=0;
TPCC_TPCC_QRAE_E0=1;TPCC_TPCC_QRAE_E1=1;TPCC_TPCC_QRAE_E2=1; TPCC_TPCC_QRAE_E3=1;TPCC_TPCC_QRAE_E4=1;TPCC_TPCC_QRAE_E5=1; TPCC_TPCC_QRAE_E6=1;TPCC_TPCC_QRAE_E7=1;
TPCC_TPCC_QRAE_E0=0;TPCC_TPCC_QRAE_E1=0;TPCC_TPCC_QRAE_E2=0; TPCC_TPCC_QRAE_E3=0;TPCC_TPCC_QRAE_E4=0;TPCC_TPCC_QRAE_E5=0; TPCC_TPCC_QRAE_E6=0;TPCC_TPCC_QRAE_E7=0;
TPCC_TPCC_QUEPRI_PRIQ0;TPCC_TPCC_QUEPRI_PRIQ1;TPCC_TPCC_QUEPRI_PRIQ2; TPCC_TPCC_QUEPRI_PRIQ3;TPCC_TPCC_QUEPRI_PRIQ4;TPCC_TPCC_QUEPRI_PRIQ5; TPCC_TPCC_QUEPRI_PRIQ6;TPCC_TPCC_QUEPRI_PRIQ7;
TPCC_TPCC_QWMTHRA_Q0;TPCC_TPCC_QWMTHRA_Q1;TPCC_TPCC_QWMTHRA_Q2; TPCC_TPCC_QWMTHRA_Q3;
TPCC_TPCC_QWMTHRB_Q4;TPCC_TPCC_QWMTHRB_Q1;TPCC_TPCC_QWMTHRB_Q2; TPCC_TPCC_QWMTHRB_Q3;
TPCC_TPCC_EEVAL_EVAL=1;
TPCC_TPCC_ICR,TPCC_TPCC_ICRH;
TPCC_TPCC_IESR_IESR0=1;TPCC_TPCC_IESR_IESR1=1;TPCC_TPCC_IESR_IESR2=1; TPCC_TPCC_IESR_IESR3=1;TPCC_TPCC_IESR_IESR4=1;TPCC_TPCC_IESR_IESR5=1; TPCC_TPCC_IESR_IESR6=1;TPCC_TPCC_IESR_IESR7=1;TPCC_TPCC_IESR_IESR8=1; TPCC_TPCC_IESR_IESR9=1;TPCC_TPCC_IESR_IESR10=1;TPCC_TPCC_IESR_IESR11=1; TPCC_TPCC_IESR_IESR12=1;TPCC_TPCC_IESR_IESR13=1;TPCC_TPCC_IESR_IESR14=1; TPCC_TPCC_IESR_IESR15=1;TPCC_TPCC_IESR_IESR16=1;TPCC_TPCC_IESR_IESR17=1; TPCC_TPCC_IESR_IESR18=1;TPCC_TPCC_IESR_IESR19=1;TPCC_TPCC_IESR_IESR20=1; TPCC_TPCC_IESR_IESR21=1;TPCC_TPCC_IESR_IESR22=1;TPCC_TPCC_IESR_IESR23=1; TPCC_TPCC_IESR_IESR24=1;TPCC_TPCC_IESR_IESR25=1;TPCC_TPCC_IESR_IESR26=1; TPCC_TPCC_IESR_IESR27=1;TPCC_TPCC_IESR_IESR28=1;TPCC_TPCC_IESR_IESR29=1; TPCC_TPCC_IESR_IESR30=1;TPCC_TPCC_IESR_IESR31=1;
TPCC_TPCC_IESRH_IESR32=1;TPCC_TPCC_IESRH_IESR33=1;TPCC_TPCC_IESRH_IESR34=1; TPCC_TPCC_IESRH_IESR35=1;TPCC_TPCC_IESRH_IESR36=1;TPCC_TPCC_IESRH_IESR37=1; TPCC_TPCC_IESRH_IESR38=1;TPCC_TPCC_IESRH_IESR39=1;TPCC_TPCC_IESRH_IESR40=1; TPCC_TPCC_IESRH_IESR41=1;TPCC_TPCC_IESRH_IESR42=1;TPCC_TPCC_IESRH_IESR43=1; TPCC_TPCC_IESRH_IESR44=1;TPCC_TPCC_IESRH_IESR45=1;TPCC_TPCC_IESRH_IESR46=1; TPCC_TPCC_IESRH_IESR47=1;TPCC_TPCC_IESRH_IESR48=1;TPCC_TPCC_IESRH_IESR49=1; TPCC_TPCC_IESRH_IESR50=1;TPCC_TPCC_IESRH_IESR51=1;TPCC_TPCC_IESRH_IESR52=1; TPCC_TPCC_IESRH_IESR53=1;TPCC_TPCC_IESRH_IESR54=1;TPCC_TPCC_IESRH_IESR55=1; TPCC_TPCC_IESRH_IESR56=1;TPCC_TPCC_IESRH_IESR57=1;TPCC_TPCC_IESRH_IESR58=1; TPCC_TPCC_IESRH_IESR59=1;TPCC_TPCC_IESRH_IESR60=1;TPCC_TPCC_IESRH_IESR61=1; TPCC_TPCC_IESRH_IESR62=1;TPCC_TPCC_IESRH_IESR63=1;
TPCC_TPCC_IECR_IECR0=1;TPCC_TPCC_IECR_IECR1=1;TPCC_TPCC_IECR_IECR2=1; TPCC_TPCC_IECR_IECR3=1;TPCC_TPCC_IECR_IECR4=1;TPCC_TPCC_IECR_IECR5=1; TPCC_TPCC_IECR_IECR6=1;TPCC_TPCC_IECR_IECR7=1;TPCC_TPCC_IECR_IECR8=1; TPCC_TPCC_IECR_IECR9=1;TPCC_TPCC_IECR_IECR10=1;TPCC_TPCC_IECR_IECR11=1; TPCC_TPCC_IECR_IECR12=1;TPCC_TPCC_IECR_IECR13=1;TPCC_TPCC_IECR_IECR14=1; TPCC_TPCC_IECR_IECR15=1;TPCC_TPCC_IECR_IECR16=1;TPCC_TPCC_IECR_IECR17=1; TPCC_TPCC_IECR_IECR18=1;TPCC_TPCC_IECR_IECR19=1;TPCC_TPCC_IECR_IECR20=1; TPCC_TPCC_IECR_IECR21=1;TPCC_TPCC_IECR_IECR22=1;TPCC_TPCC_IECR_IECR23=1; TPCC_TPCC_IECR_IECR24=1;TPCC_TPCC_IECR_IECR25=1;TPCC_TPCC_IECR_IECR26=1; TPCC_TPCC_IECR_IECR27=1;TPCC_TPCC_IECR_IECR28=1;TPCC_TPCC_IECR_IECR29=1; TPCC_TPCC_IECR_IECR30=1;TPCC_TPCC_IECR_IECR31=1;
TPCC_TPCC_IECRH_IECR32=1;TPCC_TPCC_IECRH_IECR33=1;TPCC_TPCC_IECRH_IECR34=1; TPCC_TPCC_IECRH_IECR35=1;TPCC_TPCC_IECRH_IECR36=1;TPCC_TPCC_IECRH_IECR37=1; TPCC_TPCC_IECRH_IECR38=1;TPCC_TPCC_IECRH_IECR39=1;TPCC_TPCC_IECRH_IECR40=1; TPCC_TPCC_IECRH_IECR41=1;TPCC_TPCC_IECRH_IECR42=1;TPCC_TPCC_IECRH_IECR43=1; TPCC_TPCC_IECRH_IECR44=1;TPCC_TPCC_IECRH_IECR45=1;TPCC_TPCC_IECRH_IECR46=1; TPCC_TPCC_IECRH_IECR47=1;TPCC_TPCC_IECRH_IECR48=1;TPCC_TPCC_IECRH_IECR49=1; TPCC_TPCC_IECRH_IECR50=1;TPCC_TPCC_IECRH_IECR51=1;TPCC_TPCC_IECRH_IECR52=1; TPCC_TPCC_IECRH_IECR53=1;TPCC_TPCC_IECRH_IECR54=1;TPCC_TPCC_IECRH_IECR55=1; TPCC_TPCC_IECRH_IECR56=1;TPCC_TPCC_IECRH_IECR57=1;TPCC_TPCC_IECRH_IECR58=1; TPCC_TPCC_IECRH_IECR59=1;TPCC_TPCC_IECRH_IECR60=1;TPCC_TPCC_IECRH_IECR61=1; TPCC_TPCC_IECRH_IECR62=1;TPCC_TPCC_IECRH_IECR63=1;
TPCC_TPCC_IEVAL_EVAL=1;
TPCC_TPCC_CCERRCLR_QTHRXD0;TPCC_TPCC_CCERRCLR_QTHRXD1;TPCC_TPCC_CCERRCLR_QTHRXD2; TPCC_TPCC_CCERRCLR_QTHRXD3;TPCC_TPCC_CCERRCLR_QTHRXD4;TPCC_TPCC_CCERRCLR_QTHRXD5; TPCC_TPCC_CCERRCLR_QTHRXD6;TPCC_TPCC_CCERRCLR_QTHRXD7, TPCC_TPCC_CCERR_TCCERR;
TPCC_TPCC_EMCR,TPCC_TPCC_EMCRH,TPCC_TPCC_QEMCR

Example

                CSL_Edma3Handle             hModule;
                CSL_Edma3Obj                edmaObj;
                CSL_Status                  status;
                CSL_Edma3CmdDrae            regionAccess;

                // Module Initialization
                CSL_edma3Init(NULL);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // DRAE Enable(Bits 0-15) for the Shadow Region 0.
                regionAccess.region = CSL_EDMA3_REGION_0 ;
                regionAccess.drae =   0xFFFF ;
                regionAccess.draeh =  0x0000 ;
                CSL_edma3HwControl(hModule,CSL_EDMA3_CMD_DMAREGION_ENABLE, &regionAccess);
                ...

=============================================================================

CSL_Status CSL_edma3HwSetup | ( | CSL_Edma3Handle | hMod,
|  | CSL_Edma3HwSetup * | setup |
| ) |  |  |

============================================================================
CSL_edma3HwSetup

Description
This function does the setup for all DMA/QDMA channels by doing the following operations:-

- Mapping DMA/QDMA Channels to PARAM Blocks.
- Mapping DMA/QDMA Channels to Event Queues.
- Setting up the trigger word for QDMA channels.

Arguments

                hMod            Edma module Handle
                setup           Pointer to the setup structure

Return Value CSL_Status
Success - CSL_SOK
Error - CSL_ESYS_BADHANDLE (The handle passed is invalid)
Error - CSL_ESYS_INVPARAMS (The parameter passed is invalid)

See also:
  CSL_Edma3HwSetup

Pre Condition
CSL_edma3Init(), CSL_edma3Open() must be called successfully in that order before this API can be invoked

Post Condition
EDMA registers are configured according to the hardware setup parameters

Writes
TPCC_TPCC_DCHMAP_PAENTRY,
TPCC_TPCC_DMAQNUM_E0;TPCC_TPCC_DMAQNUM_E1;TPCC_TPCC_DMAQNUM_E2; TPCC_TPCC_DMAQNUM_E3;TPCC_TPCC_DMAQNUM_E4;TPCC_TPCC_DMAQNUM_E5; TPCC_TPCC_DMAQNUM_E6;TPCC_TPCC_DMAQNUM_E7;
TPCC_TPCC_QCHMAP_PAENTRY,
TPCC_TPCC_QCHMAP_TRWORD,
TPCC_TPCC_QDMAQNUM_E0;TPCC_TPCC_QDMAQNUM_E1;TPCC_TPCC_QDMAQNUM_E2; TPCC_TPCC_QDMAQNUM_E3;TPCC_TPCC_QDMAQNUM_E4;TPCC_TPCC_QDMAQNUM_E5; TPCC_TPCC_QDMAQNUM_E6;TPCC_TPCC_QDMAQNUM_E7

Example

                CSL_Edma3Handle             hModule;
                CSL_Edma3Obj                edmaObj;
                CSL_Status                  status;
                CSL_Edma3HwSetup            hwSetup;
                CSL_Edma3HwDmaChannelSetup  dmahwSetup[64];
                CSL_Edma3HwQdmaChannelSetup qdmahwSetup[8];

                // Module Initialization
                CSL_edma3Init(NULL);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Module Setup
                hwSetup.dmaChaSetup  = &dmahwSetup[0];
                hwSetup.qdmaChaSetup = &qdmaSetup[0];
                CSL_edma3HwSetup(hModule,&hwSetup);
                ...

=============================================================================

CSL_Status CSL_edma3Init | ( | CSL_Edma3Context * | pContext | ) |

============================================================================
CSL_edma3Init

Description
This is the initialization function for the EDMA CSL. The function must be called before calling any other API from this CSL.This function is idem-potent. Currently, the function just return status CSL_SOK, without doing anything.

Arguments

                pContext    Pointer to module-context. As EDMA doesn't have
                            any context based information user is expected
                            to pass NULL.

Return Value
Always returns CSL_SOK

Pre Condition
None

Post Condition
The CSL for EDMA is initialized

Affects
None

Example

                // Initialize the EDMA3 Module.
                CSL_edma3Init(NULL);
                ...
                // All EDMA Functions should follow this.
                ...

=============================================================================

CSL_IDEF_INLINE void CSL_edma3InterruptEval | ( | CSL_Edma3Handle | hModule,
|  | Int | region |
| ) |  |  |

============================================================================
CSL_edma3InterruptEval

Description
The API is used to set the EVAL bit which will cause an interrupt to be generated if any enabled interrupts are still pending.

Arguments

            hModule           Module Handle
            region            Region (Shadown Region or Global)

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_IEVAL_EVAL=1

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                CSL_BitMask32           edmaIntrLo;
                CSL_BitMask32           edmaIntrHi;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Interrupt Evaluate for Global Region.
                status = CSL_edma3InterruptEval(hModule, CSL_EDMA3_REGION_GLOBAL);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3InterruptHiDisable | ( | CSL_Edma3Handle | hModule,
|  | Int | region,
|  | CSL_BitMask32 | intrHi |
| ) |  |  |

============================================================================
CSL_edma3InterruptHiDisable

Description
The API disables the specified high interrupt Number.

Arguments

            hModule           Module Handle
            region            Region (Shadow or Global)
            intrHi            Interrupt 32-63 (BitMask32) to be disabled

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_IECRH_IECR32=1;TPCC_TPCC_IECRH_IECR33=1;TPCC_TPCC_IECRH_IECR34=1; TPCC_TPCC_IECRH_IECR35=1;TPCC_TPCC_IECRH_IECR36=1;TPCC_TPCC_IECRH_IECR37=1; TPCC_TPCC_IECRH_IECR38=1;TPCC_TPCC_IECRH_IECR39=1;TPCC_TPCC_IECRH_IECR40=1; TPCC_TPCC_IECRH_IECR41=1;TPCC_TPCC_IECRH_IECR42=1;TPCC_TPCC_IECRH_IECR43=1; TPCC_TPCC_IECRH_IECR44=1;TPCC_TPCC_IECRH_IECR45=1;TPCC_TPCC_IECRH_IECR46=1; TPCC_TPCC_IECRH_IECR47=1;TPCC_TPCC_IECRH_IECR48=1;TPCC_TPCC_IECRH_IECR49=1; TPCC_TPCC_IECRH_IECR50=1;TPCC_TPCC_IECRH_IECR51=1;TPCC_TPCC_IECRH_IECR52=1; TPCC_TPCC_IECRH_IECR53=1;TPCC_TPCC_IECRH_IECR54=1;TPCC_TPCC_IECRH_IECR55=1; TPCC_TPCC_IECRH_IECR56=1;TPCC_TPCC_IECRH_IECR57=1;TPCC_TPCC_IECRH_IECR58=1; TPCC_TPCC_IECRH_IECR59=1;TPCC_TPCC_IECRH_IECR60=1;TPCC_TPCC_IECRH_IECR61=1; TPCC_TPCC_IECRH_IECR62=1;TPCC_TPCC_IECRH_IECR63=1;

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Interrupts 32 disabled for Global Region.
                CSL_edma3InterruptHiDisable(hModule, CSL_EDMA3_REGION_GLOBAL, 0x1);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3InterruptHiEnable | ( | CSL_Edma3Handle | hModule,
|  | Int | region,
|  | CSL_BitMask32 | intrHi |
| ) |  |  |

============================================================================
CSL_edma3InterruptHiEnable

Description
The API enables the specific High interrupt.

Arguments

            hModule          Module Handle
            region           Region (Shadow or Global)
            intrHi           Interrupt 32-63 (BitMask32) to be enabled

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_IESRH_IESR32=1;TPCC_TPCC_IESRH_IESR33=1;TPCC_TPCC_IESRH_IESR34=1; TPCC_TPCC_IESRH_IESR35=1;TPCC_TPCC_IESRH_IESR36=1;TPCC_TPCC_IESRH_IESR37=1; TPCC_TPCC_IESRH_IESR38=1;TPCC_TPCC_IESRH_IESR39=1;TPCC_TPCC_IESRH_IESR40=1; TPCC_TPCC_IESRH_IESR41=1;TPCC_TPCC_IESRH_IESR42=1;TPCC_TPCC_IESRH_IESR43=1; TPCC_TPCC_IESRH_IESR44=1;TPCC_TPCC_IESRH_IESR45=1;TPCC_TPCC_IESRH_IESR46=1; TPCC_TPCC_IESRH_IESR47=1;TPCC_TPCC_IESRH_IESR48=1;TPCC_TPCC_IESRH_IESR49=1; TPCC_TPCC_IESRH_IESR50=1;TPCC_TPCC_IESRH_IESR51=1;TPCC_TPCC_IESRH_IESR52=1; TPCC_TPCC_IESRH_IESR53=1;TPCC_TPCC_IESRH_IESR54=1;TPCC_TPCC_IESRH_IESR55=1; TPCC_TPCC_IESRH_IESR56=1;TPCC_TPCC_IESRH_IESR57=1;TPCC_TPCC_IESRH_IESR58=1; TPCC_TPCC_IESRH_IESR59=1;TPCC_TPCC_IESRH_IESR60=1;TPCC_TPCC_IESRH_IESR61=1; TPCC_TPCC_IESRH_IESR62=1;TPCC_TPCC_IESRH_IESR63=1;

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Interrupts 32 enabled for the global region.
                CSL_edma3InterruptHiEnable(hModule,CSL_EDMA3_REGION_GLOBAL, 0x1);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3InterruptLoDisable | ( | CSL_Edma3Handle | hModule,
|  | Int | region,
|  | CSL_BitMask32 | intrLo |
| ) |  |  |

============================================================================
CSL_edma3InterruptLoDisable

Description
The API disables the specified low interrupt Number.

Arguments

            hModule           Module Handle
            region            Region (Shadow or Global)
            intrLo            Interrupt 0-31 (BitMask32) to be disabled

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_IECR_IECR0=1;TPCC_TPCC_IECR_IECR1=1;TPCC_TPCC_IECR_IECR2=1; TPCC_TPCC_IECR_IECR3=1;TPCC_TPCC_IECR_IECR4=1;TPCC_TPCC_IECR_IECR5=1; TPCC_TPCC_IECR_IECR6=1;TPCC_TPCC_IECR_IECR7=1;TPCC_TPCC_IECR_IECR8=1; TPCC_TPCC_IECR_IECR9=1;TPCC_TPCC_IECR_IECR10=1;TPCC_TPCC_IECR_IECR11=1; TPCC_TPCC_IECR_IECR12=1;TPCC_TPCC_IECR_IECR13=1;TPCC_TPCC_IECR_IECR14=1; TPCC_TPCC_IECR_IECR15=1;TPCC_TPCC_IECR_IECR16=1;TPCC_TPCC_IECR_IECR17=1; TPCC_TPCC_IECR_IECR18=1;TPCC_TPCC_IECR_IECR19=1;TPCC_TPCC_IECR_IECR20=1; TPCC_TPCC_IECR_IECR21=1;TPCC_TPCC_IECR_IECR22=1;TPCC_TPCC_IECR_IECR23=1; TPCC_TPCC_IECR_IECR24=1;TPCC_TPCC_IECR_IECR25=1;TPCC_TPCC_IECR_IECR26=1; TPCC_TPCC_IECR_IECR27=1;TPCC_TPCC_IECR_IECR28=1;TPCC_TPCC_IECR_IECR29=1; TPCC_TPCC_IECR_IECR30=1;TPCC_TPCC_IECR_IECR31=1;

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Interrupts 5-7 disabled for Global Region.
                CSL_edma3InterruptLoDisable(hModule, CSL_EDMA3_REGION_GLOBAL, 0x000000E0);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3InterruptLoEnable | ( | CSL_Edma3Handle | hModule,
|  | Int | region,
|  | CSL_BitMask32 | intrLo |
| ) |  |  |

============================================================================
CSL_edma3InterruptLoEnable

Description
The API enables the specific lower interrupts

Arguments

            hModule          Module Handle
            region           Region (Shadow or Global)
            intrLo           Interrupt 0-31 (BitMask32) to be enabled

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_IESR_IESR0=1;TPCC_TPCC_IESR_IESR1=1;TPCC_TPCC_IESR_IESR2=1; TPCC_TPCC_IESR_IESR3=1;TPCC_TPCC_IESR_IESR4=1;TPCC_TPCC_IESR_IESR5=1; TPCC_TPCC_IESR_IESR6=1;TPCC_TPCC_IESR_IESR7=1;TPCC_TPCC_IESR_IESR8=1; TPCC_TPCC_IESR_IESR9=1;TPCC_TPCC_IESR_IESR10=1;TPCC_TPCC_IESR_IESR11=1; TPCC_TPCC_IESR_IESR12=1;TPCC_TPCC_IESR_IESR13=1;TPCC_TPCC_IESR_IESR14=1; TPCC_TPCC_IESR_IESR15=1;TPCC_TPCC_IESR_IESR16=1;TPCC_TPCC_IESR_IESR17=1; TPCC_TPCC_IESR_IESR18=1;TPCC_TPCC_IESR_IESR19=1;TPCC_TPCC_IESR_IESR20=1; TPCC_TPCC_IESR_IESR21=1;TPCC_TPCC_IESR_IESR22=1;TPCC_TPCC_IESR_IESR23=1; TPCC_TPCC_IESR_IESR24=1;TPCC_TPCC_IESR_IESR25=1;TPCC_TPCC_IESR_IESR26=1; TPCC_TPCC_IESR_IESR27=1;TPCC_TPCC_IESR_IESR28=1;TPCC_TPCC_IESR_IESR29=1; TPCC_TPCC_IESR_IESR30=1;TPCC_TPCC_IESR_IESR31=1;

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Interrupts 5-7 enabled for the global region.
                CSL_edma3InterruptLoEnable(hModule,CSL_EDMA3_REGION_GLOBAL, 0x000000E0);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3IsDMAChannelEventPending | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | dmaChannel,
|  | Bool * | response |
| ) |  |  |

============================================================================
CSL_edma3IsDMAChannelEventPending

Description
The function gets the status of the specified DMA channel i.e. if there is a pending event on the specific channel.

Arguments

            hModule         Module Handle
            dmaChannel      DMA Channel for which status is being inquired.
            response        Place holder for whether an event is set(TRUE) or not (FALSE)

Return Value
None.

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_ER_E0;TPCC_TPCC_ER_E1;TPCC_TPCC_ER_E2;TPCC_TPCC_ER_E3; TPCC_TPCC_ER_E4;TPCC_TPCC_ER_E5;TPCC_TPCC_ER_E6;TPCC_TPCC_ER_E7; TPCC_TPCC_ER_E8;TPCC_TPCC_ER_E9;TPCC_TPCC_ER_E10;TPCC_TPCC_ER_E11; TPCC_TPCC_ER_E12;TPCC_TPCC_ER_E13;TPCC_TPCC_ER_E14;TPCC_TPCC_ER_E15; TPCC_TPCC_ER_E16;TPCC_TPCC_ER_E17;TPCC_TPCC_ER_E18;TPCC_TPCC_ER_E19; TPCC_TPCC_ER_E20;TPCC_TPCC_ER_E21;TPCC_TPCC_ER_E22;TPCC_TPCC_ER_E23; TPCC_TPCC_ER_E24;TPCC_TPCC_ER_E25;TPCC_TPCC_ER_E26;TPCC_TPCC_ER_E27; TPCC_TPCC_ER_E28;TPCC_TPCC_ER_E29;TPCC_TPCC_ER_E30;TPCC_TPCC_ER_E31;
TPCC_TPCC_ERH_E32;TPCC_TPCC_ERH_E33;TPCC_TPCC_ERH_E34;TPCC_TPCC_ERH_E35; TPCC_TPCC_ERH_E36;TPCC_TPCC_ERH_E37;TPCC_TPCC_ERH_E38;TPCC_TPCC_ERH_E39; TPCC_TPCC_ERH_E40;TPCC_TPCC_ERH_E41;TPCC_TPCC_ERH_E42;TPCC_TPCC_ERH_E43; TPCC_TPCC_ERH_E44;TPCC_TPCC_ERH_E45;TPCC_TPCC_ERH_E46;TPCC_TPCC_ERH_E47; TPCC_TPCC_ERH_E48;TPCC_TPCC_ERH_E49;TPCC_TPCC_ERH_E50;TPCC_TPCC_ERH_E51; TPCC_TPCC_ERH_E52;TPCC_TPCC_ERH_E53;TPCC_TPCC_ERH_E54;TPCC_TPCC_ERH_E55; TPCC_TPCC_ERH_E56;TPCC_TPCC_ERH_E57;TPCC_TPCC_ERH_E58;TPCC_TPCC_ERH_E59; TPCC_TPCC_ERH_E60;TPCC_TPCC_ERH_E61;TPCC_TPCC_ERH_E62;TPCC_TPCC_ERH_E63;

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                Bool                    dmaStatus;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Determine if there is an event pending on DMA Channel 0.
                CSL_edma3IsDMAChannelEventPending(hModule, 0, &dmaStatus);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3IsDMAChannelMissedEventSet | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | dmaChannel,
|  | Bool * | response |
| ) |  |  |

============================================================================
CSL_edma3IsDMAChannelMissedEventSet

Description
The API checks determines if there is a missed Event for a specific DMA channel

Arguments

            hModule         Module Handle
            dmaChannel      DMA Channel to be checked
            response        This is populated by the API and returns TRUE if the
                            event was missed else it returns FALSE.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_EMR_EMR0;TPCC_TPCC_EMR_EMR1;TPCC_TPCC_EMR_EMR2; TPCC_TPCC_EMR_EMR3;TPCC_TPCC_EMR_EMR4;TPCC_TPCC_EMR_EMR5; TPCC_TPCC_EMR_EMR6;TPCC_TPCC_EMR_EMR7;TPCC_TPCC_EMR_EMR8; TPCC_TPCC_EMR_EMR9;TPCC_TPCC_EMR_EMR10;TPCC_TPCC_EMR_EMR11; TPCC_TPCC_EMR_EMR12;TPCC_TPCC_EMR_EMR13;TPCC_TPCC_EMR_EMR14; TPCC_TPCC_EMR_EMR15;TPCC_TPCC_EMR_EMR16;TPCC_TPCC_EMR_EMR17; TPCC_TPCC_EMR_EMR18;TPCC_TPCC_EMR_EMR19;TPCC_TPCC_EMR_EMR20; TPCC_TPCC_EMR_EMR21;TPCC_TPCC_EMR_EMR22;TPCC_TPCC_EMR_EMR23; TPCC_TPCC_EMR_EMR24;TPCC_TPCC_EMR_EMR25;TPCC_TPCC_EMR_EMR26; TPCC_TPCC_EMR_EMR27;TPCC_TPCC_EMR_EMR28;TPCC_TPCC_EMR_EMR29; TPCC_TPCC_EMR_EMR30;TPCC_TPCC_EMR_EMR31; TPCC_TPCC_EMRH_EMR32;TPCC_TPCC_EMRH_EMR33;TPCC_TPCC_EMRH_EMR34; TPCC_TPCC_EMRH_EMR35;TPCC_TPCC_EMRH_EMR36;TPCC_TPCC_EMRH_EMR37; TPCC_TPCC_EMRH_EMR38;TPCC_TPCC_EMRH_EMR39;TPCC_TPCC_EMRH_EMR40; TPCC_TPCC_EMRH_EMR41;TPCC_TPCC_EMRH_EMR42;TPCC_TPCC_EMRH_EMR43; TPCC_TPCC_EMRH_EMR44;TPCC_TPCC_EMRH_EMR45;TPCC_TPCC_EMRH_EMR46; TPCC_TPCC_EMRH_EMR47;TPCC_TPCC_EMRH_EMR48;TPCC_TPCC_EMRH_EMR49; TPCC_TPCC_EMRH_EMR50;TPCC_TPCC_EMRH_EMR51;TPCC_TPCC_EMRH_EMR52; TPCC_TPCC_EMRH_EMR53;TPCC_TPCC_EMRH_EMR54;TPCC_TPCC_EMRH_EMR55; TPCC_TPCC_EMRH_EMR56;TPCC_TPCC_EMRH_EMR57;TPCC_TPCC_EMRH_EMR58; TPCC_TPCC_EMRH_EMR59;TPCC_TPCC_EMRH_EMR60;TPCC_TPCC_EMRH_EMR61; TPCC_TPCC_EMRH_EMR62;TPCC_TPCC_EMRH_EMR63;

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                Bool                    missed;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Check if DMA Channel 1 has an event missed.
                CSL_edma3IsDMAChannelMissedEventSet(hModule, 1, &missed);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3IsDMAChannelSecondaryEventSet | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | dmaChannel,
|  | Bool * | response |
| ) |  |  |

============================================================================
CSL_edma3IsDMAChannelSecondaryEventSet

Description
This API is used to determine if the secondary Event for a specific DMA channel is set or not?

Arguments

            hModule         Module Handle
            dmaChannel      DMA Channel for which secondary Events are being checked
            response        Status of the check populated by the API (TRUE if event
                            is missed else FALSE)

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_SER_SER0;TPCC_TPCC_SER_SER1;TPCC_TPCC_SER_SER2; TPCC_TPCC_SER_SER3;TPCC_TPCC_SER_SER4;TPCC_TPCC_SER_SER5; TPCC_TPCC_SER_SER6;TPCC_TPCC_SER_SER7;TPCC_TPCC_SER_SER8; TPCC_TPCC_SER_SER9;TPCC_TPCC_SER_SER10;TPCC_TPCC_SER_SER11; TPCC_TPCC_SER_SER12;TPCC_TPCC_SER_SER13;TPCC_TPCC_SER_SER14; TPCC_TPCC_SER_SER15;TPCC_TPCC_SER_SER16;TPCC_TPCC_SER_SER17; TPCC_TPCC_SER_SER18;TPCC_TPCC_SER_SER19;TPCC_TPCC_SER_SER20; TPCC_TPCC_SER_SER21;TPCC_TPCC_SER_SER22;TPCC_TPCC_SER_SER23; TPCC_TPCC_SER_SER24;TPCC_TPCC_SER_SER25;TPCC_TPCC_SER_SER26; TPCC_TPCC_SER_SER27;TPCC_TPCC_SER_SER28;TPCC_TPCC_SER_SER29; TPCC_TPCC_SER_SER30;TPCC_TPCC_SER_SER31;
TPCC_TPCC_SERH_SER32;TPCC_TPCC_SERH_SER33;TPCC_TPCC_SERH_SER34; TPCC_TPCC_SERH_SER35;TPCC_TPCC_SERH_SER36;TPCC_TPCC_SERH_SER37; TPCC_TPCC_SERH_SER38;TPCC_TPCC_SERH_SER39;TPCC_TPCC_SERH_SER40; TPCC_TPCC_SERH_SER41;TPCC_TPCC_SERH_SER42;TPCC_TPCC_SERH_SER43; TPCC_TPCC_SERH_SER44;TPCC_TPCC_SERH_SER45;TPCC_TPCC_SERH_SER46; TPCC_TPCC_SERH_SER47;TPCC_TPCC_SERH_SER48;TPCC_TPCC_SERH_SER49; TPCC_TPCC_SERH_SER50;TPCC_TPCC_SERH_SER51;TPCC_TPCC_SERH_SER52; TPCC_TPCC_SERH_SER53;TPCC_TPCC_SERH_SER54;TPCC_TPCC_SERH_SER55; TPCC_TPCC_SERH_SER56;TPCC_TPCC_SERH_SER57;TPCC_TPCC_SERH_SER58; TPCC_TPCC_SERH_SER59;TPCC_TPCC_SERH_SER60;TPCC_TPCC_SERH_SER61; TPCC_TPCC_SERH_SER62;TPCC_TPCC_SERH_SER63;

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                Bool                    response;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Check if the DMA Channel 1 Secondary Event is set or not?
                CSL_edma3IsDMAChannelSecondaryEventSet(hModule, 1, &response);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3IsQDMAChannelEventPending | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | qdmaChannel,
|  | Bool * | response |
| ) |  |  |

============================================================================
CSL_edma3IsQDMAChannelEventPending

Description
The function gets the status of the specified QDMA channel i.e. if there is a pending event on the specific channel.

Arguments

            hModule         Module Handle
            qdmaChannel     QDMA Channel for which status is being inquired.
            response        Place holder for whether an event is set(TRUE) or not (FALSE)

Return Value
None.

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_QER_QER0;TPCC_TPCC_QER_QER1;TPCC_TPCC_QER_QER2;TPCC_TPCC_QER_QER3; TPCC_TPCC_QER_QER4;TPCC_TPCC_QER_QER5;TPCC_TPCC_QER_QER6;TPCC_TPCC_QER_QER7

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                Bool                    qdmaStatus;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Is QDMA Channel 1 event pending.
                CSL_edma3IsQDMAChannelEventPending(hModule, 1, &qdmaStatus);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3IsQDMAChannelMissedEventSet | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | qdmaChannel,
|  | Bool * | response |
| ) |  |  |

============================================================================
CSL_edma3IsQDMAChannelMissedEventSet

Description
The API checks determines if there is a missed Event for a specific DMA channel

Arguments

            hModule         Module Handle
            qdmaChannel     QDMA Channel to be checked
            response        This is populated by the API and returns TRUE if the
                            event was missed else it returns FALSE.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_QEMR_QEMR0;TPCC_TPCC_QEMR_QEMR1;TPCC_TPCC_QEMR_QEMR2; TPCC_TPCC_QEMR_QEMR3;TPCC_TPCC_QEMR_QEMR4;TPCC_TPCC_QEMR_QEMR5; TPCC_TPCC_QEMR_QEMR6;TPCC_TPCC_QEMR_QEMR7

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                Bool                    missed;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Check if DMA Channel 0 has an event missed.
                CSL_edma3IsQDMAChannelMissedEventSet(hModule, 0, &missed);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3IsQDMAChannelSecondaryEventSet | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | qdmaChannel,
|  | Bool * | response |
| ) |  |  |

============================================================================
CSL_edma3IsDMAChannelSecondaryEventSet

Description
This API is used to determine if the secondary Event for a specific DMA channel is set or not?

Arguments

            hModule         Module Handle
            qdmaChannel     QDMA Channel for which secondary Events are being checked
            response        Status of the check populated by the API (TRUE if event
                            is missed else FALSE)

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Reads
TPCC_TPCC_QSER_QSER0;TPCC_TPCC_QSER_QSER1;TPCC_TPCC_QSER_QSER2; TPCC_TPCC_QSER_QSER3;TPCC_TPCC_QSER_QSER4;TPCC_TPCC_QSER_QSER5; TPCC_TPCC_QSER_QSER6;TPCC_TPCC_QSER_QSER7;

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;
                Bool                    response;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Check if the QDMA Channel 1 Secondary Event is set or not?
                CSL_edma3IsQDMAChannelSecondaryEventSet(hModule, 1, &response);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3MapDMAChannelToEventQueue | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | dmaChannel,
|  | Uint8 | eventQueue |
| ) |  |  |

============================================================================
CSL_edma3MapDMAChannelToEventQueue

Description
The function maps the event ID to the specific DMA Queue.

Arguments

            hModule     Module Handle
            dmaChannel  DMA Channel to which the event is mapped.
            eventQueue  Event Queue which is to be mapped.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
DMA Channel is mapped to the specified Event Queue.

Writes
TPCC_TPCC_DMAQNUM_E0;TPCC_TPCC_DMAQNUM_E1;TPCC_TPCC_DMAQNUM_E2; TPCC_TPCC_DMAQNUM_E3;TPCC_TPCC_DMAQNUM_E4;TPCC_TPCC_DMAQNUM_E5; TPCC_TPCC_DMAQNUM_E6;TPCC_TPCC_DMAQNUM_E7

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, CSL_EDMA3, NULL, &status);

                // Maps DMA Channel 1 to Event Queue 2
                CSL_edma3MapDMAChannelToEventQueue(hModule, 1, 2);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3MapDMAChannelToParamBlock | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | dmaChannel,
|  | Uint16 | paramId |
| ) |  |  |

============================================================================
CSL_edma3MapDMAChannelToParamBlock

Description
The function maps the DMA Channel to the specified PARAM Entry Block.

Arguments

            hModule     Module Handle
            dmaChannel  DMA Channel Number which is to be mapped.
            paramId     Parameter Identifier to be mapped to.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
DMA Channel is mapped to the specified PARAM Block.

Writes
TPCC_TPCC_DCHMAP_PAENTRY

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, CSL_EDMA3, NULL, &status);

                // Maps DMA Channel 1 to Param ID Block 5.
                CSL_edma3MapDMAChannelToParamBlock(hModule, 1, 5);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3MapEventQueueToTC | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | eventQueue,
|  | Uint8 | tcNum |
| ) |  |  |

============================================================================
CSL_edma3MapEventQueueToTC

Description
The function maps the event queue to a specific TC

Arguments

            hModule     Module Handle
            eventQueue  Event Queue which is to be mapped.
            tcNum       TC to which the queue is to be mapped to.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
Event Queue is mapped to the specific TC

Writes
TPCC_TPCC_QUETCMAP_TCNUMQ0;TPCC_TPCC_QUETCMAP_TCNUMQ1;TPCC_TPCC_QUETCMAP_TCNUMQ2; TPCC_TPCC_QUETCMAP_TCNUMQ3;TPCC_TPCC_QUETCMAP_TCNUMQ4;TPCC_TPCC_QUETCMAP_TCNUMQ5; TPCC_TPCC_QUETCMAP_TCNUMQ6;TPCC_TPCC_QUETCMAP_TCNUMQ7

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, CSL_EDMA3, NULL, &status);

                // Maps Event Queue 1 to TC0
                CSL_edma3MapEventQueueToTC(hModule, 1, 0);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3MapQDMAChannelToEventQueue | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | qdmaChannel,
|  | Uint8 | eventQueue |
| ) |  |  |

============================================================================
CSL_edma3MapQDMAChannelToEventQueue

Description
The function maps the event ID to the specific DMA Queue.

Arguments

            hModule     Module Handle
            qdmaChannel QDMA Channel to which the event is mapped.
            eventQueue  Event Queue which is to be mapped.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
DMA Channel is mapped to the specified Event Queue.

Writes
TPCC_TPCC_QDMAQNUM_E0;TPCC_TPCC_QDMAQNUM_E1;TPCC_TPCC_QDMAQNUM_E2; TPCC_TPCC_QDMAQNUM_E3;TPCC_TPCC_QDMAQNUM_E4;TPCC_TPCC_QDMAQNUM_E5; TPCC_TPCC_QDMAQNUM_E6;TPCC_TPCC_QDMAQNUM_E7

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, CSL_EDMA3, NULL, &status);

                // Maps QDMA Channel 1 to Event Queue 2
                CSL_edma3MapQDMAChannelToEventQueue(hModule, 1, 2);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3MapQDMAChannelToParamBlock | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | qdmaChannel,
|  | Uint16 | paramId |
| ) |  |  |

============================================================================
CSL_edma3MapQDMAChannelToParamBlock

Description
The function maps the QDMA Channel to the specified PARAM Entry Block.

Arguments

            hModule     Module Handle
            qdmaChannel QDMA Channel Number which is to be mapped.
            paramId     Parameter Identifier to be mapped to.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
QDMA Channel is mapped to the specified PARAM Block.

Writes
TPCC_TPCC_QCHMAP_PAENTRY

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, CSL_EDMA3, NULL, &status);

                // Maps QDMA Channel 1 to Param ID Block 5.
                CSL_edma3MapQDMAChannelToParamBlock(hModule, 1, 5);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3MemFaultClear | ( | CSL_Edma3Handle | hModule | ) |

============================================================================
CSL_edma3MemFaultClear

Description
The function clears the memory fault.

Arguments

            hModule           Module Handle

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_MPFCR_MPFCLR=1

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Clear the memory protection fault
                CSL_edma3MemFaultClear(hModule);
                ...

===========================================================================

CSL_Edma3Handle CSL_edma3Open | ( | CSL_Edma3Obj * | pEdmaObj,
|  | CSL_InstNum | edmaNum,
|  | CSL_Edma3ModuleAttr * | pAttr,
|  | CSL_Status * | pStatus |
| ) |  |  |

============================================================================
CSL_edma3Open

Description
This function returns the handle to the EDMA instance. This handle is passed to all other CSL APIs.

Arguments

                pEdmaObj         EDMA Module Object pointer
                edmaNum          Instance of EDMA
                pAttr            EDMA Attribute pointer
                pStatus          Status of the function call

Return Value
Success - Valid Edma handle will be returned if status value is equal to CSL_SOK.
Failure - NULL

Pre Condition
The EDMA must be succesfully initialized via CSL_edma3Init() before calling this function.

Post Condition
1. The status is returned in the status variable. If status returned is

- CSL_SOK Valid EDMA handle is returned
- CSL_ESYS_FAIL The EDMA instance is invalid
- CSL_ESYS_INVPARAMS The Parameter passed is invalid

2. Edma object structure is populated

Affects
None

Example

                CSL_Edma3Handle     hModule;
                CSL_Edma3Obj        edmaObj;
                CSL_Status          status;

                // Module Initialization
                CSL_edma3Init(NULL);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

=============================================================================

CSL_Status CSL_edma3ParamSetup | ( | CSL_Edma3ParamHandle | hParamHndl,
|  | CSL_Edma3ParamSetup * | setup |
| ) |  |  |

============================================================================
CSL_edma3ParamSetup

Description
The function is used to configure the PARAM Entry block with the specific parameter information.

Arguments

                hParamHndl      Handle to the param entry
                setup           Pointer to param setup structure

Return Value
Success - CSL_SOK
Error - CSL_ESYS_BADHANDLE (The handle passed is invalid)
Error - CSL_ESYS_INVPARAMS (The parameter passed is invalid)

Pre Condition
CSL_edma3Init(), CSL_edma3Open() and CSL_edma3ChannelOpen() must be called successfully in that order before this API can be invoked

Post Condition
Configures the EDMA parameter Entry

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Status              status;
                CSL_Edma3ChannelHandle  hChannel;
                CSL_Edma3ChannelAttr    chAttr;
                CSL_Edma3ParamHandle    hParamBasic;
                CSL_Edma3ParamSetup     myParamSetup;

                // Module Initialization
                CSL_edma3Init(NULL);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Open DMA Channel 1.
                chAttr.regionNum = CSL_EDMA3_REGION_GLOBAL;
                chAttr.chaNum    = 1;
                hChannel = CSL_edma3ChannelOpen(&chObj, 0, &chAttr, &status);
                if ((hChannel == NULL) || (status != CSL_SOK))
                {
                    printf ("Error: Unable to open EDMA Channel:%d\n", channelNum);
                    return -1;
                }
                ...
                // Obtain a handle to PARAM Entry 0
                hParamBasic = CSL_edma3GetParamHandle(hChannel,0,&status);
                ...
                // Setup the first param Entry (Ping buffer)
                myParamSetup.option = CSL_EDMA3_OPT_MAKE(CSL_EDMA3_ITCCH_DIS, \
                                                         CSL_EDMA3_TCCH_DIS, \
                                                         CSL_EDMA3_ITCINT_DIS, \
                                                         CSL_EDMA3_TCINT_EN,\
                                                         0,CSL_EDMA3_TCC_NORMAL,\
                                                         CSL_EDMA3_FIFOWIDTH_NONE, \
                                                         CSL_EDMA3_STATIC_DIS, \
                                                         CSL_EDMA3_SYNC_A, \
                                                         CSL_EDMA3_ADDRMODE_INCR, \
                                                         CSL_EDMA3_ADDRMODE_INCR);
                myParamSetup.srcAddr     = (Uint32)srcBuff1;
                myParamSetup.aCntbCnt    = CSL_EDMA3_CNT_MAKE(256,1);
                myParamSetup.dstAddr     = (Uint32)dstBuff1;
                myParamSetup.srcDstBidx  = CSL_EDMA3_BIDX_MAKE(1,1);
                myParamSetup.linkBcntrld = CSL_EDMA3_LINKBCNTRLD_MAKE(CSL_EDMA3_LINK_NULL,0);
                myParamSetup.srcDstCidx  = CSL_EDMA3_CIDX_MAKE(0,1);
                myParamSetup.cCnt        = 1;

                // Configure the PARAM Entry with the setup information.
                CSL_edma3ParamSetup(hParamBasic,&myParamSetup);
                ...

=============================================================================

CSL_Status CSL_edma3ParamWriteWord | ( | CSL_Edma3ParamHandle | hParamHndl,
|  | Uint16 | wordOffset,
|  | Uint32 | word |
| ) |  |  |

============================================================================
CSL_edma3ParamWriteWord

Description
This is for the ease of QDMA channels. Once the QDMA channel transfer is triggered, subsequent triggers may be done with only writing the modified words in the parameter entry along with the trigger word. This API is expected to achieve this purpose. Most usage scenarios, the user should not be writing more than the trigger word entry.

Arguments

                hParamHndl      Handle to the param entry
                wordOffset      word offset in the 8 word paramater entry
                word            word to be written

Return Value
Success - CSL_SOK (Param Write Word successful)
Error - CSL_ESYS_BADHANDLE (Invalid handle)

Pre Condition
CSL_edma3Init(), CSL_edma3Open() and CSL_edma3ChannelOpen() and must be CSL_edma3GetParamHandle(), CSL_edma3ParamSetup() called successfully in that order before this API can be invoked. The main setup structure consists of pointers to sub-structures.The user has to allocate space for & fill in the parameter setup structure.

Post Condition
Configure trigger word

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Status              status;
                CSL_Edma3ChannelHandle  hChannel;
                CSL_Edma3ChannelAttr    chAttr;
                CSL_Edma3ParamHandle    hParamBasic;

                // Module Initialization
                CSL_edma3Init(NULL);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Open DMA Channel 1.
                chAttr.regionNum = CSL_EDMA3_REGION_GLOBAL;
                chAttr.chaNum    = 1;
                hChannel = CSL_edma3ChannelOpen(&chObj, 0, &chAttr, &status);
                if ((hChannel == NULL) || (status != CSL_SOK))
                {
                    printf ("Error: Unable to open EDMA Channel:%d\n", channelNum);
                    return -1;
                }
                ...
                // Obtain a handle to PARAM Entry 0
                hParamBasic = CSL_edma3GetParamHandle(hChannel,0,&status);
                ...
                // Write trigger word
                CSL_edma3ParamWriteWord(hParamBasic, 7, myParamSetup.cCnt);
                ...

=============================================================================

CSL_IDEF_INLINE void CSL_edma3QDMAChannelDisable | ( | CSL_Edma3Handle | hModule,
|  | Int | region,
|  | Uint8 | qdmaChannel |
| ) |  |  |

============================================================================
CSL_edma3QDMAChannelDisable

Description
This API disables the specified QDMA Channel.

Arguments

            hModule         Module Handle
            region          Region (Shadown Region or Global)
            qdmaChannel     QDMA Channel to be disabled.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_QEECR_QEECR0=1;TPCC_TPCC_QEECR_QEECR1=1;TPCC_TPCC_QEECR_QEECR2=1; TPCC_TPCC_QEECR_QEECR3=1;TPCC_TPCC_QEECR_QEECR4=1;TPCC_TPCC_QEECR_QEECR5=1; TPCC_TPCC_QEECR_QEECR6=1;TPCC_TPCC_QEECR_QEECR7=1;

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Disables QDMA Channel 0
                CSL_edma3QDMAChannelDisable(hModule, 0);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3QDMAChannelEnable | ( | CSL_Edma3Handle | hModule,
|  | Int | region,
|  | Uint8 | qdmaChannel |
| ) |  |  |

============================================================================
CSL_edma3QDMAChannelEnable

Description
This API enables the specified QDMA Channel.

Arguments

            hModule         Module Handle
            region          Region (Shadown Region or Global)
            qdmaChannel     QDMA Channel to be enabled.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_QEESR_QEESR0=1;TPCC_TPCC_QEESR_QEESR1=1;TPCC_TPCC_QEESR_QEESR2=1; TPCC_TPCC_QEESR_QEESR3=1;TPCC_TPCC_QEESR_QEESR4=1;TPCC_TPCC_QEESR_QEESR5=1; TPCC_TPCC_QEESR_QEESR6=1;TPCC_TPCC_QEESR_QEESR7=1;

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Enables QDMA Channel 1 for Global Region.
                CSL_edma3QDMAChannelEnable(hModule, CSL_EDMA3_REGION_GLOBAL, 1);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3QdmaRegionAccessDisable | ( | CSL_Edma3Handle | hModule,
|  | Int | edmaRegion,
|  | CSL_BitMask32 | qrae |
| ) |  |  |

============================================================================
CSL_edma3QdmaRegionAccessDisable

Description
This API disables read/write access to the shadow regions for the specific QDMA channels.

Arguments

            hModule           Module Handle
            edmaRegion        Shadow Region.
            qrae              Bitmask to be enabled in QRAE

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_QRAE_E0=0;TPCC_TPCC_QRAE_E1=0;TPCC_TPCC_QRAE_E2=0; TPCC_TPCC_QRAE_E3=0;TPCC_TPCC_QRAE_E4=0;TPCC_TPCC_QRAE_E5=0; TPCC_TPCC_QRAE_E6=0;TPCC_TPCC_QRAE_E7=0

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Disable read/write access in Region 0 for QDMA 0 to 3
                CSL_edma3QdmaRegionAccessDisable(hModule, 0, 0x0000000F);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3QdmaRegionAccessEnable | ( | CSL_Edma3Handle | hModule,
|  | Int | edmaRegion,
|  | CSL_BitMask32 | qrae |
| ) |  |  |

============================================================================
CSL_edma3QdmaRegionAccessEnable

Description
This API enables read/write access to the shadow regions for the specific QDMA channels.

Arguments

            hModule           Module Handle
            edmaRegion        Shadow Region
            qrae              Bitmask to be enabled in QRAE

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_QRAE_E0=1;TPCC_TPCC_QRAE_E1=1;TPCC_TPCC_QRAE_E2=1; TPCC_TPCC_QRAE_E3=1;TPCC_TPCC_QRAE_E4=1;TPCC_TPCC_QRAE_E5=1; TPCC_TPCC_QRAE_E6=1;TPCC_TPCC_QRAE_E7=1

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);

                // Enable read/write access in Region 0 for QDMA 0 to 3
                CSL_edma3QdmaRegionAccessEnable(hModule, 0, 0x0000000F);

===========================================================================

CSL_IDEF_INLINE void CSL_edma3SetDMAChannelEvent | ( | CSL_Edma3Handle | hModule,
|  | Int | region,
|  | Uint8 | dmaChannel |
| ) |  |  |

============================================================================
CSL_edma3SetDMAChannelEvent

Description
This API sets the event for the specific DMA channel.

Arguments

            hModule         Module Handle
            region          Region (Shadow or Global)
            dmaChannel      DMA Channel for which the event is to be set

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_ESR_E0=1;TPCC_TPCC_ESR_E1=1;TPCC_TPCC_ESR_E2=1;TPCC_TPCC_ESR_E3=1; TPCC_TPCC_ESR_E4=1;TPCC_TPCC_ESR_E5=1;TPCC_TPCC_ESR_E6=1;TPCC_TPCC_ESR_E7=1; TPCC_TPCC_ESR_E8=1;TPCC_TPCC_ESR_E9=1;TPCC_TPCC_ESR_E10=1;TPCC_TPCC_ESR_E11=1; TPCC_TPCC_ESR_E12=1;TPCC_TPCC_ESR_E13=1;TPCC_TPCC_ESR_E14=1;TPCC_TPCC_ESR_E15=1; TPCC_TPCC_ESR_E16=1;TPCC_TPCC_ESR_E17=1;TPCC_TPCC_ESR_E18=1;TPCC_TPCC_ESR_E19=1; TPCC_TPCC_ESR_E20=1;TPCC_TPCC_ESR_E21=1;TPCC_TPCC_ESR_E22=1;TPCC_TPCC_ESR_E23=1; TPCC_TPCC_ESR_E24=1;TPCC_TPCC_ESR_E25=1;TPCC_TPCC_ESR_E26=1;TPCC_TPCC_ESR_E27=1; TPCC_TPCC_ESR_E28=1;TPCC_TPCC_ESR_E29=1;TPCC_TPCC_ESR_E30=1;TPCC_TPCC_ESR_E31=1;
TPCC_TPCC_ESRH_E32=1;TPCC_TPCC_ESRH_E33=1;TPCC_TPCC_ESRH_E34=1;TPCC_TPCC_ESRH_E35=1; TPCC_TPCC_ESRH_E36=1;TPCC_TPCC_ESRH_E37=1;TPCC_TPCC_ESRH_E38=1;TPCC_TPCC_ESRH_E39=1; TPCC_TPCC_ESRH_E40=1;TPCC_TPCC_ESRH_E41=1;TPCC_TPCC_ESRH_E42=1;TPCC_TPCC_ESRH_E43=1; TPCC_TPCC_ESRH_E44=1;TPCC_TPCC_ESRH_E45=1;TPCC_TPCC_ESRH_E46=1;TPCC_TPCC_ESRH_E47=1; TPCC_TPCC_ESRH_E48=1;TPCC_TPCC_ESRH_E49=1;TPCC_TPCC_ESRH_E50=1;TPCC_TPCC_ESRH_E51=1; TPCC_TPCC_ESRH_E52=1;TPCC_TPCC_ESRH_E53=1;TPCC_TPCC_ESRH_E54=1;TPCC_TPCC_ESRH_E55=1; TPCC_TPCC_ESRH_E56=1;TPCC_TPCC_ESRH_E57=1;TPCC_TPCC_ESRH_E58=1;TPCC_TPCC_ESRH_E59=1; TPCC_TPCC_ESRH_E60=1;TPCC_TPCC_ESRH_E61=1;TPCC_TPCC_ESRH_E62=1;TPCC_TPCC_ESRH_E63=1;

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Set the DMA Channel 0 Event for the Global Region.
                CSL_edma3SetDMAChannelEvent(hModule, CSL_EDMA3_REGION_GLOBAL, 0);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3SetEventQueuePriority | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | eventQueue,
|  | Uint8 | priority |
| ) |  |  |

============================================================================
CSL_edma3SetEventQueuePriority

Description
The function sets the priority of the specific event queue.

Arguments

            hModule     Module Handle
            eventQueue  Event Queue whose priority is to be configured.
            priority    Priority to be configured.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
Event Queue is configured to the specific priority.

Writes
TPCC_TPCC_QUEPRI_PRIQ0;TPCC_TPCC_QUEPRI_PRIQ1;TPCC_TPCC_QUEPRI_PRIQ2; TPCC_TPCC_QUEPRI_PRIQ3;TPCC_TPCC_QUEPRI_PRIQ4;TPCC_TPCC_QUEPRI_PRIQ5; TPCC_TPCC_QUEPRI_PRIQ6;TPCC_TPCC_QUEPRI_PRIQ7

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, CSL_EDMA3, NULL, &status);

                // Maps Event Queue 2 to Priority 4
                CSL_edma3SetEventQueuePriority(hModule, 2, 4);
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3SetMemoryProtectionAttrib | ( | CSL_Edma3Handle | hModule,
|  | Int | region,
|  | CSL_BitMask32 | mppa |
| ) |  |  |

============================================================================
CSL_edma3SetMemoryProtectionAttrib

Description
This API sets the memory protection attributes for the specified region.

Arguments

            hModule         Module Handle
            region          Region being configured.
            mpa             Value to be programmed into the MPPAG/MPPA[0/1/2/../n]
                            This is a Bitmask of the protection attributes.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
None

Writes
TPCC_TPCC_MPPAG;TPCC_TPCC_MPPA

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj,CSL_EDMA3,NULL,&status);
                ...
                // Set the memory protection attributes of region 0.
                CSL_edma3SetMemoryProtectionAttrib (hModule, 0, CSL_EDMA3_MEMACCESS_UX |
                                                                CSL_EDMA3_MEMACCESS_UW |
                                                                CSL_EDMA3_MEMACCESS_UR |
                                                                CSL_EDMA3_MEMACCESS_AID2));
                ...

===========================================================================

CSL_IDEF_INLINE void CSL_edma3SetQDMATriggerWord | ( | CSL_Edma3Handle | hModule,
|  | Uint8 | qdmaChannel,
|  | Uint8 | trword |
| ) |  |  |

============================================================================
CSL_edma3SetQDMATriggerWord

Description
The function sets the trigger word of the PaRAM Entry block.

Arguments

            hModule     Module Handle
            qdmaChannel QDMA Channel Number which is to be configured.
            trword      Trigger Word to be configured.

Return Value
None

Pre Condition
Both CSL_edma3Init() and CSL_edma3Open() must be called.

Post Condition
QDMA Channel is mapped to the specified PARAM Block.

Writes
TPCC_TPCC_QCHMAP_TRWORD

Example

                CSL_Edma3Handle         hModule;
                CSL_Edma3Obj            edmaObj;
                CSL_Edma3Context        context;
                CSL_Status              status;

                // Module Initialization
                CSL_edma3Init(&context);

                // Module Level Open
                hModule = CSL_edma3Open(&edmaObj, CSL_EDMA3, NULL, &status);

                // Configure QDMA Channel 1 Trigger Word as 0
                CSL_edma3SetQDMATriggerWord(hModule, 1, 0);
                ...

===========================================================================

Copyright 2012, Texas Instruments Incorporated