# pcieActStatusReg_s Struct Reference
[PCIE LLD Application Register Definitions]

Specification of the Activity Status Register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint8_t | obNotEmpty
| [ro] Outbound Buffers Not Empty
uint8_t | ibNotEmpty
| [ro] Inbound Buffers Not Empty

## Detailed Description

Specification of the Activity Status Register.

## Field Documentation

uint8_t pcieActStatusReg_s::ibNotEmpty

[ro] Inbound Buffers Not Empty

Field size: 1 bit

uint8_t pcieActStatusReg_s::obNotEmpty

[ro] Outbound Buffers Not Empty

Field size: 1 bit

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated