# Srio_DrvManagedTxCfg Struct Reference
[SRIO LLD Data Structures]

The structure describes the SRIO Driver Managed Transmit Configuration. More...

`#include <srio_drv.h>`

## Data Fields

uint32_t | numTxBuffers
| The number of transmit buffers available to the driver instance which can be used to transmit data.
Qmss_MemRegion | txMemRegion
| This is the memory region to be used for allocating the transmit buffer descriptors.
uint32_t | txMTU
| For Normal sockets this is the Maximum data size which can be transmitted.

## Detailed Description

The structure describes the SRIO Driver Managed Transmit Configuration.

This specifies the Transmit configuration which is a part of the Driver Managed configuration.

The documentation for this struct was generated from the following file:

- srio_drv.h

Copyright 2012, Texas Instruments Incorporated