/*
 * config.bld
 *
 * Build configuration Script for the EMAC Driver
 *
 * Copyright (C) 2010 Texas Instruments Incorporated - http://www.ti.com/ 
 * 
 * 
 *  Redistribution and use in source and binary forms, with or without 
 *  modification, are permitted provided that the following conditions 
 *  are met:
 *
 *    Redistributions of source code must retain the above copyright 
 *    notice, this list of conditions and the following disclaimer.
 *
 *    Redistributions in binary form must reproduce the above copyright
 *    notice, this list of conditions and the following disclaimer in the 
 *    documentation and/or other materials provided with the   
 *    distribution.
 *
 *    Neither the name of Texas Instruments Incorporated nor the names of
 *    its contributors may be used to endorse or promote products derived
 *    from this software without specific prior written permission.
 *
 *  THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS 
 *  "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT 
 *  LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
 *  A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT 
 *  OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, 
 *  SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT 
 *  LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
 *  DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY
 *  THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT 
 *  (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE 
 *  OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
 *
*/

/******************************************************************************
 * FILE PURPOSE: Build configuration Script for the EMAC Driver
 ******************************************************************************
 * FILE NAME: config.bld
 *
 * DESCRIPTION: 
 *  This file contains the build configuration script for the EMAC Driver
 *  Package. The file is responsible for configuring the BUILD 
 *  Environment to be able to build the package.
 *****************************************************************************/

/* Get the Tools Base directory from the Environment Variable. */
var toolsBaseDir = java.lang.System.getenv("XDCCGROOT");

/* Get the base directory for the EMAC LLD Package */
var lldPath = new java.io.File(".//").getPath();

var lldInstallType;

/* Read the part number from the environment variable. */
var lldPartNumber = java.lang.System.getenv("PARTNO");

/* Include Path */
var lldIncludePath = " -i" + lldPath + "/src" + " -i" + lldPath  + " -i" + lldPath + "/test";

/* Configure the EMAC LLD Release Version Information */
var lldReleaseVersion = [01,00,03,00];

/* EMAC LLD Coverity Analysis: Check the environment variable to determine if Static
 * Analysis has to be done on the EMAC LLD Code base or not? */
var lldCoverityAnalysis = java.lang.System.getenv("LLDCOV");

/* EMAC Driver Package Release type.
 * 
 * Indicates if the release package should include the XDC build
 * files or not. By default, the release package does not contain
 * the XDC build files.
 */
var emacReleaseType;

/* Configure the C66 compiler to operate in Little Endian Mode. */
var C66LE           = xdc.useModule('ti.targets.elf.C66');
C66LE.rootDir       = toolsBaseDir;
C66LE.ccOpts.prefix = "-mo -o3 -q -k -eo.o";

/* Configure the C66 compiler to operate in Big Endian Mode. */
var C66BE           = xdc.useModule('ti.targets.elf.C66_big_endian');
C66BE.rootDir       = toolsBaseDir;
C66BE.ccOpts.prefix = "-mo -o3 -q -k -eo.o -DBIGENDIAN";

/* Check if we need to run the STATIC Analysis or not? */
var coverityAnalysis = java.lang.System.getenv("STATIC_ANALYZE");

/* Setup the Coverity Filters to perform Static Analysis. */
if (coverityAnalysis == "ON") {
    var coverityInstallPath = java.lang.System.getenv("STATIC_ANALYZE_PATH");
    var cfgBase = xdc.getPackageBase("tisb.coverity.filters") + "cfg";

    var coverityFilter = [
    {
        moduleName: "tisb.coverity.filters.Coverity",
        params: {
            cfgDir:  cfgBase,  // The Coverity configuration file directory
            rootDir: coverityInstallPath,
            outDir: xdc.csd() + "cov_out",
            analyzeLibs: true
        }
    },
    ];

    /* Run the coverity filters on the LE Build only. */
    C66LE.profiles["release"].filters = coverityFilter;
}

/* List all the build targets here. The EMAC has a C66 DSP core. */
Build.targets = [ C66LE, C66BE ];

