# pcieMsiDataReg_s Struct Reference
[PCIE LLD Message Signaled Interrupt Capabilities Register Definitions]

Specification of the MSI Data Register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint16_t | data
| [rw] MSI data

## Detailed Description

Specification of the MSI Data Register.

This register may be used for both endpoint and root complex modes.

## Field Documentation

uint16_t pcieMsiDataReg_s::data

[rw] MSI data

Field size: 16 bits

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated