# pcieUncErrMaskReg_s Struct Reference
[PCIE LLD Extended Capabilities Register Definitions]

Specification of the Uncorrectable Error Mask register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
uint8_t | urErrMsk
| [rw] Unsupported Request Error Mask
uint8_t | ecrcErrMsk
| [rw] ECRC Error Mask
uint8_t | mtlpErrMsk
| [rw] Malformed TLP Mask
uint8_t | rcvrOfMsk
| [rw] Receiver Overflow Mask
uint8_t | ucmpMsk
| [rw] Unexpected Completion Mask
uint8_t | cmplAbrtMsk
| [rw] Completer Abort Mask
uint8_t | cmplTmotMsk
| [rw] Completion Timeout Mask
uint8_t | fcpErrMsk
| [rw] Flow Control Protocol Error Mask
uint8_t | psndTlpMsk
| [rw] Poisoned TLP Mask
uint8_t | srpsDnMsk
| [ro] Surprise Down Error Mask. Not supported (always 0)
uint8_t | dlpErrMsk
| [rw] Data Link Protocol Error Mask

## Detailed Description

Specification of the Uncorrectable Error Mask register.

This register may be used for both endpoint and root complex modes.

## Field Documentation

uint8_t pcieUncErrMaskReg_s::cmplAbrtMsk

[rw] Completer Abort Mask

Field size: 1 bit

uint8_t pcieUncErrMaskReg_s::cmplTmotMsk

[rw] Completion Timeout Mask

Field size: 1 bit

uint8_t pcieUncErrMaskReg_s::dlpErrMsk

[rw] Data Link Protocol Error Mask

Field size: 1 bit

uint8_t pcieUncErrMaskReg_s::ecrcErrMsk

[rw] ECRC Error Mask

Field size: 1 bit

uint8_t pcieUncErrMaskReg_s::fcpErrMsk

[rw] Flow Control Protocol Error Mask

Field size: 1 bit

uint8_t pcieUncErrMaskReg_s::mtlpErrMsk

[rw] Malformed TLP Mask

Field size: 1 bit

uint8_t pcieUncErrMaskReg_s::psndTlpMsk

[rw] Poisoned TLP Mask

Field size: 1 bit

uint32_t pcieUncErrMaskReg_s::raw

[ro] Raw image of register on read; actual value on write

uint8_t pcieUncErrMaskReg_s::rcvrOfMsk

[rw] Receiver Overflow Mask

Field size: 1 bit

uint8_t pcieUncErrMaskReg_s::srpsDnMsk

[ro] Surprise Down Error Mask. Not supported (always 0)

Field size: 1 bit

uint8_t pcieUncErrMaskReg_s::ucmpMsk

[rw] Unexpected Completion Mask

Field size: 1 bit

uint8_t pcieUncErrMaskReg_s::urErrMsk

[rw] Unsupported Request Error Mask

Field size: 1 bit

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated