# pcieCorErrMaskReg_s Struct Reference
[PCIE LLD Extended Capabilities Register Definitions]

Specification of the Correctable Error Mask register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
uint8_t | advNFErrMsk
| [rw] Advisory Non-Fatal Error Mask
uint8_t | rplyTmrMsk
| [rw] Replay Timer Timeout Mask
uint8_t | rpltRoMsk
| [rw] REPLAY_NUM Rollover Mask
uint8_t | badDllpMsk
| [rw] Bad DLLP Mask
uint8_t | badTlpMsk
| [rw] Bad TLP Mask
uint8_t | rcvrErrMsk
| [rw] Receiver Error Mask

## Detailed Description

Specification of the Correctable Error Mask register.

This register may be used for both endpoint and root complex modes.

## Field Documentation

uint8_t pcieCorErrMaskReg_s::advNFErrMsk

[rw] Advisory Non-Fatal Error Mask

Field size: 1 bit

uint8_t pcieCorErrMaskReg_s::badDllpMsk

[rw] Bad DLLP Mask

Field size: 1 bit

uint8_t pcieCorErrMaskReg_s::badTlpMsk

[rw] Bad TLP Mask

Field size: 1 bit

uint32_t pcieCorErrMaskReg_s::raw

[ro] Raw image of register on read; actual value on write

uint8_t pcieCorErrMaskReg_s::rcvrErrMsk

[rw] Receiver Error Mask

Field size: 1 bit

uint8_t pcieCorErrMaskReg_s::rpltRoMsk

[rw] REPLAY_NUM Rollover Mask

Field size: 1 bit

uint8_t pcieCorErrMaskReg_s::rplyTmrMsk

[rw] Replay Timer Timeout Mask

Field size: 1 bit

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated