# pciePrefLimitUpperReg_s Struct Reference
[PCIE LLD Type1 (root) Register Definitions]

Specification of the Prefetchable Memory Limit Upper Register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint32_t | limit
| [rw] Base upper 32bits

## Detailed Description

Specification of the Prefetchable Memory Limit Upper Register.

## Field Documentation

uint32_t pciePrefLimitUpperReg_s::limit

[rw] Base upper 32bits

Upper 32 bits of Prefetchable Memory Limit Address. Used with 64 bit prefetchable memory addressing only.

Field size: 32 bits

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated