# Srio_DrvConfig Struct Reference
[SRIO LLD Data Structures]

The structure describes the SRIO Driver Configuration. More...

`#include <srio_drv.h>`

## Data Fields

uint16_t | bAppManagedConfig
| The SRIO driver can be configured to use either of the following configurations:

- Application Managed configuration
- Driver Managed configuration This flag can be used to select which configuration is specified.

Srio_DrvConfigType | u
| Union structure for the driver configuration.

## Detailed Description

The structure describes the SRIO Driver Configuration.

SRIO Driver users are expected to populate the driver configuration block and pass it to the driver during initialization.

The documentation for this struct was generated from the following file:

- srio_drv.h

Copyright 2012, Texas Instruments Incorporated