# pcieEndianReg_s Struct Reference
[PCIE LLD Application Register Definitions]

Specification of the Endian Register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
uint8_t | mode
| [rw] Endian mode.

## Detailed Description

Specification of the Endian Register.

## Field Documentation

uint8_t pcieEndianReg_s::mode

[rw] Endian mode.

mode | Endian Swap Mode
--- | ---
0 | Swap on 1 byte
1 | Swap on 2 bytes
2 | Swap on 4 bytes
3 | Swap on 8 bytes

Field size: 2 bits

uint32_t pcieEndianReg_s::raw

[ro] Raw image of register on read; actual value on write

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated