# CSL_Edma3MemFaultStat Struct Reference
[EDMA3 Data Structures]

Edma Memory Protection Fault Error Status. More...

`#include <csl_edma3.h>`

## Data Fields

Uint32 | addr
CSL_BitMask16 | error
Uint16 | fid

## Detailed Description

Edma Memory Protection Fault Error Status.

An object of this type is allocated by the user and its address is passed as a parameter to the CSL_edma3GetMemoryFaultError() / CSL_edma3GetHwStatus() with the relevant command. This is relevant only is MPEXIST is present for a given device.

## Field Documentation

Uint32 CSL_Edma3MemFaultStat::addr

Memory Protection Fault Address

CSL_BitMask16 CSL_Edma3MemFaultStat::error

Bit Mask of the Errors

Uint16 CSL_Edma3MemFaultStat::fid

Faulted ID

The documentation for this struct was generated from the following file:

- csl_edma3.h

Copyright 2012, Texas Instruments Incorporated