# Tcp3d_Config Struct Reference
[TCP3D Driver Data Structures]

Structure to store TCP3 decoder specific values to identify its instance configuration information. This is created to facilitate the application to choose TCP3 decoder (either TCP3D_A or TCP3D_B) for which the driver will be configured. More...

`#include <tcp3d_drv.h>`

## Data Fields

uint32_t | inCfgStart
uint32_t | llrStart
uint32_t | interStart
uint32_t | hdStart
uint32_t | sdStart
uint32_t | stsStart
uint32_t | revtCh

## Detailed Description

Structure to store TCP3 decoder specific values to identify its instance configuration information. This is created to facilitate the application to choose TCP3 decoder (either TCP3D_A or TCP3D_B) for which the driver will be configured.

This structure could be used for both PING and PONG specific values.

## Field Documentation

uint32_t Tcp3d_Config::hdStart

output hard decision start address

uint32_t Tcp3d_Config::inCfgStart

input configuration registers start address

uint32_t Tcp3d_Config::interStart

inter leaver start address

uint32_t Tcp3d_Config::llrStart

input data (LLR) start address

uint32_t Tcp3d_Config::revtCh

Channel number associated with REVT

uint32_t Tcp3d_Config::sdStart

output soft decision start address

uint32_t Tcp3d_Config::stsStart

output status registers start address

The documentation for this struct was generated from the following file:

- tcp3d_drv.h

Copyright 2012, Texas Instruments Incorporated