# CSL_BWMNGMT_MDMAPRI_SETUP Struct Reference
[BWMNGMT Data Structures]

CSL_BWMNGMT_MDMAPRI_SETUP has all the fields required to configure Master DMA (MDMA) Arbitration Control Register of BWMNGMT for L2/UMC memory control block. More...

`#include <csl_bwmngmt.h>`

## Data Fields

Uint32 | priority
Uint32 | uPriority

## Detailed Description

CSL_BWMNGMT_MDMAPRI_SETUP has all the fields required to configure Master DMA (MDMA) Arbitration Control Register of BWMNGMT for L2/UMC memory control block.

## Field Documentation

Uint32 CSL_BWMNGMT_MDMAPRI_SETUP::priority

MDMA (Master DMA) Requestor Arbitration Settings - PRI

Uint32 CSL_BWMNGMT_MDMAPRI_SETUP::uPriority

MDMA (Master DMA) Requestor Arbitration Settings - EPRI (Urgent Priority)

The documentation for this struct was generated from the following file:

- csl_bwmngmt.h

Copyright 2012, Texas Instruments Incorporated