# EDMA3 Enumerated Data Types
[EDMA3]

## Enumerations

enum | CSL_Edma3QuePri { CSL_EDMA3_QUE_PRI_0 = 0, CSL_EDMA3_QUE_PRI_1 = 1, CSL_EDMA3_QUE_PRI_2 = 2, CSL_EDMA3_QUE_PRI_3 = 3, CSL_EDMA3_QUE_PRI_4 = 4, CSL_EDMA3_QUE_PRI_5 = 5, CSL_EDMA3_QUE_PRI_6 = 6, CSL_EDMA3_QUE_PRI_7 = 7 }
| Enumeration for System priorities. More...
enum | CSL_Edma3Que { CSL_EDMA3_QUE_DEFAULT = 0, CSL_EDMA3_QUE_0 = 0, CSL_EDMA3_QUE_1 = 1, CSL_EDMA3_QUE_2 = 2, CSL_EDMA3_QUE_3 = 3, CSL_EDMA3_QUE_4 = 4, CSL_EDMA3_QUE_5 = 5, CSL_EDMA3_QUE_6 = 6, CSL_EDMA3_QUE_7 = 7 }
| Enumeration for EDMA Event Queues. More...
enum | CSL_Edma3QueThr { CSL_EDMA3_QUE_THR_0 = 0, CSL_EDMA3_QUE_THR_1 = 1, CSL_EDMA3_QUE_THR_2 = 2, CSL_EDMA3_QUE_THR_3 = 3, CSL_EDMA3_QUE_THR_4 = 4, CSL_EDMA3_QUE_THR_5 = 5, CSL_EDMA3_QUE_THR_6 = 6, CSL_EDMA3_QUE_THR_7 = 7, CSL_EDMA3_QUE_THR_8 = 8, CSL_EDMA3_QUE_THR_9 = 9, CSL_EDMA3_QUE_THR_10 = 10, CSL_EDMA3_QUE_THR_11 = 11,
CSL_EDMA3_QUE_THR_12 = 12, CSL_EDMA3_QUE_THR_13 = 13, CSL_EDMA3_QUE_THR_14 = 14, CSL_EDMA3_QUE_THR_15 = 15,
CSL_EDMA3_QUE_THR_16 = 16
}
| Enumeration for EDMA Que Thresholds. More...
enum | CSL_Edma3HwControlCmd { CSL_EDMA3_CMD_MEMPROTECT_SET, CSL_EDMA3_CMD_MEMFAULT_CLEAR, CSL_EDMA3_CMD_DMAREGION_ENABLE, CSL_EDMA3_CMD_DMAREGION_DISABLE, CSL_EDMA3_CMD_QDMAREGION_ENABLE, CSL_EDMA3_CMD_QDMAREGION_DISABLE, CSL_EDMA3_CMD_QUEPRIORITY_SET, CSL_EDMA3_CMD_QUETHRESHOLD_SET,
CSL_EDMA3_CMD_ERROR_EVAL, CSL_EDMA3_CMD_INTRPEND_CLEAR, CSL_EDMA3_CMD_INTR_ENABLE, CSL_EDMA3_CMD_INTR_DISABLE,
CSL_EDMA3_CMD_INTR_EVAL, CSL_EDMA3_CMD_CTRLERROR_CLEAR, CSL_EDMA3_CMD_EVENTMISSED_CLEAR
}
enum | CSL_Edma3HwStatusQuery { CSL_EDMA3_QUERY_MEMFAULT, CSL_EDMA3_QUERY_MEMPROTECT, CSL_EDMA3_QUERY_CTRLERROR, CSL_EDMA3_QUERY_INTRPEND, CSL_EDMA3_QUERY_EVENTMISSED, CSL_EDMA3_QUERY_QUESTATUS, CSL_EDMA3_QUERY_ACTIVITY, CSL_EDMA3_QUERY_INFO }
| MODULE Level Queries. More...
enum | CSL_Edma3HwChannelControlCmd { CSL_EDMA3_CMD_CHANNEL_ENABLE, CSL_EDMA3_CMD_CHANNEL_DISABLE, CSL_EDMA3_CMD_CHANNEL_SET, CSL_EDMA3_CMD_CHANNEL_CLEAR, CSL_EDMA3_CMD_CHANNEL_CLEARERR }
| CHANNEL Commands. More...
enum | CSL_Edma3HwChannelStatusQuery { CSL_EDMA3_QUERY_CHANNEL_STATUS, CSL_EDMA3_QUERY_CHANNEL_ERR }
| CHANNEL Queries. More...

## Enumeration Type Documentation

enum CSL_Edma3HwChannelControlCmd

CHANNEL Commands.

Enumerator:

  CSL_EDMA3_CMD_CHANNEL_ENABLE | Enables specified Channel.
  Parameters:

    | (None) |

  CSL_EDMA3_CMD_CHANNEL_DISABLE | Disables specified Channel.
  Parameters:

    | (None) |

  CSL_EDMA3_CMD_CHANNEL_SET | Manually sets the Channel Event,writes into ESR/ESRH and not ER.NA for QDMA.
  Parameters:

    | (None) |

  CSL_EDMA3_CMD_CHANNEL_CLEAR | Manually clears the Channel Event, does not write into ESR/ESRH or ER/ERH but the ECR/ECRH. NA for QDMA.
  Parameters:

    | (None) |

  CSL_EDMA3_CMD_CHANNEL_CLEARERR | In case of DMA channels clears SER/SERH(by writing into SECR/SECRH if "secEvt" and "missed" are both TRUE) and EMR/EMRH(by writing into EMCR/EMCRH if "missed" is TRUE). In case of QDMA channels clears QSER(by writing into QSECR if "ser" and "missed" are both TRUE) and QEMR(by writing into QEMCR if "missed" is TRUE).
  Parameters:

    | (CSL_Edma3ChannelErr | *)

enum CSL_Edma3HwChannelStatusQuery

CHANNEL Queries.

Enumerator:

  CSL_EDMA3_QUERY_CHANNEL_STATUS | In case of DMA channels returns TRUE if ER/ERH is set, In case of QDMA channels returns TRUE if QER is set.
  Parameters:

    | (Bool | *)

  CSL_EDMA3_QUERY_CHANNEL_ERR | In case of DMA channels,'missed' is set to TRUE if EMR/EMRH is set, 'secEvt' is set to TRUE if SER/SERH is set.In case of QDMA channels,'missed' is set to TRUE if QEMR is set, 'secEvt' is set to TRUE if QSER is set. It should be noted that if secEvt ONLY is set to TRUE it may not be a valid error condition.
  Parameters:

    | (CSL_Edma3ChannelErr | *)

enum CSL_Edma3HwControlCmd

MODULE Level Commands

Enumerator:

  CSL_EDMA3_CMD_MEMPROTECT_SET | Programmation of MPPAG,MPPA[0-7] attributes.
  Parameters:

    | (CSL_Edma3CmdRegion | *)

  CSL_EDMA3_CMD_MEMFAULT_CLEAR | Clear Memory Fault.
  Parameters:

    | (None) |

  CSL_EDMA3_CMD_DMAREGION_ENABLE | Enables bits as specified in the argument passed in DRAE/DRAEH. Please note:If bits are already set in DRAE/DRAEH this Control command will cause additional bits (as specified by the bitmask) to be set and does.
  Parameters:

    | (CSL_Edma3CmdDrae | *)

  CSL_EDMA3_CMD_DMAREGION_DISABLE | Disables bits as specified in the argument passed in DRAE/DRAEH.
  Parameters:

    | (CSL_Edma3CmdDrae | *)

  CSL_EDMA3_CMD_QDMAREGION_ENABLE | Enables bits as specified in the argument passed in QRAE.Pleasenote:If bits are already set in QRAE/QRAEH this Control command will cause additional bits (as specified by the bitmask) to be set and does.
  Parameters:

    | (CSL_Edma3CmdQrae | *)

  CSL_EDMA3_CMD_QDMAREGION_DISABLE | Disables bits as specified in the argument passed in QRAE DRAE/DRAEH.
  Parameters:

    | (CSL_Edma3CmdQrae | *)

  CSL_EDMA3_CMD_QUEPRIORITY_SET | Programmation of QUEPRI register with the specified priority DRAE/DRAEH.
  Parameters:

    | (CSL_Edma3CmdQuePri | *)

  CSL_EDMA3_CMD_QUETHRESHOLD_SET | Programmation of QUE Threshold levels.
  Parameters:

    | (CSL_Edma3CmdQueThr | *)

  CSL_EDMA3_CMD_ERROR_EVAL | Sets the EVAL bit in the EEVAL register.
  Parameters:

    | (None) |

  CSL_EDMA3_CMD_INTRPEND_CLEAR | Clears specified (Bitmask)pending interrupt at Module/Region Level.
  Parameters:

    | (CSL_Edma3CmdIntr | *)

  CSL_EDMA3_CMD_INTR_ENABLE | Enables specified interrupts(BitMask) at Module/Region Level.
  Parameters:

    | (CSL_Edma3CmdIntr | *)

  CSL_EDMA3_CMD_INTR_DISABLE | Disables specified interrupts(BitMask) at Module/Region Level.
  Parameters:

    | (CSL_Edma3CmdIntr | *)

  CSL_EDMA3_CMD_INTR_EVAL | Interrupt Evaluation asserted for the Module/Region.
  Parameters:

    | (Int | *)

  CSL_EDMA3_CMD_CTRLERROR_CLEAR | Clear the EDMA Controller Erorr.
  Parameters:

    | (CSL_Edma3CtrlErrStat | *)

  CSL_EDMA3_CMD_EVENTMISSED_CLEAR | Pointer to an array of 3 elements, where element0 refers to the EMR register to be cleared, element1 refers to the EMRH register to be cleared, element2 refers to the QEMR register to be cleared.
  Parameters:

    | (CSL_BitMask32 | *)

enum CSL_Edma3HwStatusQuery

MODULE Level Queries.

Enumerator:

  CSL_EDMA3_QUERY_MEMFAULT | Return the Memory fault details.
  Parameters:

    | (CSL_Edma3MemFaultStat | *)

  CSL_EDMA3_QUERY_MEMPROTECT | Return memory attribute of the specified region.
  Parameters:

    | (CSL_Edma3CmdRegion | *)

  CSL_EDMA3_QUERY_CTRLERROR | Return Controller Error.
  Parameters:

    | (CSL_Edma3CtrlErrStat | *)

  CSL_EDMA3_QUERY_INTRPEND | Return pend status of specified interrupt.
  Parameters:

    | (CSL_Edma3CmdIntr | *)

  CSL_EDMA3_QUERY_EVENTMISSED | Returns Miss Status of all Channels Pointer to an array of 3 elements, where element0 refers to the EMR registr, element1 refers to the EMRH register, element2 refers to the QEMR register.
  Parameters:

    | (CSL_BitMask32 | *)

  CSL_EDMA3_QUERY_QUESTATUS | Returns the Que status.
  Parameters:

    | (CSL_Edma3QueStat | *)

  CSL_EDMA3_QUERY_ACTIVITY | Returns the Channel Controller Active Status.
  Parameters:

    | (CSL_Edma3ActivityStat | *)

  CSL_EDMA3_QUERY_INFO | Returns the Channel Controller Information viz. Configuration, Revision Id.
  Parameters:

    | (CSL_Edma3QueryInfo | *)

enum CSL_Edma3Que

Enumeration for EDMA Event Queues.

These are a list of all the event queues.

Enumerator:

  CSL_EDMA3_QUE_DEFAULT | Default Event Queue
  CSL_EDMA3_QUE_0 | Event Queue 0
  CSL_EDMA3_QUE_1 | Event Queue 1
  CSL_EDMA3_QUE_2 | Event Queue 2
  CSL_EDMA3_QUE_3 | Event Queue 3
  CSL_EDMA3_QUE_4 | Event Queue 4
  CSL_EDMA3_QUE_5 | Event Queue 5
  CSL_EDMA3_QUE_6 | Event Queue 6
  CSL_EDMA3_QUE_7 | Event Queue 7

enum CSL_Edma3QuePri

Enumeration for System priorities.

This is used for Setting up the Que Priority level

Enumerator:

  CSL_EDMA3_QUE_PRI_0 | System priority level 0
  CSL_EDMA3_QUE_PRI_1 | System priority level 1
  CSL_EDMA3_QUE_PRI_2 | System priority level 2
  CSL_EDMA3_QUE_PRI_3 | System priority level 3
  CSL_EDMA3_QUE_PRI_4 | System priority level 4
  CSL_EDMA3_QUE_PRI_5 | System priority level 5
  CSL_EDMA3_QUE_PRI_6 | System priority level 6
  CSL_EDMA3_QUE_PRI_7 | System priority level 7

enum CSL_Edma3QueThr

Enumeration for EDMA Que Thresholds.

This is used for Setting up the Que thresholds

Enumerator:

  CSL_EDMA3_QUE_THR_0 | EDMA Que Threshold 0
  CSL_EDMA3_QUE_THR_1 | EDMA Que Threshold 1
  CSL_EDMA3_QUE_THR_2 | EDMA Que Threshold 2
  CSL_EDMA3_QUE_THR_3 | EDMA Que Threshold 3
  CSL_EDMA3_QUE_THR_4 | EDMA Que Threshold 4
  CSL_EDMA3_QUE_THR_5 | EDMA Que Threshold 5
  CSL_EDMA3_QUE_THR_6 | EDMA Que Threshold 6
  CSL_EDMA3_QUE_THR_7 | EDMA Que Threshold 7
  CSL_EDMA3_QUE_THR_8 | EDMA Que Threshold 8
  CSL_EDMA3_QUE_THR_9 | EDMA Que Threshold 9
  CSL_EDMA3_QUE_THR_10 | EDMA Que Threshold 10
  CSL_EDMA3_QUE_THR_11 | EDMA Que Threshold 11
  CSL_EDMA3_QUE_THR_12 | EDMA Que Threshold 12
  CSL_EDMA3_QUE_THR_13 | EDMA Que Threshold 13
  CSL_EDMA3_QUE_THR_14 | EDMA Que Threshold 14
  CSL_EDMA3_QUE_THR_15 | EDMA Que Threshold 15
  CSL_EDMA3_QUE_THR_16 | EDMA Que Threshold 16

Copyright 2012, Texas Instruments Incorporated