# hyplnkIntStatusClrReg_s Struct Reference
[HYPLNK LLD Register Definitions]

Specification of the Hyperlink Interrupt Status/Clear Register. More...

`#include <hyplnk.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint32_t | intClr
| [rw] Interrupt Status/Clear Bitfield

## Detailed Description

Specification of the Hyperlink Interrupt Status/Clear Register.

The Interrupt Status/Clear Register indicates the unmasked interrupt status. Writing 1 to any bit in this register will clear the corresponding interrupt.

## Field Documentation

uint32_t hyplnkIntStatusClrReg_s::intClr

[rw] Interrupt Status/Clear Bitfield

Field size: 32 bits

Each bit represents the unmasked status of its respective interrupt. Writing a 1 to a particular bit will clear it.

The documentation for this struct was generated from the following file:

- hyplnk.h

Copyright 2012, Texas Instruments Incorporated