# hyplnkIntPendSetReg_s Struct Reference
[HYPLNK LLD Register Definitions]

Specification of the Hyperlink Interrupt Pending/Set Register. More...

`#include <hyplnk.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint32_t | intSet
| [rw] Interrupt Pending/Set Bitfield

## Detailed Description

Specification of the Hyperlink Interrupt Pending/Set Register.

The Interrupt Pending/Set Register indicates the pending interrupt status. This register can be written by the local host or by remote interrupt packets when the hyplnkControlReg_s::int2cfg bit is set. When bits are set in this register, an interrupt output is signaled, if not already pending. Any write with a value of 0x0000 to this register will EOI the hyplnkIntPendSetReg_s interrupt output pins so they retrigger the interrupt. That is, writing a zero to hyplnkIntPendSetReg_s retriggers the output interrupt lines if any bits are still set in this register.

## Field Documentation

uint32_t hyplnkIntPendSetReg_s::intSet

[rw] Interrupt Pending/Set Bitfield

Field size: 32 bits

Each bit represents the unmasked status of its respective pending interrupt. Writing a 1 to a particular bit will activate it.

The documentation for this struct was generated from the following file:

- hyplnk.h

Copyright 2012, Texas Instruments Incorporated