# CSL_TmrHwSetup Struct Reference
[TIMER Data Structures]

Hardware setup structure. More...

`#include <csl_tmr.h>`

## Data Fields

Uint32 | tmrTimerPeriodLo
Uint32 | tmrTimerPeriodHi
Uint32 | tmrTimerCounterLo
Uint32 | tmrTimerCounterHi
CSL_TmrIpGate | tmrIpGateHi
CSL_TmrClksrc | tmrClksrcHi
CSL_TmrPulseWidth | tmrPulseWidthHi
CSL_TmrClockPulse | tmrClockPulseHi
CSL_TmrInvInp | tmrInvInpHi
CSL_TmrInvOutp | tmrInvOutpHi
CSL_TmrIpGate | tmrIpGateLo
CSL_TmrClksrc | tmrClksrcLo
CSL_TmrPulseWidth | tmrPulseWidthLo
CSL_TmrClockPulse | tmrClockPulseLo
CSL_TmrInvInp | tmrInvInpLo
CSL_TmrInvOutp | tmrInvOutpLo
Uint8 | tmrPreScalarCounterHi
CSL_TmrMode | tmrTimerMode

## Detailed Description

Hardware setup structure.

## Field Documentation

CSL_TmrClksrc CSL_TmrHwSetup::tmrClksrcHi

CLKSRC determines the selected clock source for the timer

CSL_TmrClksrc CSL_TmrHwSetup::tmrClksrcLo

CLKSRC determines the selected clock source for the timer

CSL_TmrClockPulse CSL_TmrHwSetup::tmrClockPulseHi

Clock/Pulse mode for timerHigh output

CSL_TmrClockPulse CSL_TmrHwSetup::tmrClockPulseLo

Clock/Pulse mode for timerLow output

CSL_TmrInvInp CSL_TmrHwSetup::tmrInvInpHi

Timer input inverter control. Only affects operation if CLKSRC=1, Timer Input pin

CSL_TmrInvInp CSL_TmrHwSetup::tmrInvInpLo

Timer input inverter control. Only affects operation if CLKSRC=1, Timer Input pin

CSL_TmrInvOutp CSL_TmrHwSetup::tmrInvOutpHi

Timer output inverter control

CSL_TmrInvOutp CSL_TmrHwSetup::tmrInvOutpLo

Timer output inverter control

CSL_TmrIpGate CSL_TmrHwSetup::tmrIpGateHi

TIEN determines if the timer clock is gated by the timer input. Applicable only when CLKSRC=0

CSL_TmrIpGate CSL_TmrHwSetup::tmrIpGateLo

TIEN determines if the timer clock is gated by the timer input. Applicable only when CLKSRC=0

Uint8 CSL_TmrHwSetup::tmrPreScalarCounterHi

CNTHI pre-scalar counter specifies the count for CNTHI

CSL_TmrPulseWidth CSL_TmrHwSetup::tmrPulseWidthHi

Pulse width. used in pulse mode (C/P_=0) by the timer

CSL_TmrPulseWidth CSL_TmrHwSetup::tmrPulseWidthLo

Pulse width. used in pulse mode (C/P_=0) by the timer

Uint32 CSL_TmrHwSetup::tmrTimerCounterHi

32 bit load value to be loaded to Timer Counter Register High

Uint32 CSL_TmrHwSetup::tmrTimerCounterLo

32 bit load value to be loaded to Timer Counter Register Low

CSL_TmrMode CSL_TmrHwSetup::tmrTimerMode

Configures the GP timer in GP mode or in general purpose timer mode or Dual 32 bit timer mode

Uint32 CSL_TmrHwSetup::tmrTimerPeriodHi

32 bit load value to be loaded to Timer Period Register High

Uint32 CSL_TmrHwSetup::tmrTimerPeriodLo

32 bit load value to be loaded to Timer Period Register low

The documentation for this struct was generated from the following file:

- csl_tmr.h

Copyright 2012, Texas Instruments Incorporated