# pciePmRstIrqStatusRawReg_s Struct Reference
[PCIE LLD Application Register Definitions]

Specification of the Raw Power Management and Reset Interrupt Status Register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
uint8_t | linkRstReq
| [rw] Link Request Reset interrupt raw status
uint8_t | pmPme
| [rw] Power management PME message received interrupt raw status
uint8_t | pmToAck
| [rw] Power mangement ACK received interrupt raw status
uint8_t | pmTurnoff
| [rw] Power management turnoff messages received raw status

## Detailed Description

Specification of the Raw Power Management and Reset Interrupt Status Register.

## Field Documentation

uint8_t pciePmRstIrqStatusRawReg_s::linkRstReq

[rw] Link Request Reset interrupt raw status

Field size: 1 bit

uint8_t pciePmRstIrqStatusRawReg_s::pmPme

[rw] Power management PME message received interrupt raw status

Field size: 1 bit

uint8_t pciePmRstIrqStatusRawReg_s::pmToAck

[rw] Power mangement ACK received interrupt raw status

Field size: 1 bit

uint8_t pciePmRstIrqStatusRawReg_s::pmTurnoff

[rw] Power management turnoff messages received raw status

Field size: 1 bit

uint32_t pciePmRstIrqStatusRawReg_s::raw

[ro] Raw image of register on read; actual value on write

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated