# BWMNGMT Symbols Defined
[BWMNGMT]

## Defines

#define | CSL_BWMNGMT_PRI_PRI0 (0x00000000u)
| Priority arbitration setting 0 - Highest priority requestor.
#define | CSL_BWMNGMT_PRI_PRI1 (0x00000001u)
| Priority arbitration setting 1 - 2nd Highest priority requestor.
#define | CSL_BWMNGMT_PRI_PRI2 (0x00000002u)
| Priority arbitration setting 2 - 3rd Highest priority requestor.
#define | CSL_BWMNGMT_PRI_PRI3 (0x00000003u)
| Priority arbitration setting 3 - 4th Highest priority requestor.
#define | CSL_BWMNGMT_PRI_PRI4 (0x00000004u)
| Priority arbitration setting 4 - 5th Highest priority requestor.
#define | CSL_BWMNGMT_PRI_PRI5 (0x00000005u)
| Priority arbitration setting 5 - 6th Highest priority requestor.
#define | CSL_BWMNGMT_PRI_PRI6 (0x00000006u)
| Priority arbitration setting 6 - 7th Highest priority requestor.
#define | CSL_BWMNGMT_PRI_PRI7 (0x00000007u)
| Priority arbitration setting 7 - Lowest priority requestor.
#define | CSL_BWMNGMT_MAXWAIT_MAXWAIT0 (0x00000000u)
| Maxwait arbitration setting 0 - Always stall due to higher priority requestor.
#define | CSL_BWMNGMT_MAXWAIT_MAXWAIT1 (0x00000001u)
| Maxwait arbitration setting 1 - Stall max of 1 cycle due to higher priority requestor.
#define | CSL_BWMNGMT_MAXWAIT_MAXWAIT2 (0x00000002u)
| Maxwait arbitration setting 2 - Stall max of 2 cycle due to higher priority requestor.
#define | CSL_BWMNGMT_MAXWAIT_MAXWAIT4 (0x00000004u)
| Maxwait arbitration setting 4 - Stall max of 4 cycle due to higher priority requestor.
#define | CSL_BWMNGMT_MAXWAIT_MAXWAIT8 (0x00000008u)
| Maxwait arbitration setting 8 - Stall max of 8 cycle due to higher priority requestor.
#define | CSL_BWMNGMT_MAXWAIT_MAXWAIT16 (0x00000010u)
| Maxwait arbitration setting 16 - Stall max of 16 cycle due to higher priority requestor.
#define | CSL_BWMNGMT_MAXWAIT_MAXWAIT32 (0x00000020u)
| Maxwait arbitration setting 32 - Stall max of 32 cycle due to higher priority requestor.

## Define Documentation

#define CSL_BWMNGMT_MAXWAIT_MAXWAIT0 (0x00000000u)

Maxwait arbitration setting 0 - Always stall due to higher priority requestor.

Max Wait Encodings for BWMNGMT

#define CSL_BWMNGMT_PRI_PRI0 (0x00000000u)

Priority arbitration setting 0 - Highest priority requestor.

Priority Encodings for BWMNGMT

Copyright 2012, Texas Instruments Incorporated