# VCP2_ConfigIc Struct Reference
[VCP2 Data Structures]

`#include <csl_vcp2.h>`

## Data Fields

Uint32 | ic0
Uint32 | ic1
Uint32 | ic2
Uint32 | ic3
Uint32 | ic4
Uint32 | ic5

## Detailed Description

VCP input configuration structure that holds all of the configuration values that are to be transferred to the VCP via the EDMA.

## Field Documentation

Uint32 VCP2_ConfigIc::ic0

Value of VCP input configuration register 0

Uint32 VCP2_ConfigIc::ic1

Value of VCP input configuration register 1

Uint32 VCP2_ConfigIc::ic2

Value of VCP input configuration register 2

Uint32 VCP2_ConfigIc::ic3

Value of VCP input configuration register 3

Uint32 VCP2_ConfigIc::ic4

Value of VCP input configuration register 4

Uint32 VCP2_ConfigIc::ic5

Value of VCP input configuration register 5

The documentation for this struct was generated from the following file:

- csl_vcp2.h

Copyright 2012, Texas Instruments Incorporated