# pcieIbTransCfg_s Struct Reference
[PCIE LLD API Data Structures]

Specification of pcieIbTransCfg. More...

`#include <pcie.h>`

## Data Fields

uint8_t | ibBar
| Inbound Translation BAR match.
uint32_t | ibStartAddrLo
| Low Inbound Start address (32bits).
uint32_t | ibStartAddrHi
| High Inbound Start address (32bits).
uint32_t | ibOffsetAddr
| Inbound Translation Address Offset (32bits).
uint8_t | region
| Identifies the translation region (0-3).

## Detailed Description

Specification of pcieIbTransCfg.

The pcieIbTransCfg is used to configure the Inbound Translation Registers

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated