# pciePlOMsgReg_s Struct Reference
[PCIE LLD Port Logic Register Definitions]

Specification of the Other Message register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
uint32_t | oMsg
| [rw] Other Message Register

## Detailed Description

Specification of the Other Message register.

This register may be used for both endpoint and root complex modes.

## Field Documentation

uint32_t pciePlOMsgReg_s::oMsg

[rw] Other Message Register

It can be used to send a specific PCI Express message in which case this register is programmed with the payload and bit pcieLnkCtrlReg_s::msgReq set to transmit the message.

Field size: 32 bits

uint32_t pciePlOMsgReg_s::raw

[ro] Raw image of register on read; actual value on write

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated