# pcieEpIrqStatusReg_s Struct Reference
[PCIE LLD Application Register Definitions]

Specification of the Endpoint Interrupt status Register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
uint8_t | epIrqStatus
| [rw] Indicates whether interrupt for function 0 is asserted or not

## Detailed Description

Specification of the Endpoint Interrupt status Register.

## Field Documentation

uint8_t pcieEpIrqStatusReg_s::epIrqStatus

[rw] Indicates whether interrupt for function 0 is asserted or not

Field size: 1 bit

uint32_t pcieEpIrqStatusReg_s::raw

[ro] Raw image of register on read; actual value on write

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated