# pciePrefBaseUpperReg_s Struct Reference
[PCIE LLD Type1 (root) Register Definitions]

Specification of the Prefetchable Memory Base Upper Register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint32_t | base
| [rw] Base upper 32bits

## Detailed Description

Specification of the Prefetchable Memory Base Upper Register.

## Field Documentation

uint32_t pciePrefBaseUpperReg_s::base

[rw] Base upper 32bits

Upper 32 bits of Prefetchable Memory Base Address. Used with 64bit prefetchable memory addressing only.

Field size: 32 bits

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated